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CIRCULAR
LIST OF POTENTIALLY UNSAFE COMMODITIES UNDER THE MANAGEMENT OF THE MINISTRY OF INFORMATION AND COMMUNICATIONS

Pursuant to the Law on Product and Goods Quality dated November 21, 2007;
Pursuant to the Law on Technical Regulations and Standards dated June 29, 2006;
Pursuant to the Law on Radio Frequencies dated November 23, 2009; the Law on Amendments to the Law on Radio Frequencies dated November 09, 2022;
Pursuant to the Law on Information Technology dated June 29, 2006;
Pursuant to the Government's Decree No. 132/2008/ND-CP dated December 31, 2008 elaborating some of articles of the Law on Product and Goods Quality, Decree No. 74/2018/ND-CP dated May 15, 2018 on amendments to Decree No. 132/2008/ND-CP.
Pursuant to the Government's Decree No.154/2018/ND-CP dated November 09, 2018 on amendments to and annulment of some regulations on conditions for investment in state management sector of the Ministry of Science and Technology and some regulations on specialized inspection;
Pursuant to the Government's Decree No. 13/2022/ND-CP dated January 21, 2022 on amendments to Decree No. 132/2008/ND-CP dated December 31, 2008, Decree No. 74/2018/ND-CP dated May 15, 2018 elaborating some of articles of the Law on Product and Goods Quality, and Decree No. 86/2012/ND-CP dated October 19, 2012 elaborating some Articles of the Law on Measurement;
Pursuant to the Government’s Decree No. 48/2022/ND-CP dated July 26, 2022 on functions, tasks, powers and organizational structure of the Ministry of Information and Communications;
At the request of the Director of Science and Technology Department,
The Minister of Information And Communications promulgates the List of potentially unsafe commodities under the management of the Ministry of Information and Communications.
Article 1. Scope
1. This Circular provides for the list of potentially unsafe commodities under the management of the Ministry of Information and Communications (hereinafter referred to as “the List of category 2 commodities”); rules for management of category 2 commodities; some cases of suspension and optional application of part/all of certain technical regulations.

2. This Circular only applies to commodities whose HS codes and descriptions are provided in the List of category 2 commodities.

Article 2. Regulated entities
This Circular applies to:

1. Organizations and individuals involved in production and sale of commodities on the List of category 2 commodities in Vietnam.

2. Organizations and individuals whose activities involve management of quality of commodities on the List of category 2 commodities in Vietnam.

Article 3. List of category 2 commodities
List of category 2 commodities and measures for management thereof:

1. The list of information technology and communications commodities subject to certification and declaration of conformity is provided in the Appendix I hereof.

2. The list of information technology and communications commodities subject to declaration of conformity is provided in the Appendix II hereof.

Article 4. Rules for management of category 2 commodities
1. Quality of commodities on the List of category 2 commodities shall be managed in accordance with regulations of the Ministry of Information and Communications on certification and declaration of conformity and inspection of quality of information technology and communications commodities, and respective technical regulations.

2. If an integral part of a commodity on the List of category 2 commodities is another commodity on the same List, it is required to certify and declare its conformity with all technical regulations applicable to both commodities.

3. Commodities on the List of category 2 commodities that are governed by two or more national technical regulations, certification and declaration of their conformity shall be carried out according to such technical regulations.

4. In case of discrepancies between regulations of a technical regulation that is promulgated before the effective date of this Circular and regulations of this Circular, regulations of this Circular shall prevail.

5. From the effective date of this Circular, if a there is a new technical regulation that replaces a technical regulation specified in the List of group 2 commodities, or there is a new technical regulation that additionally applies to the commodities on the List of group 2 commodities, regulations of the Circular promulgating the newest technical regulation shall apply.

Article 5. Some cases of exemption of category 2 commodities from certification and declaration of conformity
1. If a commodity specified in section 1 or section 2 of Appendix II hereof has an integrated short-range radio device in section 2 of Appendix I or section 4 of Appendix II hereof and does not have integrated other radio transceivers, it shall be exempted from certification and declaration of conformity if all of the following requirements are satisfied:

a) It is imported for internal used by the importer;

b) The import quantity does not exceed 03 products per category in the shipment;

c) Its frequency band and specifications meet the technical conditions and operational conditions as set out in Circular No. 08/2021/TT-BTTTT dated October 14, 2021 of the Minister of Information and Communications on the List of radio equipment which is exempt from a radio frequency license, with technical and operational conditions attached.

2. A commodity specified in section 1 or section 2 of Appendix II hereof shall be exempted from certification and declaration of conformity with QCVN 101:2020/BTTTT, QCVN 132:2022/BTTTT, and the part of technical regulations that require destructive testing if all of the following requirements are satisfied:

a) The import quantity does not exceed 03 products per category in the shipment;

b) The importer has a written declaration that the commodities comply with part/all of technical regulations that require destructive testing and to take total responsibility for the safety of the imported commodities.

3. The exemption of the commodities specified in Clause 1 and Clause 2 of this Article from certification and declaration of conformity shall comply with Point c Clause 2 Article 16 of Circular No. 30/2011/TT-BTTTT dated October 31, 2011, which is amended by Circular No. 15/2018/TT-BTTTT dated November 15, 2018 and Circular No. 10/2020/TT-BTTTT dated May 07, 2020 of the Minister of Information And Communications. 

Article 6. Some cases of suspension, optional application of part/all of certain technical regulations
1. Some cases of suspension, optional application of part/all of certain technical regulations until the end of June 30, 2025 are specified in Appendix I and Appendix II hereof.

2. From the effective date of this Circular until the end of June 30, 2025, it is recommended to carry out certification and declaration of conformity of the commodities of Clause 1 of this Article with all respective technical regulations.

3. From July 01, 2025, if the commodities specified in Clause 1 of this Article continue to be manufactured or imported after having undergone certification and declaration of conformity during the period from July 15, 2023 to the end of June 30, 2025, they must undergo supplementary certification and declaration of conformity with respective technical regulations, or undergo new certification and declaration of conformity with respective technical regulations.

Article 7. Effect
1. This Circular comes into force from May 15, 2024.

2. Circular No. 04/2023/TT-BTTTT dated May 31, 2023 of the Minister of Information And Communications 
on the List of potentially unsafe commodities under the management of the Ministry of Information and Communications and Circular No. 10/2023/TT-BTTTT dated September 05, 2023 of the Minister of Information And Communications on suspension of part/all of certain technical regulations in Circular No. 04/2023/TT-BTTTT dated May 31, 2023 of the Minister of Information And Communications cease to have effect from the effective date of this Circular.

Article 8. Transition clauses
1. Unexpired certificates of conformity, notifications of receipt of declaration of conformity that are issued to commodities specified in Clause 1 Article 6 of this Circular during the period from July 15, 2023 to before the effective date of this Circular may to be used until their expiration dates written therein.

2. Importers may choose to complete their declarations of conformity and apply for quality inspection of imported goods during the period from January 01, 2024 to before the effective date of this Circular regarding technical regulations in Circular No. 04/2023/TT-BTTTT dated May 31, 2023 and Circular No. 10/2023/TT-BTTTT, or the technical regulations specified in Clause 1 Article 6 of this Circular. 

Article 9. Organization of implementation
1. Chief of Office, Director of Department of Science and Technology, heads of affiliates of the Ministry of Information and Communications and relevant organizations and individuals are responsible for the implementation of this Circular.

2. During the implementation of this Circular, organizations and individuals have the responsibility to promptly report the issues that occur and follow the guidelines laid down by the Department of Science and Technology (affiliated to the Ministry of Information and Communications).

3. The Ministry of Information and Communications shall cooperate with the General Department of Vietnam Customs (affiliated to the Ministry of Finance) in resolving any issue that arises from assigning HS codes to imports that are potentially unsafe commodities within the scope of this Circular./.

 

	 
	THE MINISTER




Nguyen Manh Hung


 

APPENDIX I
LIST OF INFORMATION TECHNOLOGY AND COMMUNICATIONS COMMODITIES SUBJECT TO CERTIFICATION AND DECLARATION OF CONFORMITY
((Enclosed with the Circular No. 02/2024/TT-BTTTT dated March 29, 2024 of the Minister of Information and Communications)
	No.
	Name of commodity
	Technical regulation
	HS code under Circular No. 31/2022/TT-BTC
	Description
	Provisions on application of technical regulations, certification  and declaration of conformity

	1
	Radio transmitters and transceivers operating in the 9 kHz to 400 kHz frequency band

	1.1
	Radio transmitters and transceivers for use in land mobile or fixed services

	1.1.1
	Land mobile user equipment (3)
	QCVN 86:2019/ BTTTT (1)
QCVN 101:2020/BTTTT (1) (8)
QCVN 117:2020/BTTTT hoặc QCVN 117:2023/BTTTT (7)
	8517.13.00
8517.14.00
	A cellular telephone using E-UTRA FDD (4G) technology, whether or not integrated with one or more of the following functions:
- W-CDMA FDD (3G) mobile terminal;
- GSM (2G and 2.5G) mobile terminal;
- Fifth generation (5G) mobile terminal;
- Wideband data transmission in the 2.4 GHz band;
- Radio access in the 5 GHz band;
- Short-range radio transmission and transmission - reception.
	- From February 15, 2024 to June 30, 2024 inclusive: select to apply QCVN 117:2020/BTTTT or QCVN 117:2023/BTTTT.
- From July 01, 2024: apply QCVN 117:2023/BTTTT; Certificate of conformity issued under QCVN 117:2020/BTTTT remains effective until its expiry, including completion of applications for state inspection under QCVN 117:2023/BTTTT.
- For QCVN 117:2020/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 117:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2024.
- Land mobile user equipment other than mobile phones must use E-UTRA (4G) technology. Certificate of conformity issued to land mobile user equipment other than mobile phones only integrated with or using W-CDMA FDD (3G) or GSM (2G and 2,5G) technology under 117:2020/BTTTT remains effective until its expiry but no later than June 30, 2024.
- For QCVN 101:2020/BTTTT: only applicable to mobile phones using stand-alone lithium batteries or lithium batteries included/installed in the equipment (an integral part of the equipment).

	
	
	
	8517.62.59
	Land mobile user equipment (transmission apparatus incorporating reception apparatus) other than mobile phones integrated with or using one or more of the following technologies: E-UTRA FDD (4G); W-CDMA FDD (30); GSM (2G and 2,5G);
and possibly integrated one or more of the following functions:
- Fifth generation (5G) mobile terminal;
- Wideband data transmission in the 2.4 GHz band;
- Radio access in the 5 GHz band;
- Short-range radio transmission and transmission - reception.
	

	1.1.2
	Fifth generation mobile user equipment (5G) (3)
	QCVN 18:2022/BTTTT (1)
QCVN 101:2020/BTTTT (1) (8)
QCVN 127:2021/BTTTT and QCVN 129:2021/BTTTT
	8517.13.00
8517.14.00
	Land mobile user equipment other than mobile phones (transmission apparatus incorporating reception apparatus), using fifth generation (5G) mobile technology, whether or not integrated with one or more of the following functions:
- Land mobile terminal;
- Wideband data transmission in the 2.4 GHz band;
- Radio access in the 5 GHz band;
- Short-range radio transmission and transmission - reception.
	- Apply both QCVN 127:2021/BTTTT and QCVN 129:2021/BTTTT; Certificate of conformity issued to fifth generation under QCVN 127:2021/BTTTT or QCVN 129:2021/BTTTT remains effective until its expiry but no later than June 30, 2024.
- For QCVN 117:2020/BTTTT and QCVN 129:2021/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 101:2020/BTTTT: only applicable to mobile phones using stand-alone lithium batteries or lithium batteries included/installed in the equipment (an integral part of the equipment).

	
	
	
	8517.62.59
	Land mobile user equipment other than mobile phones (transmission apparatus incorporating reception apparatus), using fifth generation (5G) mobile technology, whether or not integrated with one or more of the following functions:
- Land mobile terminal;
- Wideband data transmission in the 2.4 GHz band;
- Radio access in the 5 GHz band;
- Short-range radio transmission and transmission - reception.
	

	1.1.3
	GSM base station (6)
	QCVN 41:2016/BTTTT
QCVN 103:2016/BTTTT (1)
	8517.61.00
	A base transceiver station in a GSM (2G and 2.5G) cellular network, whether or not integrated with one or more of the following functions:
- W-CDMA FDD (3G) base station;
- E-UTRA FDD (4G) base station;
- Fifth generation (5G) base station.
	- For QCVN 41:2016/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	1.1.4
	W-CDMA FDD base station (6)
	QCVN 16:2018/BTTTT
QCVN 103:2016/BTTTT (1)
	8517.61.00
	A base transceiver station in a W-CDMA FDD (3G) cellular network, whether or not integrated with one or more of the following functions:
- GSM (2G and 2.5G) base station;
- E-UTRA FDD (4G) base station;
- Fifth generation (5G) base station.
	- For QCVN 16:2018/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	1.1.5
	E-UTRA base station (6)
	QCVN 103:2016/BTTTT (1)
QCVN 110:2017/BTTTT or QCVN 110:2023/BTTTT
 
	8517.61.00
	A base transceiver station in an E-UTRA (4G) cellular network, whether or not integrated with one or more of the following functions:
- GSM (2G and 2.5G) base station;
- W-CDMA FDD (3G) base station;
- Fifth generation (5G) base station.
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 110:2017/BTTTT or QCVN 110:2023/BTTTT.
- From July 01, 2024: apply QCVN 110:2023/BTTTT; Certificate of conformity issued under 110:2017/BTTTT remains effective until its expiry, including completion of applications for state inspection under QCVN 110:2023/BTTTT.
- For QCVN 110:2017/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
 - For QCVN 110:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025.

	1.1.6
	Fifth generation (5G) base station (6)
	- For single-mode base station type 1-C or 1-H:
QCVN 128:2021/BTTTT (10)
QCVN 18:2022/BTTTT (1)
 
- For single-mode base station type 1-O or 2-O:
QCVN 128:2021/BTTTT (10)
QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT (1)
 
- For mixed-mode base station:
QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT (1)
	8517.61.00
	A base transceiver station in a fifth generation (5G) cellular network, whether or not integrated with one or more of the following functions:
- GSM (2G and 2.5G) base station;
- W-CDMA FDD (3G) base station;
- E-UTRA (4G) base station.
	- For single-mode base station type 1-C or 1-H: suspend the technical requirements under severe/critical conditions in QCVN 128:2021/BTTTT until June 30, 2025.
- For single-mode base station type 1-O or 2-O: totally suspend QCVN 128:2021/BTTTT until June 30, 2025.
- The importer must declare and include a statement of the type of the fifth generation base station (single-mode base station type 1-C, 1-H, 1-O, or 2-O; mixed-mode base station) in their application for quality inspection.

	1.1.7
	GSM repeater (6)
	QCVN 47:2015/BTTTT (2)
QCVN 103:2016/BTTTT (1)
	8517.62.59
	Radio equipment capable of receiving and transmitting GSM (2G and 2.5G) cellular network signals, whether or not integrated with one or more of the following functions:
- W-CDMA FDD (3G) repeater;
- E-UTRA FDD (4G) repeater;
- Fifth generation (5G) mobile terminal.
	 

	1.1.8
	W-CDMA FDD repeater (6)
	QCVN 66:2018/BTTTT
QCVN 103:2016/BTTTT (1)
	8517.62.59
	Radio equipment capable of receiving and transmitting W-CDMA FDD (3G) cellular network signals, whether or not integrated with one or more of the following functions:
- GSM (2G and 2.5G) repeater;
- E-UTRA FDD (4G) repeater;
- Fifth generation (5G) mobile terminal.
	- For QCVN 66:2018/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	1.1.9
	E-UTRA FDD repeater (6)
	QCVN 103:2016/BTTTT (1)
QCVN 111:2017/BTTTT or QCVN 111:2023/BTTTT
	8517.62.59
	Radio equipment capable of receiving and transmitting E-UTRA FDD (4G) cellular network signals, whether or not integrated with one or more of the following functions:
- GSM (2G and 2.5G) repeater;
- W-CDMA FDD (3G) repeater;
- Fifth generation (5G) mobile terminal.
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 111:2017/BTTTT or QCVN 111:2023/BTTTT.
- From July 01, 2024: apply QCVN 110:2023/BTTTT; Certificate of conformity issued under QCVN 111:2017/BTTTT remains effective until its expiry, including completion of applications for state inspection under QCVN 111:2023/BTTTT.
- For QCVN 111:2017/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024. 
- For QCVN 110:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025.

	1.1.10
	Fifth generation (5G) repeater (6)
	QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT (1)
 
	8517.62.59
	Radio equipment capable of receiving and transmitting fifth generation (5G) cellular network signals, whether or not integrated with one or more of the following functions:
- GSM (2G and 2.5G) repeater;
- W-CDMA FDD (3G) repeater;
- E-UTRA FDD (4G) repeater.
	 

	1.1.11
	Radio equipment in the Low Power Wide Area Networks (LPWAN) (5)
	- For equipment operating in the 920 MHz to 923 MHz frequency band:
+ For equipment having an effective radiated power of up to 25 mW ERP 
QCVN 122:2020/BTTTT (12)
QCVN 18:2022/BTTTT (1)
+ For equipment having a maximum effective radiated power of more than 25 mW ERP to 306 mW ERP 
QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT (1)
- For equipment operating in the 433,05 MHz to 434,79 MHz frequency band and having a maximum effective radiated power of up to 100 mW ERP: 
QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT (1)
	8517.61.00
8517.62.43
8517.62.59
8517.62.69
8517.62.99
8517.69.00
	Base stations, radio access equipment or terminal equipment having the functions of sensing, measuring, recording and transmitting parameters to be measured via a radio interface.
	- For QCVN 122:2020/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	
	9015.10.90
 
	Water level sensors transmitting measured parameters via an LPWAN radio interface.
	

	
	
	
	9025.19.19
 
	Air temperature sensors transmitting measured parameters via an LPWAN radio interface.
	

	
	
	
	9025.80.00
	Air humidity sensors transmitting measured parameters via an LPWAN radio interface.
	

	
	
	
	9027.89.90
	Air dust sensors transmitting measured parameters via an LPWAN radio interface.
	

	
	
	
	8531.10.30
8531.90.90
	Smoke detectors in the smoke detection system having the functions of analyzing smoke in the air and transmitting signals to the control center or smoke detection device via an LPWAN radio interface.
	

	
	
	- For E-UTRA NB IoT user equipment:
QCVN 131:2022/BTTTT (11)
QCVN 18:2022/BTTTT (1)
	8517.14.00
	NB IoT land mobile user equipment using designed for operation in E-UTRA frequency bands.
	 

	1.1.12
	Land mobile radio equipment using an integral antenna intended primarily for analogue speech(3)
	QCVN 37:2018/BTTTT (12)
QCVN 18:2022/BTTTT (1)
	8517.14.00
	Land mobile hand-held radio angle-modulated equipment with an integral antenna in the 30 MHz to 1000 MHz frequency band with channel separations of 12,5 kHz and 25 kHz, intended primarily for analogue speech (telephones for wireless networks, other than smartphones, other than line telephone sets with cordless handsets).
	- For QCVN 37:2018/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	1.1.13
	Land mobile radio equipment having an antenna connector intended primarily for analogue speech (3)
	QCVN 43:2011/BTTTT 
QCVN 18:2022/BTTTT (1)
	 
	Stations in the angle modulation systems for use in the land mobile service, operating in the frequency range between 30 MHz and 1000 MHz with channel separations of 12,5 kHz and 25 kHz and intended for analogue speech (telephones for wireless networks, other than smartphones, other than line telephone sets with cordless handsets), including:
	- For QCVN 43:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	
	8517.61.00
	- Base station (fitted with an antenna socket);
	

	
	
	
	8517.14.00
	- Mobile station (fitted with an antenna socket);
- Handportable stations fitted with an antenna socket; or without an external antenna socket (integral antenna equipment) but fitted with a permanent internal or a temporary internal 50 Ω RF connector which allows access to the transmitter output and the receiver input.
	

	1.1.14
	Land mobile radio equipment using an integral antenna intended for the transmission of data (and speech)(3)
 
	QCVN 44:2018/BTTTT (12)
QCVN 18:2022/BTTTT (1)
	8517.62.59
	Land mobile radio equipment using constant envelope angle modulation, operating in the frequency range between 30 MHz and 1 GHz with channel separations of 12,5 kHz and 25 kHz, and including digital hand-held radio equipment or combined analogue and digital hand-held radio equipment using an integral antenna and intended for the transmission of data and/or speech.
	- For QCVN 44:2018/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	1.1.15
	Land mobile radio equipment having an antenna connector intended for the transmission of data (and speech) (3)
	QCVN 42:2011/BTTTT
QCVN 18:2022/BTTTT (1)
	 
	Digital radio equipment and combined analogue/digital radio having an antenna connector and intended for the transmission of data and/or speech, including:
	- For QCVN 42:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	
	8517.61.00
	- Base station (fitted with an antenna socket and intended for use in a fixed location);
	

	
	
	
	8517.62.59
	- Mobile station (fitted with an antenna socket, normally used in a vehicle or as a transportable station) or handportable station intended for the transmission of data and/or speech.
	

	1.2
	Radio transmitters and transceivers used in television broadcasting and sound broadcasting

	1.2.1
	Second generation terrestrial digital television (DVB-T2) transmitter
	QCVN 77:2013/BTTTT
	8525.50.00
	Transmitting equipment for the terrestrial digital television broadcasting service DVB-T2, with 8 MHz RF channel.
	 

	1.2.2
	Transmitting equipment for the amplitude modulated (AM) sound broadcasting service
	QCVN 29:2011/BTTTT
	8525.50.00
	Transmitting equipment for the amplitude modulated (AM) sound broadcasting service operating in the medium wave band (from 526,5 kHz to 1606,5 kHz) and short wave band (from 3,2 MHz to 26,1 MHz).
	 

	1.2.3
	Transmitting equipment for the frequency modulated (FM) sound broadcasting service
	QCVN 30:2011/BTTTT
	8525.50.00
	Transmitting equipment for frequency modulated (FM) sound broadcasting service operating in both Monophonic and Stereophonic operating in the 87 MHz to 108 MHz frequency band.
	 

	1.2.4
	Frequency modulated (FM) radio sound transmitting equipment operating in the 54 MHz to 68 MHz frequency band
	QCVN 70:2013/BTTTT
	8525.50.00
	Frequency modulated (FM) radio sound transmitting equipment operating in monophonic operating in the 54 MHz to 68 MHz frequency band.
	 

	1.3
	Radar equipment

	1.3.1
	Radar equipment (except that used on seagoing vessels and that of a short-range radio transmitter and transceiver)
	QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT(1)
	8526.10.10
8526.10.90
	All kinds of radar equipment, ground based, or installed in civil aircraft, except that used on sea-going vessels and that of a short-range radio transmitter and transceiver.
	 

	2
	Short-range radio transmitters and transceivers (4)

	2.1
	DECT cordless telephone equipment, subscriber extension type (3)
	QCVN 47:2015/BTTTT (2)
QCVN 113:2017/BTTTT (1)
QCVN 132:2022/BTTTT (12)(13)
	8517.11.00
	A line telephone set consisting of a base (base station) attaching one or more cordless mobile phones (handsets) using DECT technology. The handset connected to a Public Switched Telephone Network (PSTN) via a base station is a telephone landline that routes telephone calls to the PSTN.
	 

	2.2
	Non-specific short-range radio transmitters and transceivers
	- For equipment operating in the 9 kHz to 25 MHz frequency band:
QCVN 96:2015/BTTTT (1)
QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT
 
- For equipment operating in the 25 MHz to 1 GHz frequency band:
QCVN 73:2013/BTTTT
QCVN 96:2015/BTTTT (1)
 
- For equipment operating in the 1 GHz to 40 GHz frequency band:
QCVN 74:2020/BTTTT
QCVN 96:2015/BTTTT (1)
	8517.62.59
8517.62.69
	Equipment fitted with an external antenna connector and/or integral antenna, and intended for transmission or reception of audio, images or other data; including equipment using active NFC (Near Field Communication) technology. Not applicable to the equipment mentioned in 4.1 in the Appendix II.
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT.
- From July 01, 2024: apply QCVN 55:2023/BTTTT; Certificate of conformity issued under QCVN 55:2011/BTTTT remains effective until its expiry, including completion of applications for state inspection under QCVN 55:2023/BTTTT.
- For QCVN 55:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 55:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	- For equipment operating in the 40 GHz to 246 GHz frequency band:
QCVN 123:2021/BTTTT (12)
QCVN 18:2022/BTTTT (1)
	8517.62.59
8526.92.00
	Radio alarm devices, remote control devices, general data communication devices, operating in the 40 GHz to 246 GHz frequency band in the following cases:
- Either with a Radio Frequency output connection and dedicated antenna or with an integral antenna;
- With all types of modulation;
- Intended for fixed, mobile or nomadic use.
Not applicable to the equipment mentioned in 4.1 in the Appendix II.
	- For QCVN 123:2021/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	
	8526.10.10
8526.10.90
	Telemetry device (short-distance measuring radar).
Not applicable to the equipment mentioned in 4.1 in the Appendix II.
	

	2.3
 
	Wideband data transmission equipment operating in the 2,4 GHz band having an Equivalent Isotropically Radiated Power (EIRP) from 60 mW to 200 mW (3)
	QCVN 54:2020/BTTTT
QCVN 112:2017/BTTTT (1)
	8517.62.51
	A WiFi transceiver (WiFi modem, WiFi transmitter) in the 2.4 GHz wireless local area network (in the 5150 MHz to 5350 MHz, 5470 MHz to 5725 MHz and 5725 MHz to 5850 MHz frequency bands) having an EIRP of 60 mW to 200 mW, whether or not integrated with one or more of the following functions:
- Radio access in the 5 GHz band;
- Land mobile terminal;
- Fifth generation (5G) mobile terminal;
- Other short-range radio equipment.
	- For QCVN 55:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025 for products and goods other than WiFi transceiver (WiFi modem, WiFi transmitter), HS code: 8517.62.51, integrated with the function of receiving and transmitting Wi-Fi signal.
 
 

	
	
	
	8806.21.00
8806.22.00
8806.23.00
8806.24.00
8806.29.00
	Flycam (television cameras, digital cameras and video camera recorders mounted on flying devices) using remote control technology, transmitting images in the 2,4 GHz frequency band (in the 2400 MHz to 2483,5 MHz frequency band) using spread spectrum modulation techniques and having an EIRP of 60 mW to 200 mW.
	

	
	
	
	8806.21.00
8806.22.00
8806.23.00
8806.24.00
8806.29.00
	Flycam (television cameras, digital cameras and video camera recorders mounted on flying devices) using remote control technology, transmitting images in the 2,4 GHz frequency band (in the 2400 MHz to 2483,5 MHz frequency band) using spread spectrum modulation techniques and having an EIRP of 60 mW to 200 mW.
	

	2.4
	Radio access equipment operating in the 5 GHz band and having an EIRP of at least 60 mW (3)
	QCVN 65:2021/BTTTT (9)
QCVN 112:2017/BTTTT (1)
	8517.62.51
	A WiFi transceiver (WiFi modem, WiFi transmitter) in the 5 GHz wireless local area network (in the 5150 MHz to 5350 MHz, 5470 MHz to 5725 MHz and 5725 MHz to 5850 MHz frequency bands) having an EIRP of at least 60 mW, whether or not integrated with one or more of the following functions:
- Wideband data transmission in the 2.4 GHz band;
- Land mobile terminal;
- Fifth generation (5G) mobile terminal;
- Other short-range radio equipment.
	- For QCVN 65:2021/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025 for products and goods other than WiFi transceiver (WiFi modem, WiFi transmitter), HS code: 8517.62.51, integrated with the function of receiving and transmitting Wi-Fi signal.
 

	
	
	
	8806.21.00
8806.22.00
8806.23.00
8806.24.00
8806.29.00
	Flycam (television cameras, digital cameras and video camera recorders mounted on flying devices) using remote control technology, transmitting images in the 5 GHz frequency band (in the 5150 MHz to 5350 MHz, 5470 MHz to 5725 MHz and 5725 MHz to 5850 MHz frequency bands) using spread spectrum modulation techniques and having an EIRP of 60 mW to 200 mW.
	

	
	
	
	8806.21.00
8806.22.00
8806.23.00
8806.24.00
8806.29.00
	UAV/Drone (a remote-controlled flying device equipped with television camera, digital camera and video camera recorder) using remote control technology, transmitting images in the 5 GHz frequency band (in the 5150 MHz to 5350 MHz, 5470 MHz to 5725 MHz and 5725 MHz to 5850 MHz frequency bands) using spread spectrum modulation techniques and having an EIRP of 60 mW to 200 mW.
	

	2.5
	Radar equipment used in road or railway transport and traffic
	- For equipment operating in the 24 GHz to 24,25 GHz frequency band:
QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT (1)
	8526.10.10
8526.10.90
	Short-range radar equipment operating in the 24 GHz to 24,25 GHz frequency band and intended for transport and traffic telematics applications (road or rail traffic) such as cruise control, protection, warning, and avoiding collisions between vehicles and other surrounding objects.
	 

	2.6
	Equipment intended for radio alarm and detection
	- For equipment operating in the 9 kHz to 25 MHz frequency band:
QCVN 96:2015/BTTTT (1)
QCVN 55:2011/BTTTT hoặc QCVN 55:2023/BTTTT
 
- For equipment operating in the 25 MHz to 1 GHz frequency band:
QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT (1)
	8517.62.69
	Equipment including sensors and control systems which are connected to each other via a radio interface for radio alarm and detection purposes
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT.
- From July 01, 2024: apply QCVN 55:2023/BTTTT; Certificate of conformity issued under QCVN 55:2011/BTTTT remains effective until its expiry, including completion of applications for state inspection under QCVN 55:2023/BTTTT.
- For QCVN 55:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 55:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025.

	2.7
	Remote control device
	- For equipment operating in the 9 kHz to 25 MHz frequency band:
QCVN 96:2015/BTTTT (1)
QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT
 
- For equipment operating in the 25 MHz to 1 GHz frequency band:
QCVN 73:2013/BTTTT
QCVN 96:2015/BTTTT (1)
 
- For equipment operating in the 1 GHz to 40 GHz frequency band:
QCVN 74:2020/BTTTT
QCVN 96:2015/BTTTT (1)
 
- For equipment not covered by QCVN 73:2013/BTTTT, QCVN 74:2020/BTTTT:
QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT (1)
	8526.92.00
	A device using radio waves to control models, and for control in the industrial and civil sectors.
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT.
- From July 01, 2024: apply QCVN 55:2023/BTTTT; Certificate of conformity issued under QCVN 55:2011/BTTTT remains effective until its expiry, including completion of applications for state inspection under QCVN 55:2023/BTTTT.
- For QCVN 55:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 55:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025.

	2.8
	Radio Frequency Identification (RFID) equipment
	- For equipment operating in the 9 kHz to 25 MHz frequency band:
QCVN 96:2015/BTTTT (1)
QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT
 
- For equipment operating in the 25 MHz to 1 GHz frequency band:
QCVN 73:2013/BTTTT
QCVN 96:2015/BTTTT (1)
 
For equipment operating in the 918,4 MHz to 923 MHz frequency band
QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT (1)
 
- For equipment operating in the 1 GHz to 40 GHz frequency band:
QCVN 74:2020/BTTTT
QCVN 96:2015/BTTTT (1)
	 
	Equipment using radio waves to automatically identify, track and manage goods, people, animals and other applications and including two separate units which are connected to each other via a radio interface:
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT.
- From July 01, 2024: apply QCVN 55:2023/BTTTT; Certificate of conformity issued under QCVN 55:2011/BTTTT remains effective until its expiry, including completion of applications for state inspection under QCVN 55:2023/BTTTT.
- For QCVN 55:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 55:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	
	8523.52.00
8523.59.10
	- Radio Frequency (RF) Tag attached to the object to be identified; only applicable to the types of tag with a power source.
Not including RFID equipment mentioned in 4.2 in the Appendix II to this Circular.
	

	
	
	
	8471.60.90
	- Radio Frequency Reader (RF reader) intended for activating the RF tag and transmitting the information received from the RF tag to the data processing system.
Not including RFID equipment mentioned in 4.2 in the Appendix II to this Circular.
	

	2.9
	Non-stop electronic toll collection system applying RFID
	QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT (1)
	 
	The non-stop electronic toll collection system applying RFID operating in the 920 MHz to 923 MHz frequency band with a radiated power of more than 500 mW ERP and including two separate units which are connected to each other via a radio interface:
	 

	
	
	
	8523.52.00
8523.59.10
	- Radio Frequency Tag attached to the object to be identified; only applicable to the types of tag with a power source.
	

	
	
	
	8471.60.90
	- Radio Frequency Reader (RF reader) intended for activating the RF tag and transmitting the information received from the RF tag to the data processing system.
	

	2.10
	Cordless audio devices
	QCVN 91:2015/BTTTT
QCVN 130:2022/BTTTT (1)
	8518.10.11
8518.10.19
8518.10.90
	Cordless headphones in the range 40,66 - 40,7 MHz; 87 - 108 MHz; 182,025 - 182,975 MHz; 217,025 - 217,975 MHz; 218,025 - 218,475 MHz; 470 - 694 MHz and 1795 - 1800 MHz.
	 

	
	
	
	8518.21.10
8518.21.90
8518.22.10
8518.22.90
8518.29.20
8518.29.90
	Cordless loudspeakers in the range 40,66 - 40,7 MHz; 87 - 108 MHz; 182,025 - 182,975 MHz; 217,025 - 217,975 MHz; 218,025 - 218,475 MHz; 470 - 694 MHz and 1795 - 1800 MHz.
	

	
	
	
	8518.30.10
8518.30.20 
	Cordless headphones in the range 40,66 - 40,7 MHz; 87 - 108 MHz; 182,025 - 182,975 MHz; 217,025 - 217,975 MHz; 218,025 - 218,475 MHz; 470 - 694 MHz and 1795 - 1800 MHz.
	

	
	
	
	8518.30.51 
8518.30.59 
8518.30.90
	Cordless loudspeakers in the range 40,66 - 40,7 MHz; 87 - 108 MHz; 182,025 - 182,975 MHz; 217,025 - 217,975 MHz; 218,025 - 218,475 MHz; 470 - 694 MHz and 1795 - 1800 MHz.
	

	2.11
	Ultra Wide Band (UWB) communications device
	QCVN 47:2015/BTTTT (2)
QCVN 94:2015/BTTTT (1)
	8517.62.59
	Devices utilizing Ultra Wide Band (UWB) technologies, intended for fixed (indoor only), mobile or portable applications and including:
- Stand-alone radio equipment with or without its own control provisions;
- Plug-in radio devices intended for use with, or within, a variety of host systems, e.g. personal computers, hand-held terminals, etc.;
- Plug-in radio devices intended for use within combined equipment, e.g. cable modems, set-top boxes, access points, etc.;
- Combined equipment or a combination of a plug-in radio device and a specific type of host equipment;
- Equipment for use in road and rail vehicles.
	 


Note: Certification and declaration of conformity of the commodities provided in the Appendix I in some cases:
(1) Regarding these technical regulations, the certification of conformity of the commodities herein is optional but the declaration of conformity thereof is compulsory.
(2) Upon application of QCVN 47:2015/BTTTT, in addition to the requirements enshrined in QCVN 47:2015/BTTTT, the commodities shall comply with Vietnam’s radio frequency planning.
(3) These types of commodities are not applicable to explosion-proof communication equipment.
(4) Short-range radio equipment in this section excludes receive-only radio equipment; wideband data transmission equipment operating in the 2,4 GHz band and having an equivalent isotropically radiated power of less than 60 mW; radio access equipment operating in the 5 GHz band and having an equivalent isotropically radiated power of less than 60 mW. It is only necessary to certify and declare conformity if the equipment meets the prescribed frequency band, technical conditions and operational conditions as set out in the Circular No. 08/2021/TT-BTTTT dated October 14, 2021 of the Minister of Information and Communications.
Conformity of wideband data transmission equipment and stand-alone radio access equipment operating in one or more bands that support the 6 GHz band (5,925 GHz to 7,125 GHz) (hereinafter referred to as “Wi-Fi 6E and Wi-Fi 7 equipment”) shall only be certified and declared provided that the manufacturer of Wi-Fi 6E and Wi-Fi 7 equipment has a written commitment confirming that the 6 GHz band has been disabled and the user cannot activate or use this band without the manufacturer's support.
Conformity of equipment integrated with functions of Wi-Fi 6E and Wi-Fi 7 equipment shall only be certified and declared provided that the manufacturer of Wi-Fi 6E and Wi-Fi 7 equipment has a written commitment confirming that the 6 GHz band has been disabled and the user cannot activate or use this band without the manufacturer's support.
(5) It is only necessary to certify and declare conformity if the equipment meets the prescribed frequency band, technical conditions and operational conditions as set out in the Circular No. 08/2021/TT-BTTTT dated October 14, 2021 of the Minister of Information and Communications on List of radio equipment which is exempt from a radio frequency license, with technical and operational conditions attached.
(6) Organizations and enterprises that produce, import, distribute and use base stations and repeaters shall undertake to strictly comply with the provisions of law on management and use of radio frequencies.
(7) For QCVN 117:2023/BTTTT, the requirements for Total Radiated Sensitivity (TRS) of the receiver in Article 2.2.12 and Total Radiated Power (TRP) in Article 2.2.13 of this technical regulation are yet to be applied.
(8) For QCVN 101:2020/BTTTT, it is only compulsory to declare conformity of the commodities herein with special safety requirements specified in Article 2.6 of this technical regulation.
(9) For QCVN 65:2021/BTTTT, in Article 2.1.2 of QCVN 65:2021/BTTTT, the formula (1) shall not be applied.
(10) For QCVN 128:2021/BTTTT, the requirement for 5G base station performance in Article 2.4 is yet to be applied. Upon application of QCVN 128:2021/BTTTT, the requirements in Appendix D to QCVN 128:2021/BTTTT shall apply to the equipment supporting bands n77 and n78, except for the requirement for spurious emission limits in section D.4 of QCVN 128:2021/BTTTT.
(11) For QCVN 131:2022/BTTTT: the requirements for Total Radiated Sensitivity (TRS) of the receiver in Article 2.2.12 and Total Radiated Power (TRP) in Article 2.2.13 of this technical regulation are yet to be applied.
(12) It is not permitted to use measurement/testing results given by any domestic or foreign testing laboratory that has not been designated or recognized or given by the manufacturer to assess the conformity with this technical regulation.
(13) For QCVN 132:2022/BTTTT, where commodities use adapters, if the adapters are attached, QCVN 132:2022/BTTTT shall be applied to test the commodities attached with adapters; if the adapters are not attached, QCVN 132:2022/BTTTT shall be applied to test the commodities not attached with adapters.
 
APPENDIX II
LIST OF INFORMATION TECHNOLOGY AND COMMUNICATIONS COMMODITIES SUBJECT TO DECLARATION OF CONFORMITY
((Enclosed with the Circular No. 02/2024/TT-BTTTT dated March 29, 2024 of the Minister of Information and Communications)
	No.
	Name of commodity
	Technical regulation
	HS code under Circular No. 31/2022/TT-BTC
	Description
	Provisions on application of technical regulations, certification  and declaration of conformity

	1
	Information technology equipment

	1.1
	Desktop computer
	QCVN 118:2018/BTTTT
QCVN 132:2022/BTTTT (12)(13)
	8471.41.10
	Comprising in the same housing at least a central processing unit and an input and output unit, whether or not combined, whether or not integrated with one or more functions:
- Wideband data transmission in the 2.4 GHz band;
- Radio access in the 5 GHz band;
- Land mobile terminal;
- Fifth generation (5G) mobile terminal;
- Short-range radio transmission and transmission - reception.
	 

	1.2
	Laptop and portable computer
	QCVN 118:2018/BTTTT
QCVN 101:2020/BTTTT (8)
QCVN 132:2022/BTTTT (12)(13)
	8471.30.20
	Portable automatic data processing machines, weighing not more than 10 kg, consisting of at least a central processing unit, a keyboard and a display, whether or not integrated with one or more functions:
- Wideband data transmission in the 2.4 GHz band;
- Radio access in the 5 GHz band;
- Land mobile terminal;
- Fifth generation (5G) mobile terminal;
- Short-range radio transmission and transmission - reception.
	 

	1.3
	Tablet
	QCVN 118:2018/BTTTT
QCVN 101:2020/BTTTT (8)
QCVN 132:2022/BTTTT (12)(13)
	8471.30.90
	Portable automatic data processing machines, weighing not more than 10 kg, consisting of at least a central processing unit, a keyboard and a display (other than laptops, notebooks and subnotebooks), whether or not integrated with one or more functions:
- Land mobile terminal;
- Fifth generation (5G) mobile terminal;
- Wideband data transmission in the 2.4 GHz band;
- Radio access in the 5 GHz band;
- Short-range radio transmission and reception.
	 

	2
	Radio and television equipment

	2.1
	Set Top Box for use in satellite television (except for DVB-S/S2 Set Top Box for use in satellite television)
	QCVN 118:2018/BTTTT
	8528.71.91
8528.71.99
	A Set Top Box in analogue form, not having a function of interactive information exchange.
	 

	2.2
	DVB- S/S2 Set Top Box
	QCVN 118:2018/BTTTT
	8528.71.91
8528.71.99
	Intended for receiving and decoding Free To Air (FTA) satellite television signals using DVB-S and/or DVB-S2 technology, supporting SDTV/HDTV, not having a communications function.
	 

	2.3
	Set Top Box for use in digital cable television networks
	QCVN 118:2018/BTTTT
QCVN 132:2022/BTTTT (12)(13)
	8528.71.11
8528.71.19
8528.71.91
8528.71.99
	Set Top Box for use in digital cable television networks, whether or not having a function of communications with the service provider.
	 

	2.4
	Set Top Box for use in digital IPTV television networks
	QCVN 118:2018/BTTTT
QCVN 132:2022/BTTTT (12)(13)
	8528.71.11
8528.71.19
8528.71.91
8528.71.99
	Set Top Box for use in digital IPTV television networks, whether or not having a function of communications with the service provider.
	 

	2.5
	Digital terrestrial television DVB-T2 Set Top Box
	QCVN 63:2020/BTTTT
QCVN 118:2018/BTTTT
	8528.71.91
8528.71.99
	Set Top Box using DVB-T2 technology for use in digital terrestrial television, not having a communications function.
	 

	2.6
	Digital receiver used in DVB-T2 digital terrestrial television broadcasting (iDTV)
	QCVN 63:2020/BTTTT
QCVN 118:2018/BTTTT
QCVN 132:2022/BTTTT (12)(13)
	8528.72.92
8528.72.99
	Digital receiver used in DVB-T2 digital terrestrial television broadcasting, designed to incorporate a video display or screen, having color, not battery operated and not using cathode-ray tubes.
	For QCVN 63:2020/BTTTT: the testing results given by other television sets using the same chassis/platform are permitted to be used for conformity declaration.
Chassis/Platform is a combination of three components: Tuner, main processing IC (IC with Demodulator and Decoder integrated inside), Software (or Firmware); or a combination of two components: Mainboard and Software (or Firmware).
Technical documents in the dossier on declaration of conformity and registration of quality inspection of imports must show that the television set uses the same chassis/platform. To be specific:
- Technical documents of types of television sets subject to declaration of conformity and registration of quality inspection of imports, sufficiently showing components of chassis/platform accompanied by codes of components of chassis/platform.
- The manufacturer's documents stating its undertaking that television sets use the same chassis/platform, List of television sets that use the same chassis/platform with the codes of components of the same chassis/platform.
- Test result of a type of television set on the List of television sets using the same chassis/platform, explicitly showing codes of the chassis/platform components.

	2.7
	Equipment in cabled distribution systems for television signal
	QCVN 72:2013/BTTTT
	8543.70.90
	Equipment in cabled distribution systems for television signals (carrier-current line systems or digital line systems).
	 

	3
	Radio transmitters and transceivers operating in the 9 kHz to 400 GHz frequency band and having effective radiated power of 60 mW or more

	3.1
	Radio transmitters and transceivers for use in land mobile or fixed services

	3.1.1
	Digital microwave radio equipment
	- For point-to-point radio equipment operating in the 1,4 GHz to 55 GHz frequency band:
QCVN 53:2017/BTTTT (12)(14)
QCVN 18:2022/BTTTT
 
- For digital microwave radio equipment that is not point-to-point radio equipment operating in the 1,4 GHz to 55 GHz frequency band:
QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT
	8517.62.59
	Transmission apparatus incorporating reception apparatus using digital microwave technology.
 
	- For QCVN 53:2017/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	3.1.2
	Terrestrial Trunked Radio (TETRA) equipment (3)
	QCVN 47:2015/BTTTT (2)
QCVN 100:2015/BTTTT
	 
	Terrestrial Trunked Radio (TETRA) equipment, including:
	 

	
	
	
	8517.61.00
	- Base Station (BS);
	

	
	
	
	8517.14.00
	- Mobile Station (MS);
- Direct Mode Mobile Station (DM-MS);
- Dual Watch Mobile Station (DW-MS);
	

	
	
	
	8517.62.59
 
	- Direct Mode REPeater (DM-REP), other than the phone;
- Direct Mode REPeater/GATEway (DM-REP/GATE), other than the phone;
- Trunked MOde REPeater (TMO-REP), other than the phone;
	

	
	
	
	8517.62.59
8517.62.69
	- Direct Mode GATEway (DM-GATE), other than the phone;
- Portable equipment of TErrestrial Trunked Radio (TETRA) radiocommunications systems, other than the phone.
	

	3.2
	Radio transmitters and transceivers used in satellite communications (excluding mobile stations used in maritime and aeronautical communications)

	3.2.1
	VSAT equipment (C band)
	QCVN 38:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT
	8517.62.59
	VSAT equipment (transmission apparatus incorporating reception apparatus) operating in C band through a geostationary satellite.
	- For QCVN 38:2011/BTTTT: suspend it in full until June 30, 2025.

	3.2.2
	VSAT equipment (Ku band)
	QCVN 39:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT
 
	8517.62.59
	VSAT equipment (transmission apparatus incorporating reception apparatus) operating in Ku band through a geostationary satellite.
	- For QCVN 39:2011/BTTTT: suspend it in full until June 30, 2025.

	3.2.3
	Mobile Earth Stations for Global Non-Geostationary Mobile-Satellite Service Systems in the Bands 1 - 3 GHz
	QCVN 40:2011/BTTTT
QCVN 18:2022/BTTTT
	8517.62.59
	Mobile Earth Stations for Global Non-Geostationary Mobile-Satellite Service Systems in the Bands 1 - 3 GHz (transmission apparatus incorporating reception apparatus).
	 

	3.2.4
	Mobile satellite Earth Station (MES) operating in the Ku band.
	QCVN 116:2017/BTTTT (12)
	8517.62.59
	Mobile Earth Stations (MES) (except for aeronautical mobile earth stations operating in the Ku band) operating in frequency ranges of the Fixed Satellite Service (FSS) (transmission apparatus incorporating reception apparatus):
- 10,70 GHz to 11,70 GHz (space to earth);
- 12,50 GHz to 12,75 GHz (space to earth);
- 14,00 GHz to 14,25 GHz (space to earth).
	 

	3.3
	Radio transmitters and transceivers used in the maritime mobile service (including ancillary equipment and satellite equipment)

	3.3.1
	VHF transmitter as coast station for GMDSS
	QCVN 24:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	 
	Transmitters, receivers and transmitters fitted with external antenna connectors, used as coast stations, operating in the VHF band of the maritime mobile service and utilizing emission G3E, and where relevant G2B for DSC signaling:
	- For QCVN 24:2011/BTTTT: suspend it in full until June 30, 2025.

	
	
	
	8517.62.53
	- Equipment capable of analogue speech, Digital Selective Calling (DSC), or both;
	

	
	
	
	8517.62.59
	- Equipment operating in the band 156 MHz - 174 MHz;
- Equipment operating under local or remote control;
- Equipment operating on 25 kHz channel spacing;
- Equipment operating in Simplex, Semi-Duplex (Half Duplex) and Duplex modes;
- Equipment which may consist of more than one unit;
- Equipment which may be single-channel or multi-channel;
- Equipment operating on shared radio sites;
- Equipment operating in isolation from other radio equipment.
	

	3.3.2
	Two-way VHF radiotelephone apparatus for fixed installation in survival craft
	QCVN 26:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.18.00
	Two-way VHF radiotelephone equipment, operating in the bands between 156 MHz and 174 MHz allocated to the Maritime Mobile Services and suitable for fixed installations in survival craft in accordance with the provisions of the Global Maritime Distress and Safety System (GMDSS).
	- For QCVN 26:2011/BTTTT: suspend it in full until June 30, 2025.

	3.3.3
	Inmarsat-C ship earth station equipment
	QCVN 28:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.62.59
	Inmarsat-C ship earth station equipment of the Global Maritime Distress and Safety System (GMDSS) (transmission apparatus incorporating reception apparatus).
	- For QCVN 28:2011/BTTTT: suspend it in full until June 30, 2025.

	3.3.4
	VHF radiotelephone used on the survival craft
	QCVN 50:2020/BTTTT (12)
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.18.00
	Portable VHF radiotelephones operating in the bands between 156 MHz and 174 MHz and suitable for use in survival craft and optionally, on board ships at sea.
	- For QCVN 50:2020/BTTTT: suspend it in full until June 30, 2025.

	3.3.5
	Emergency Position Indicating Radio Beacons (EPIRBs) operating in the 406,0 MHz to 406,1 MHz frequency band (5) 
	QCVN 57:2018/BTTTT (12)
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8526.91.10
 
	Satellite Emergency Position-Indicating Radio Beacons (EPIRB) (only used for radio telegraphy), operating in the COSPAS-SARSAT satellite system, concerning radio communications for the Global Maritime Distress and Safety System (GMDSS).
	- For QCVN 57:2018/BTTTT: suspend it in full until June 30, 2025.

	3.3.6
	Personal Locator Beacon (PLB) operating in the 406,0 MHz to 406,1 MHz frequency band
	QCVN 108:2016/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	 
	Satellite Personal Locator Beacons (PLBs) (only used for radio telegraphy), operating in the COSPAS-SARSAT satellite system. Satellite PLBs operate in the 406,0 MHz to 406,1 MHz frequency band and over the temperature ranges of:
- From -40°C to +55°C (Class 1); or
- From -20°C to +55°C (Class 2).
	- For QCVN 108:2016/BTTTT: suspend it in full until June 30, 2025.

	
	
	
	8526.91.10
	Of a kind for personal use in civil aircraft, or of a kind used solely on sea-going vessels.
	

	
	
	
	8526.91.90
	Other kind for personal use.
	

	3.3.7
	Emergency Locator Transmitter (ELT) (5)
	QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT
	8526.91.10
	Emergency Locator Transmitter (ELT) intended for use in aircrafts.
	 

	3.3.8
	Digital Selective Calling DSC
	QCVN 58:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.62.59
	Digital Selective Calling (DSC), not telephone, operating in the MF, MF/HF and/or VHF band in the Global Maritime Distress and Safety System (GMDSS) and normally used on board ships (transmission apparatus incorporating reception apparatus).
	- For QCVN 58:2011/BTTTT: suspend it in full until June 30, 2025.

	3.3.9
	Transponders for search and rescue radar (5)
	QCVN 60:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.62.59
	Search and rescue radar transponders operating in the frequency range 9200 - 9500 MHz (transmission apparatus incorporating reception apparatus).
	- For QCVN 60:2011/BTTTT: suspend it in full until June 30, 2025.

	3.3.10
	Radiotelex equipment operating in maritime MF/HF service
	QCVN 62:2011/BTTTT (15)
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.62.59
	Radiotelex equipment for use on board ships in the Global Maritime Distress and Safety System (GMDSS) (transmission apparatus incorporating reception apparatus).
	- For QCVN 62:2011/BTTTT: suspend it in full until June 30, 2025.
 

	3.3.11
	Shipborne equipment of the automatic identification systems (AIS) (5) 
	QCVN 68:2013/BTTTT (15)
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8526.91.10
	Radio navigational aid apparatus, used in shipborne automatic identification systems (detection of locations of ships within a certain range for the purposes of navigation and speed control).
	- For QCVN 68:2013/BTTTT: suspend it in full until June 30, 2025.

	3.3.12
	AIS Search and Rescue Transmitter (5)
	QCVN 107:2016/BTTTT (15)
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.62.53
	AIS Search and Rescue Transmitter (AIS SART) (transmission apparatus incorporating reception apparatus used for telegraphy).
	- For QCVN 107:2016/BTTTT: suspend it in full until June 30, 2025.

	3.3.13
	VHF radiotelephone for the maritime mobile service
	QCVN 52:2020/BTTTT (12)
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.18.00
	VHF transmitters used for telephone and Digital Selective Calling (DSC), fitted with an external antenna connector and used on board ships.
	- For QCVN 52:2020/BTTTT: suspend it in full until June 30, 2025.

	3.3.14
	MF and HF radio telephone
	QCVN 59:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.18.00
	Radio transmitters and receivers, for use on large ships, operating in either Medium Frequency (MF) only or in the Medium and High Frequency (MF/HF) bands allocated to the Maritime Mobile Service (MMS), including:
- Single Side Band (SSB) for telephony transmission and reception (J3F);
- Frequency Shift Keying (FSK) or SSB modulation of a keyed sub-carrier to transmit and receive Digital Selective Calling (DSC) signals;
- Radio equipment, not integrated with the DSC encoder or decoder, but the interfaces with such equipment are defined.
	- For 59:2011/BTTTT: suspend it in full until June 30, 2025.

	3.3.15
	UHF radio telephone
	QCVN 61:2011/BTTTT
QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8517.18.00
	UHF on board vessels radio equipment and systems operating on frequencies allocated to the maritime mobile services.
	- For 61:2011/BTTTT: suspend it in full until June 30, 2025.

	3.3.16
	Radar equipment used on sea-going vessels
	QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8526.10.10
8526.10.90
	All kinds of radar equipment used on sea-going vessels.
	Imported radar equipment used on sea-going vessels is exempted from quality inspection according to the Government’s Resolution 99/NQ-CP dated November 13, 2019 but is required to have its conformity declared before being put into use.

	3.4
	Radio transmitters and transceivers used in the aeronautical mobile service (including ancillary equipment and satellite equipment)

	3.4.1
	Ground-based radio equipment for the aeronautical mobile service using amplitude modulation in the frequency band 117,975 - 137 MHz
	QCVN 105:2016/BTTTT
QCVN 106:2016/BTTTT
	 
	DSB AM UHF radio transmitters or receivers and transmitters, with channel separations of 8,33 kHz or 25 kHz intended for analogue speech intended for ACARS data communication, including: 
	 

	
	
	
	8517.61.00
	- Ground based stations;
	

	
	
	
	8517.14.00
8517.62.59
8517.62.69
	- Mobile stations;
	

	
	
	
	8517.14.00
8517.62.59
8517.62.69
	- Portable stations and hand held radios for ground use.
	

	3.4.2
	Ground-based radio equipment for the aeronautical mobile service in the frequency band 117,975 - 137 MHz
	QCVN 47:2015/BTTTT (2)
QCVN 106:2016/BTTTT
	 
	Radio equipment for the aeronautical mobile service, operating in all or any part of the frequency band between 117,975 and 137 MHz, including:
	 

	
	
	
	8517.61.00
	Ground based stations;
	

	
	
	
	8517.14.00
8517.62.59
8517.62.69
	Mobile stations, portable stations and hand held radios for ground use.
	

	3.4.3
	Glidepath equipment for radio navigation aids
	QCVN 104:2016/BTTTT
QCVN 18:2022/BTTTT
	8526.91.10
	Ground-based glidepath equipment for radio navigation aids operating in the frequency band between 328,6 and 335,4 MHz.
	 

	3.5
	Radio transmitters and transceivers used for location and telemetry (except for those used offshore in petroleum industry)
	QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT
	8517.62.59
8517.62.69
	Radio transmitters and transceivers used for location and telemetry (except for those used offshore in petroleum industry) but not used for telegraph/telephone.
	 

	3.6
	Radio navigation aids
	QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT
	8526.91.10
8526.91.90
	Radio navigation aids used for the purposes of navigation and obstruction warning in the radionavigation-satellite service, aeronautical radionavigation service, aeronautical radionavigation-satellite service.
	 

	
	
	QCVN 47:2015/BTTTT (2)
QCVN 119:2019/BTTTT
	8526.91.10
8526.91.90
	Radio navigation aids used for the purposes of navigation and obstruction warning in the maritime radionavigation service, maritime radionavigation-satellite service.
	 

	3.7
	Amateur radio equipment
	QCVN 56:2011/BTTTT
	8517.62.59
	Radio transmitters and transceivers operating in the frequency range allotted to the amateur radio service (allocated according to the National Radio Spectrum Plan).
	 

	3.8
	Other equipment
	QCVN 47:2015/BTTTT (2)
QCVN 18:2022/BTTTT
	8517.62.59
8517.62.69
8517.62.99
8517.69.00
8526.10.10
8526.10.90
8526.91.10
8526.91.90
8526.92.00
	- Radio transmitters and transceivers operating in the frequency range between 9 kHz and 400 GHz and having an effective radiated power of 60 mW or more, which have not been included in section 1 of the List in the Appendix I and section 3 of the List in the Appendix II hereof.
- Radio transmitters and transceivers operating in the frequency range between 9 kHz and 400 GHz and having an effective radiated power of 60 mW or more, which have been included in section 1 of the List in the Appendix I and section 3 of the List in the Appendix II hereof but do not fall within the scope of the respective technical regulations applied.
	 

	4
	Short-range radio transmitters and transceivers (4)

	4.1
	Non-specific short-range radio transmitters and transceivers
	- For equipment operating in the 13,553-13,567 MHz frequency band:
QCVN 96:2015/BTTTT
QCVN 55:2011/BTTTT hoặc QCVN 55:2023/BTTTT
 
- For equipment operating in the 26,957-27,283 MHz; 40,66-40,7 MHz frequency band:
QCVN 73:2013/BTTTT
QCVN 96:2015/BTTTT
 
- For equipment operating in the 5725-5850 MHz; 24,00-24,25 GHz frequency band:
QCVN 74:2020/BTTTT (12)
QCVN 96:2015/BTTTT
	8517.62.59
8517.62.69
	Equipment fitted with an external antenna connector and/or integral antenna, and intended for transmission or reception of audio, images or other data; including equipment using active NFC (Near Field Communication) technology and mainly operating in the13,553-13,567 MHz, 26,957-27,283 MHz; 40,66-40,7 MHz, 5725-5850 MHz, 24,00-24,25 GHz frequency band.
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT.
- From July 01, 2024: apply QCVN 55:2023/BTTTT.
- For QCVN 55:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 55:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025. 

	
	
	- For equipment operating in the 61,0-61,5 GHz, 122- 123 GHz, 244-246 GHz frequency band:
QCVN 123:2021/BTTTT (12)
QCVN 18:2022/BTTTT
	8517.62.59
8526.92.00
	Radio alarm devices, remote control devices, general data communication devices, operating in the 61,0-61,5 GHz, 122-123 GHz, 244-246 GHz frequency band in the following cases:
- Either with a Radio Frequency output connection and dedicated antenna or with an integral antenna;
- With all types of modulation;
- Intended for fixed, mobile or nomadic use.
	- For QCVN 123:2021/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	
	8526.10.10
8526.10.90
	Telemetry device (short-distance measuring radar).
	

	4.2
	Radio Frequency Identification (RFID) equipment
	For equipment operating in the 13,553 MHz to 13,567 MHz frequency band:
QCVN 96:2015/BTTTT
QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT
	 
	Equipment using radio waves to automatically identify, track and manage goods, people, animals and other applications operating in the 13,553 MHz - 13,567 MHz frequency band and including two separate units which are connected to each other via a radio interface:
	- From the effective date of this Circular to June 30, 2024 inclusive: select to apply QCVN 55:2011/BTTTT or QCVN 55:2023/BTTTT.
- From July 01, 2024: apply QCVN 55:2023/BTTTT.
- For QCVN 55:2011/BTTTT: suspend the technical requirements under severe/critical conditions until June 30, 2024.
- For QCVN 55:2023/BTTTT: optionally apply the technical requirements under severe/critical conditions until June 30, 2025.

	
	
	
	8523.52.00
8523.59.10
	- Radio Frequency (RF) Tag attached to the object to be identified; only applicable to the types of tag with a power source.
	

	
	
	
	8471.60.90
	- Radio Frequency Reader (RF reader) intended for activating the RF tag and transmitting the information received from the RF tag to the data processing system.
	

	4.3
	Radar equipment used in road or railway transport and traffic
	For equipment operating in the 76 GHz to 77 GHz frequency band:
QCVN 18:2022/BTTTT
	8526.10.10
8526.10.90
	Short-range radar equipment operating in the 76 GHz to 77 GHz frequency band and intended for transport and traffic telematics applications (road or rail traffic) such as cruise control, protection, warning, and avoiding collisions between vehicles and other surrounding objects.
	 

	4.4
	Wireless Power Transfer
	QCVN 96:2015/BTTTT
	8504.40.19
8504.40.90
	A radio device that transmits electrical energy and signal from a power source to a receiver device according to electromagnetic induction theory (adapter).
	 

	4.5
	Telemetry device
	QCVN 73:2013/BTTTT
QCVN 96:2015/BTTTT
	8526.92.00
	A telemetry device automatically displaying or recording measurement data and controlling functions of other devices via a radio interface.
	 

	
	
	QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT
	8526.10.10
8526.10.90
	Short-range radar equipment, operating in the frequency range between 24 GHz and 24,25 GHz, intended for positioning and distance measurement applications (not being radar applications for road or railway transport and traffic).
	 

	4.6
	Medical Implant Communication System (MICS) and Medical Implant Test System (MITS)
	QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT
	8517.62.59
	A short-range radio transceiver operating in the frequency range between 401 MHz and 406 MHz, used in programmers or sensors and intended for remote data transmission.
	 

	4.7
	Wireless access equipment operating at Multiple-Gigabit data rates in the 60 GHz band
	QCVN 88:2015/BTTTT
QCVN 112:2017/BTTTT
	8517.62.51
	Applied to wireless access equipment operating at multiple-gigabit data rates and intended for short-range Wireless Personal Area Networks (WPAN) or Wireless Local Area Networks (WLAN) operating in the 60 GHz frequency range (not applied to radio equipment operating in the 60 GHz frequency range intended for outdoor Fixed Local Area Network Extension (FLANE) or Fixed Point-to-Point applications).
	 

	4.8
	Wireless digital video link equipment
	QCVN 92:2015/BTTTT
QCVN 93:2015/BTTTT
	 
	Wireless digital video link equipment operating in the 1,3 GHz to 50 GHz frequency band and using maximum allowable channel bandwidths of 5 MHz, 10 MHz and 20 MHz, including:
	 

	
	
	
	8525.50.00
	- Transmitter;
	

	
	
	
	8525.60.00
	- Transmitter incorporating receiver.
	

	4.9
	Short-range radio transmitters and transceivers
	- For equipment operating in the 9 kHz to 40 GHz frequency band: 
QCVN 47:2015/BTTTT (2)
QCVN 96:2015/BTTTT
 
- For equipment operating in the frequency range of more than 40 GHz: 
QCVN 18:2022/BTTTT
	8517.62.59
8526.10.10
8526.10.90
8526.92.00
	- Short-range radio transmitters and transceivers not included in section 2 of the List in the Appendix I hereof and section 4 of the List in the Appendix II hereof;
- Short-range radio transmitters and transceivers that have been included in section 2 of the List in the Appendix I hereof and section 4 of the List in the Appendix II hereof but do not fall within the scope of the respective technical regulations applied.
	 

	5
	Lithium batteries for portable applications

	5.1
	Lithium batteries for laptops, mobile phones and tablets
	QCVN 101:2020/BTTTT (8)
	8507.60.90
	Stand-alone lithium batteries for mobile phones. Not applicable to stand-alone lithium batteries that are rechargeable batteries for charging mobile phones.
	 

	
	
	
	8507.60.31
	Stand-alone lithium batteries for laptops and tablets. Not applicable to stand-alone lithium batteries that are rechargeable batteries for charging mobile phones.
	


Note: Declaration of conformity of the commodities provided in the Appendix II in some cases:
(2) Upon application of QCVN 47:2015/BTTTT, in addition to the requirements enshrined in QCVN 47:2015/BTTTT, the commodities shall comply with Vietnam’s radio frequency planning.
(3) These types of commodities are not applicable to explosion-proof communication equipment.
(4) Short-range radio equipment in this section excludes receive-only radio equipment; wideband data transmission equipment operating in the 2,4 GHz band and having an equivalent isotropically radiated power of less than 60 mW; radio access equipment operating in the 5 GHz band and having an equivalent isotropically radiated power of less than 60 mW. It is only necessary to declare conformity if the equipment meets the prescribed frequency band, technical conditions and operational conditions as set out in the Circular No. 08/2021/TT-BTTTT of the Minister of Information and Communications.
Conformity of wideband data transmission equipment and stand-alone radio access equipment operating in one or more bands that support the 6 GHz band (5,925 GHz to 7,125 GHz) (hereinafter referred to as “Wi-Fi 6E and Wi-Fi 7 equipment”) shall only be declared provided that the manufacturer of Wi-Fi 6E and Wi-Fi 7 equipment has a written commitment confirming that the 6 GHz band has been disabled and the user cannot activate or use this band without the manufacturer's support.
Conformity of equipment integrated with functions of Wi-Fi 6E and Wi-Fi 7 equipment shall only be declared provided that the manufacturer of Wi-Fi 6E and Wi-Fi 7 equipment has a written commitment confirming that the 6 GHz band has been disabled and the user cannot activate or use this band without the manufacturer's support.
(5) It is only necessary to declare conformity if the equipment meets the prescribed frequency band, technical conditions and operational conditions as set out in the Circular No. 08/2021/TT-BTTTT dated October 14, 2021 of the Minister of Information and Communications on List of radio equipment which is exempt from a radio frequency license, with technical and operational conditions attached.
(8) For QCVN 101:2020/BTTTT, it is only compulsory to declare conformity of the commodities herein with special safety requirements specified in Article 2.6 of the Regulation.
(12) It is not permitted to use measurement/testing results given by any domestic or foreign testing laboratory that has not been designated or recognized or given by the manufacturer to assess the conformity with this technical regulation.
(13) For QCVN 132:2022/BTTTT, where commodities use adapters, if the adapters are attached, QCVN 132:2022/BTTTT shall be applied to test the commodities attached with adapters; if the adapters are not attached, QCVN 132:2022/BTTTT shall be applied to test the commodities not attached with adapters.
(14) For QCVN 53:2017/BTTTT: the requirement for antenna in Article 2.3 of the Technical Regulation is yet to be applied.
(15) The electromagnetic compatibility requirements specified in this technical regulation shall not apply.
 
 

