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DECREE
ON LIST OF DANGEROUS GOODS, TRANSPORT OF DANGEROUS GOODS BY ROAD MOTOR VEHICLES AND INLAND WATERCRAFT
Pursuant to the Law on Government Organization dated June 19, 2015 and the Law on Amendments to the Law on Government Organization and the Law on Local Government Organization dated November 22, 2019;
Pursuant to the Law on Road Traffic dated November 13, 2008;
Pursuant to the Law on Atomic Energy of Vietnam dated June 3, 2008;
Pursuant to the Law on Chemicals dated June 29, 2018;
The Law on Environmental Protection dated November 17, 2020;
Pursuant to Law on  Inland Waterway Transport dated June 15, 2004 and Law on Amendment to some Articles of the Law on Inland Waterway Transport dated June 17, 2014;
At the request of the Minister of Transport;
The government hereby promulgates a Decree on list of dangerous goods, transport of dangerous goods by road motor vehicles and inland watercraft.
Chapter I
GENERAL PROVISIONS 
Article 1. Scope 
1. This Decree provides for list of dangerous goods, transport of dangerous goods and grant of licences to transport dangerous goods by road motor vehicles and by inland waterways.
2.  Radioactive substances shall be transported in accordance with the regulations of this Decree and laws on atomic energy.
3. Weapons, explosives, combat gears, explosives precursors and pyrotechnics shall be transported in accordance with laws on weapons, explosives, combat gears, explosives precursors and pyrotechnics. 
4. Dangerous goods serving national defense and security tasks of armed forces shall be transported in compliance with regulations of this Decree and in accordance with the organization and management of the Minister of Public Security and Minister of National Defense.
5. Hazardous waste shall be transported according to the regulations of this Decree and laws on environmental protection.
6. In case of conflict between a regulation of this Decree and a regulation of a law on atomic energy, weapons, explosives, combat gears, explosives precursors, pyrotechnics, environmental protection, or fire prevention and fighting, the regulation of the law on atomic energy, weapons, explosives, combat gears, explosives precursors and pyrotechnics, environmental protection or fire prevention and fighting shall prevail.
Article 2. Regulated entities
1. This Decree is applied to Vietnamese and foreign organizations and individuals involved in transport of dangerous goods by road motor vehicles and by inland waterways within the territory of the Socialist Republic of Vietnam.
2. The Prime Minister has the power to decide application of special regulations and measures to transport dangerous goods in the following cases:
a) Urgent transport of goods for prevention and control of infectious diseases, acts of god or conflicts;
b) Transit of goods from countries and international organizations that are not signatories to Vietnam-related international conventions.
Article 3. Definitions 
For the purposes of this Decree, the terms below are construed as follows:
1. “dangerous substance” refers to a gas, liquid or solid substance or compound that may pose a threat to human life or health, the environment or national security and safety.
2. “dangerous goods” means goods containing dangerous substances that are a risk to human life or health, the environment or national security and safety when transported by land or inland waterways.
3. “carrier" means an organization or individual that uses a road motor vehicle or an inland watercraft to transport dangerous goods.
4. “consignor” refers to an organization or individual that has concluded a contract on transport of dangerous goods by land or inland waterways with the carrier.
5. “loader" means an organization or individual involved in loading and unloading of dangerous goods into or from a road motor vehicle or an inland watercraft or at a warehouse or yard storing dangerous goods.
6. “consignee” means an organization or individual whose name is written on the consignment note.
7. “driver/operator" means a driver of a road motor vehicle or a crew member or operator of an inland watercraft.
8. “escort" refers to an individual employed by the consignor (or goods owner) for the secure carriage of dangerous goods during the transport.
9. “warehouse-keeper” means the main person responsible for managing the status and quantity of all goods from the time they are transferred into the warehouse until they leave the warehouse.
Chapter II
CLASSIFICATION, LISTING, PACKING, LABELLING OF DANGEROUS GOODS AND DANGEROUS GOODS TRAINING PROVISION 
Article 4. Classification of dangerous goods
1. Based on their chemical and physical characteristics, dangerous goods are classified into the 9 following classes and divisions:
a) Class 1. Explosives;
Division 1.1: Substances and articles which have a mass explosion hazard.
Division 1.2: Substances and articles which have a projection hazard but not a mass explosion hazard.
Division 1.3: Substances and articles which have a fire hazard and either a minor blast hazard or a minor projection hazard or both, but not a mass explosion hazard.
Division 1.4: Substances and articles which are classified as explosives but which present no significant hazard.
Division 1.5: Very insensitive substances which have a mass explosion hazard.
Division 1.6: No hazard statement.
b) Class 2. Gasses.
Division 2.1: Flammable gases.
Division 2.2: Non-flammable non-toxic gases.
Division 2.3: Toxic gases.
c) Class 3. Flammable liquids and liquid desensitized explosives.
d) Class 4;
Division 4.1: Flammable solids, self-reactive substances and solid desensitized explosives.
Division 4.2: Substances liable to spontaneous combustion.
Division 4.3: Substances which in contact with water emit flammable gases.
dd) Class 5;
Division 5.1: Oxidizing substances.
Division 5.2: Organic peroxides.
e) Class 6;
Division 6.1: Toxic substances.
Division 6.2: Infectious substances.
g) Class 7: Radioactive materials;
h) Class 8: Corrosive substances;
i) Class 9: Miscellaneous dangerous substances and articles.
2. Containers and wrappings of dangerous goods that have not been cleaned inside and outside after all goods are unloaded shall also be deemed to be dangerous goods.
Article 5. List of dangerous goods
1. List of dangerous goods which are classified into appropriate classes and divisions and associated UN substance identification numbers and hazard identification numbers is prescribed in Appendix I of this Decree.
2. The hazard level of each substance in the list of dangerous goods is expressed in terms of a hazard identification number consisting of two or three figures which is provided for in Appendix II of this Decree.
Article 6. Packages and containers of dangerous goods
1. Packages and containers of dangerous goods and packaging of dangerous goods in Vietnam’s territory must satisfy the national standards (TCVN) or national technical regulations (QCVN) or relevant laws applicable to such goods. Packages and containers of imports shall comply with the manufacturer's recommendations and requirements.
2.  In case national standards, national technical regulations or relevant laws or international technical standards or regulations announced by relevant ministries have not been provided for, at least the following requirements must be satisfied:
a) Quality of packages and containers must be capable of withstanding shocks and vibrations during transport or transit among vehicles and loading/unloading;
b) Packages and containers must be constructed and closed so as to prevent any loss of contents when prepared for transport which may be caused under normal conditions of transport, by vibration, or by changes in temperature, humidity or pressure;
c) No dangerous residue shall adhere to the outside of packages and containers;
d) Parts of packages and containers that are in direct contact with dangerous substances must be designed to ensure that they are not affected or degraded in quality due to the impact of dangerous substances packed inside; do not affect the composition, features and effects of dangerous goods;
dd) Packages and containers of dangerous goods in a liquid state must be designed to ensure that neither leakage nor permanent distortion occurs as a result of expansion of the liquid caused by changes in temperature; also have an appropriate resistance to the internal pressure that may be developed under normal conditions of transport; conforms to a design type which has passed the drop test before leaving factories;
e) Inner packages and containers that are liable to break or be punctured easily such as those made of glass, porcelain or stoneware or of certain plastics materials, etc., shall be secured in outer packages and containers with suitable cushioning materials; 
g) Packages and containers containing volatile substances must be designed to ensure that they are kept from evaporating under normal conditions of transport at the manufacturer's request;
h) Packages and containers of dangerous goods in solid state, granules or powders, shall be designed to ensure that they are not scattered during loading and unloading or under normal conditions of transport. 
Article 7. Hazard labels, placards and signs
1. Dangerous goods shall be labelled in accordance with regulations of the Law on Chemicals and laws on goods labels.
2. Hazard placards and signs shall be affixed at a location easily noticed on outer packages and containers.  Size, designs and colours of hazard placards are provided for in Appendix III enclosed therewith.
3. Rectangular hazard signs, their size and colours are provided for using the form specified in Appendix III enclosed therewith. Hazard signs shall be affixed under hazard placards.
Article 8. Dangerous goods training
1. Organization of dangerous goods training
a) Consignors or carriers shall organize dangerous goods training or appoint subjects prescribed in clause 2 of this Article to join training courses of units in charge of dangerous goods training every 02 years;
b) Dangerous goods training shall be organized separately or in combination with other safety training;
c) Persons who have completed dangerous goods training courses must be retrained in the following cases: When there is a change in the category of dangerous goods during transport; when the trained person changes their working position; after 02 inspections of unsatisfactory trained persons; upon expiry of 02 years from the previous training.
2. Operators, escorts, warehouse-keepers and loaders involved in the transport of dangerous goods must be trained.
3. Dangerous goods training contents
a) Dangerous goods training contents must be appropriate to the position and responsibilities of the trainee; nature, type of hazard and level of hazard of dangerous goods. The training manual shall be compiled by consignors or carriers in accordance with classes and divisions specified in Article 4 of this Decree;
b) Training contents include: name of dangerous goods, dangerous nature, classification and labelling; safety risks during storage, loading, unloading, and transportation of dangerous goods; Storage, loading, unloading, and transportation procedures appropriate to the working location; dangerous goods safety regulations; incident response procedures: Use rescue equipment to handle fires, explosions, leaks, dispersal of dangerous substances, provide first aid to victims in incidents, use, preserve, and check safety equipment, vehicles, personal protective equipment to respond to incidents, incident reporting flowchart, cooperate with competent authorities to mobilize resources to respond, troubleshoot incidents, prevent and limit sources of pollution spreading to the environment, collect spilled dangerous substances, and repair the environment after incidents.
4. A dangerous goods training instructor must has either a bachelor’s degree or a higher degree and has at least 5 years of relevant professional work experience.
5. The minimum duration of dangerous goods training shall be 16 hours for each class and division of dangerous goods, including testing period.
6. Evaluating results and maintaining records of dangerous goods training
a) Consignor or carrier or person in charge of dangerous goods training shall take a test for evaluating results of the dangerous goods training;
b) The test of training contents: the test contents must be consistent with the training contents. The maximum testing period is 02 hours. The trainee must achieve at least an average score to pass the test;
c) Within 07 working days from the day on which the dangerous goods training and testing course is completed, the training and testing provider shall make a decision to recognize the testing result and grant a dangerous goods certificate.
7. A dangerous goods training record includes: Training content; list of trainees with information: Full name, date of birth, title, working position, signature confirming participation in training; Information about the instructor includes: Full name, date of birth, educational qualifications, professional qualifications, work experience, accompanied by documentation; testing content and result of the dangerous goods training; Decision to recognize the testing result of dangerous goods training of the provider.
8. The provider shall keep all of the record prescribed in clause 7 of this Article for 03 years and submit them to regulatory authorities upon request.
Chapter III
TRANSPORT OF DANGEROUS GOODS
Section 1. TRANSPORT OF DANGEROUS GOODS BY ROAD MOTOR VEHICLES
Article 9. Requirements for participants in transport of dangerous goods
1. Operators of vehicles carrying dangerous goods (hereinafter referred to as “vehicles”) must satisfy all conditions for operating these vehicles and must receive training and obtain a certificate of completion of dangerous goods training programme according to regulations of this Decree.
2. Escorts, warehouse-keepers, loaders of dangerous goods must receive training and obtain a certificate of completion of dangerous goods training programme applicable to the classes of dangerous goods that they escort, load/unload or store.
Article 10. Requirements for vehicles carrying dangerous goods
1. Vehicles must be roadworthy according to regulations of law.  Specialized equipment of such vehicles must satisfy national technical standards or national technical regulations or regulations of relevant ministries.
2. Each vehicle must have hazard placards affixed on both of its sides as well as on the front and rear in a manner that is easy to observe and recognize. If a vehicle carries multiple classes of dangerous goods, it must be affixed with hazard placards for all those classes of goods.
3. Vehicles must be cleaned and have all hazard placards removed from their bodies when all cargoes have been unloaded and the vehicles no longer transport the same classes of goods. Transport units, operators shall clean and remove the hazard placards from vehicles when the vehicles no longer transport the same classes of goods.
Article 11. Loading and unloading and storage of dangerous goods in warehouses or yards
1. Organizations and individuals involved in loading, unloading and storage of dangerous goods in warehouses or yards must adhere to the guidelines on preservation, loading, unloading and transport of each class of dangerous goods or the instructions provided by the consignor.
2. Loading and unloading of dangerous goods must be directly instructed and supervised by the warehouse-keeper, consignor or escort. Classes of dangerous goods that might react to each other and increase the level of hazard shall not be transported on the same vehicle. Classes and divisions of dangerous goods that require separate loading, unloading and storage must be loaded and unloaded at separate warehouses or yards.
3. When transporting dangerous goods that do not require escorts, the carrier shall load and unload the goods following the consignor's instructions.
4. After all dangerous goods have been moved out, warehouses and yards must be cleaned to avoid affecting other classes of goods.
Article 12. Transport of flammable and explosive substances through tunnels and on ferries
1. Explosives, gases, gasoline, oils and other flammable and explosive substances, solid desensitized explosives shall not be transported through tunnels longer than 100m.
2. A vehicle transporting explosives, gases, gasoline, oils and other flammable and explosive substances shall not be transported together with road users or passengers on a ferry.
Section 2. TRANSPORT OF DANGEROUS GOODS BY INLAND WATERWAYS
Article 13. Requirements for participants in transport of dangerous goods
1. Crew members and drivers working on inland watercraft carrying dangerous goods must receive training and obtain a professional qualification of transport of dangerous goods according to regulations of the Minister of Transport; receive training and obtain a certificate of completion of dangerous goods training programme according to regulations herein.
2. Escorts, warehouse-keepers, loaders of dangerous goods working on inland watercraft and at inland waterway ports and terminals must receive training and obtain a certificate of completion of dangerous goods training programme applicable to the dangerous goods that they escort, load/unload or store.
Article 14. Requirements for inland watercraft carrying dangerous goods (hereinafter referred to watercraft)
1. Watercraft must be seaworthy according to regulations of law. 
2. Each watercraft must have hazard placards affixed on both of its sides. If a watercraft carries multiple classes of dangerous goods, it must be affixed with hazard placards for all those classes of goods.
3. Watercraft must be cleaned and have all hazard placards removed from its body when all cargoes have been unloaded and the watercraft no longer transports the same class of goods. Transport unit, crew members or operator of inland watercraft shall clean and remove the hazard placards from the watercraft when the watercraft no longer transports the same class of goods.
Article 15. Loading and unloading and storage of dangerous goods in warehouses or yards
Loaders must load and unload dangerous goods according to regulations on loading and unloading of goods on inland watercraft and the following regulations:
1. Loading and unloading of dangerous goods must be directly instructed and supervised by the warehouse-keeper, consignor or escort; and the captain shall decide positions of the dangerous goods on their watercraft and decide cargo-securing measures suitable to each class or division of dangerous goods. Classes of dangerous goods that might react to each other and increase the level of hazard shall not be placed in the same hold or hatch on the watercraft.
2. When transporting dangerous goods that do not require escorts, the carrier shall load and unload the goods following the consignor's instructions.
3. Classes and divisions of dangerous goods that require separate loading, unloading and storage must be loaded and unloaded at separate wharfs, terminals or warehouses.
4. After all dangerous goods have been moved out, warehouses and yards must be cleaned to avoid affecting other classes of goods.
Chapter IV
DANGEROUS GOODS TRANSPORT LICENCE
Article 16. Contents, template and effective period of the dangerous goods transport licence
1. A dangerous goods transport licence (hereinafter referred to as “licence”) shall consist of the following information
a) Name, address and phone number of the licence holder; full name and title of the legal representative;
b) Class and division of the dangerous goods;
c) Transport route and schedule (if the licence is granted separately to each trip);
d) Effective period of the licence.
If the licence is granted separately to each trip, it must include information on the vehicle and operator/driver thereof, escort(s) (if the transport of dangerous goods requires escort(s)).
2. Each licence template must have a QR code thereon and danger signs provided by the licensing authority. 
3. Licences are valid nationwide. The effective period of a licence is that requested by the carrier but does not exceed 24 months and the service life of the vehicle.
Article 17. Authority to grant licences and cases of exemption from grant thereof
1. Ministry of Public Security shall organize grant of licences to transport dangerous goods of class 1, class 2, class 3, class 4 and class 9 prescribed in Clause 1 Article 4 of this Decree (excluding crop protection chemicals and regulations in clause 2 of this Article).
2. Ministry of National Defense shall organize grant of licences to organizations and enterprises under its management.
3. Ministry of Science and Technology shall organize grant of licences to transport dangerous goods of class 5 and class 8 prescribed in Clause 1 Article 4 of this Decree.
4. The People’s Committees of provinces and municipalities shall organize grant of licences to transport dangerous crop protection chemicals.
5. Agencies issuing licences (hereinafter referred to as “licensing authorities”) shall decide transport routes and schedules for classes and divisions of dangerous goods specified in clause 1 Article 4 of this Decree.
6. The licence to transport dangerous goods of class 7 shall be granted according to regulations in Decrees on radiation work and auxiliary atomic energy application services.
7. Licensing authorities shall refuse to grant licences to transport flammable and explosive substances through tunnels or on ferries as prescribed in Article 12 of this Decree.
8. Licences in accordance with regulations herein are not required for the following cases:
a) Transport of less than 1.080 kilogram of liquefied natural gas (LNG) and compressed natural gas (CNG) in total;
b) Transport of less than 2.250 kilogram of liquefied petroleum gas (LPG) in total;
c) Transport of less than 1.500 liter of liquid fuels in total;

d) Transport of less than 1.000 kilogram of crop protection chemicals in total;
dd) Transport of other dangerous substances of each class or division of dangerous goods.
9. Vehicles are not required to be licensed to transport dangerous goods prescribed in clause 8 of this Article shall ensure fire prevention and fighting safety requirements as prescribed by laws on fire prevention and fighting during transportation.
Article 18. Applications for grant or renewal of licences
1. An application for grant or renewal of a licence includes:
a) An application form for the licence made using the form in Appendix IV of this Decree;
b) A certified true copy or certified true electronic copy  or original of the list of vehicles used for the transport  with unexpired certificates of roadworthiness; 
c) A certified true copy or certified true electronic copy or original of the list of drivers/operators of the vehicle carrying dangerous goods (including, full name; ID card number or citizen identification number or passport number; licence number, licence class (for drivers); number of the professional qualification, class (for crew members)) and the list of escorts in cases where an escort is required (including: Full name, ID card number or citizen identification number or passport number) and a certified true copy of the certificate of completion of dangerous goods training programme;
d) A certified true copy or certified true electronic copy or original of the dangerous goods transport plan prepared by the transport unit using the form in Appendix V of this Decree (which includes at least the following contents: Vehicle licence plate; full name of vehicle driver/operator; class of goods; mass; transport route, transport schedule; measures to respond to chemical incidents in transport of dangerous goods);
dd) A certified true copy or certified true electronic copy of the certificate of completion of dangerous goods training programme (for drivers of vehicles carrying dangerous goods by road motor vehicles); A certified true copy or certified true electronic copy of the professional qualification (for crew members transporting dangerous goods by inland watercraft).
2. An application for grant of a licence to transport dangerous goods of class 1, class 2, class 3, class 4 and class 9 includes:
a) An application form for the licence made using the form in Appendix IV of this Decree;
b) A certified true copy or certified true electronic copy or original of the list of vehicles used for the transport  with unexpired certificates of roadworthiness; 
c) A certified true copy or certified true electronic copy or original of the list of drivers/operators of the vehicle carrying dangerous goods (including, full name; ID card number or citizen identification number or passport number; licence number, licence class (for drivers); number of the professional qualification, class (for crew members)) and the list of escorts in cases where an escort is required (including: Full name, ID card number or citizen identification number or passport number) and a certified true copy of the certificate of completion of dangerous goods training programme;
d) A certified true copy or certified true electronic copy of the certificate of completion of dangerous goods training programme (for drivers of vehicles carrying dangerous goods by road motor vehicles); A certified true copy or certified true electronic copy of the professional qualification (for crew members transporting dangerous goods by inland watercraft);
dd) A certified true copy or certified true electronic copy or original of the dangerous goods transport plan prepared by the transport unit using the form in Appendix V of this Decree (which includes at least the following contents: Vehicle licence plate; full name of vehicle driver/operator; class of goods; mass; transport route, transport schedule; emergency management in case of fire or explosion incidents); A certified true copy or certified true electronic copy or original of the Oil spill response plan (only applicable to petroleum transport on inland waterways).
3. An application for grant of a licence to transport crop protection chemicals includes:
a) An application form for the licence made using the form in Appendix IV of this Decree;
b) A certified true copy or certified true electronic copy or original of the list of vehicles used for the transport with unexpired certificates of roadworthiness; 
c) A certified true copy or certified true electronic copy or original of the list of drivers/operators of the vehicle carrying dangerous goods (including, full name; ID card number or citizen identification number or passport number; licence number, licence class (for drivers); number of the professional qualification, class (for crew members)) and the list of escorts in cases where an escort is required (including: Full name, ID card number or citizen identification number or passport number) and a certified true copy of the certificate of completion of dangerous goods training programme;
d) A physical copy or electronic copy or original of the supply contract or financial invoice for the import and export of pesticides;
dd) A certified true copy or certified true electronic copy or original of the dangerous goods transport plan prepared by the transport unit using the form in Appendix V of this Decree (which includes at least the following contents: Vehicle licence plate; full name of vehicle driver/operator; class of goods; mass; transport route, transport schedule);
e) A certified true copy or certified true electronic copy of the certificate of completion of dangerous goods training programme (for drivers of vehicles carrying dangerous goods by road motor vehicles); A certified true copy or certified true electronic copy of the professional qualification (for crew members transporting dangerous goods by inland watercraft);
4. An application for modifying a licence if there is a change relating to contents of the licence includes:
a) An application form for modifying the licence made using the form in Appendix IVa of this Decree;
b) Documentary evidence for the changes.
5. An application for renewal of a licence upon loss or damage includes an application form for renewal of the licence with reasons for the loss or damage.
Article 19. Procedures for grant or renewal of licences
1. Procedures for grant of a licence
a) The carrier shall submit an application for grant of the licence according to regulations in Clause 1, Clause 2 or Clause 3 of Article 18 of this Decree to a licensing authority.
If the application is submitted in person, the competent administrative authority shall verify the application components and reply as soon as the application is submitted by the applicant; and instruct the applicant to complete the application if it is inadequate or incorrect.
In case the application is submitted by post or the online public services system, within 01 working day after receiving the application, the competent administrative authority shall consider the validity of the application; if the application is invalid, the competent administrative authority shall notify in writing or via the online public services system to the applicant for supplementation and provide instructions on completion of the application.
Licences to transport dangerous goods of class 7 shall be granted according to regulations on radiation work and auxiliary atomic energy application services;
b) Within 05 working days from the date of receipt of the adequate application, the licensing authority shall appraise the application.  If the licensing authority refuses to grant a licence, the authority must inform the applicant in writing or via the online public service system of the refusal and of the reasons for the refusal.
2. Procedures for modifying a licence if there is a change relating to the licence's contents
a) The carrier shall submit an application for grant of the licence according to regulations in Clause 4 Article 18 of this Decree to a licensing authority.
If the application is submitted in person, the competent administrative authority shall verify the application components and reply as soon as the application is submitted by the applicant; and instruct the applicant to complete the application if it is inadequate or incorrect.
In case the application is submitted by post or the online public service system, within 01 working day after receiving the application, the competent administrative authority shall consider the validity of the application; if the application is invalid, the competent administrative authority shall notify in writing or via the online public service system to the applicant for supplementation and provide instructions on completion of the application.
b) Within 03 working days from the date of receipt of the adequate application, the licensing authority shall appraise the application and grant a written document modifying the licence’s contents. If the application is rejected, the licensing authority shall explain the reason to the applicant in writing or via the online public services system.
3. Procedures for renewal of a licence if it is lost or destroyed
a) The carrier shall submit an application for renewal of the licence according to regulations in Clause 5 Article 18 of this Decree to a licensing authority.
If the application is submitted in person, the competent administrative authority shall verify the application components and reply as soon as the application is submitted by the applicant; and instruct the applicant to complete the application if it is inadequate or incorrect.
In case the application is submitted by post or the online public service system, within 01 working day after receiving the application, the competent administrative authority shall consider the validity of the application; if the application is invalid, the competent administrative authority shall notify in writing or via the online public service system to the applicant for supplementation and provide instructions on completion of the application;
b) Within 02 working days from the date of receipt of the adequate application, the licensing authority shall appraise the application.  If the licensing authority refuses to renew a licence, the authority must inform the applicant in writing or via the online public service system of the refusal and of the reasons for the refusal.
4. During transport of dangerous goods, if there is any change to the vehicles and/or drivers listed in the approved licence application, the transport unit must send a notification of the list enclosed with a dossier on the substitute vehicles and drivers to the licensing authority at least 03 working days before transporting the dangerous goods.
Within 01 working day from the date of receipt of the notification enclosed with the dossier from the transport unit, the licensing authority shall verify and send a written notification of the list of substitute vehicles and drivers. If the application is rejected, the licensing authority shall explain the reason to the applicant in writing or via the online public services system.
5. Applications shall be received and results shall be informed at offices of licensing authorities or by post or via the internet environment.
Article 20. Revocation of licences
1. A carrier will have his/her licence revoked in one of the following cases:
a) The carrier provides a copy inconsistent with its original or erroneous information in the application for grant of the licence;
b) The carrier does not transport dangerous goods in accordance with the application for grant of the licence or the licence granted;
c) The carrier terminates his/her operation according to regulations of law;
d) The carrier employs participants in the transport of dangerous goods who do not receive dangerous goods training as prescribed. 
2. A licensing authority has the power to revoke a licence that it granted following the procedure belows:
a) Promulgate a decision to revoke the licence;
b) Send the licence revocation decision to the carrier and post it on the licensing authority’s website (if any);
c) Upon promulgation of the licence revocation decision, the carrier shall submit his/her licence to the licensing authority and stop transporting dangerous goods according to the licence revocation decision immediately after its entry into force. If the carrier commits the violations specified in point a, point b and point d clause 1 of this Article, which leads to revocation of the licence, the licensing authority shall not renew the licence for 30 days from the entry into force of the licence revocation decision. After these 30 days, if the carrier wishes to continue transporting dangerous goods, the carrier shall reapply for the licence according to the regulations in Article 18 of this Decree;
d) Announce the revocation of the granted licence via mass media, on web portal or website of the licensing authority.
Chapter V
IMPLEMENTATION 
Article 21. Ministry of Transport shall:
1. Take charge and cooperate with relevant ministries and central authorities in amending the list of dangerous goods and proposing it to the Government for promulgation; consolidating reports on transport of dangerous goods in accordance with this Decree.
2. Promulgate national technical regulations on technical safety and environmental protection applicable to inland watercraft and road motor vehicles carrying dangerous goods and specialized equipment permanently attached to these vehicles/watercraft.
3. Cooperate with relevant ministries in management, inspection and handling of violations concerning transport of dangerous goods.
Article 22. Ministry of Public Security shall: 
1. Manage the list of dangerous goods of class 1 and class 4 within the Ministry's jurisdiction; manage transport of dangerous goods and grant licences according to Clause 1 Article 17 of this Decree.
2. Cooperate with the Ministry of Transport, the Ministry of National Defense, the Ministry of Industry and Trade and Ministry of Natural Resources and Environment in amending the list of dangerous goods of class 1, class 4 and class 9 according to Clause 1 Article 4 of this Decree.
3. Take charge and cooperate with relevant ministries and central authorities in management, inspection and handling of violations against regulations on transport of dangerous goods within the Ministry's jurisdiction. Manage, inspect and handle violations against regulations on dangerous goods training within the Ministry's jurisdiction.
Article 23. Ministry of National Defense shall
1. Manage transport of dangerous goods and issue licences within the Ministry's jurisdiction according to Clause 2 Article 17 of this Decree.
2. Carry out immigration inspection and control, and cooperate in inspecting and supervising dangerous goods, vehicles carrying dangerous goods by road motor vehicles and by inland watercraft in border areas, land border checkpoints, and port border checkpoints according to regulations of law; arrange dedicated lanes for vehicles carrying dangerous goods to circulate at land border checkpoints where many vehicles carrying dangerous goods operate.
Article 24. Ministry of Science and Technology shall:
1. Manage transport of dangerous goods and the list of dangerous goods, and issue licences within the Ministry's jurisdiction according to Clause 3 Article 17 of this Decree.
2. Take charge and cooperate with the Ministry of Transport and the Ministry of Industry and Trade in amending the list of dangerous goods of class 5, class 7 and class 8 according to Clause 1 Article 4 of this Decree for submission thereof for competent authorities’ approval to be disclosed.
3. Stipulate the dangerous goods of class 5 and class 8 that require escorts when transported.
4. Take charge and cooperate with relevant ministries and central authorities in management, inspection and handling of violations against regulations on transport of dangerous goods within the Ministry's jurisdiction. Manage, inspect and handle violations against regulations on dangerous goods training within the Ministry's jurisdiction.
Article 25. Ministry of Health
1. Manage list of dangerous goods of classes of toxic chemicals used in the health section and insecticidal and antibacterial chemicals used in the household sector within the Ministry’s jurisdiction according to Clause 1 Article 4 of this Decree.
2. Take charge and cooperate with the Ministry of Transport in consulting the Government on amendments to list of dangerous goods relating to toxic chemicals, infectious substances used in the health sector and insecticidal and antibacterial chemicals used in the household sector.
3. Stipulate dangerous goods relating to toxic chemicals, infectious substances used in the health sector and insecticidal and antibacterial chemicals used in the household sector which require escorts upon transport.
4. Cooperate with relevant ministries and central authorities in management, inspection and handling of violations concerning transport of dangerous goods within the Ministry's jurisdiction. Manage, inspect and handle violations against regulations on dangerous goods training within the Ministry's jurisdiction.
Article 26. Ministry of Industry and Trade 
1. Manage list of dangerous goods of class 2, class 3, class 9, gasoline, oil, gas and other dangerous chemicals, remaining hazardous toxic chemicals according to Clause 1 Article 4 of this Decree.
2. Take charge and cooperate with the Ministry of Transport, the Ministry of Public Security and relevant ministry and central authorities in consulting the Government on amendments to the list of dangerous goods of class 2, class 3, class 9, gasoline, oil, gas and other dangerous chemicals, remaining hazardous toxic chemicals according to Clause 1 Article 4 of this Decree.
3. Cooperate with relevant ministries and central authorities in management, inspection and handling of violations concerning transport of dangerous goods within the Ministry's jurisdiction. Manage, inspect and handle violations against regulations on dangerous goods training within the Ministry's jurisdiction.
Article 27. Ministry of Agriculture and Rural Development shall:
1. Manage list of dangerous goods being crop protection chemicals.
2. Take charge and cooperate with the Ministry of Transport in consulting the Government on amendments to list of dangerous goods relating to crop protection chemicals.
3. Cooperate with relevant ministries and central authorities in management, inspection and handling of violations concerning transport of dangerous goods within the Ministry's jurisdiction.
Article 28. Ministry of Natural Resources and Environment shall:
Cooperate with relevant ministries and central authorities in management, inspection and handling of violations concerning transport of dangerous goods within the Ministry's jurisdiction.
Article 29. Ministry of Finance
Carry out immigration inspection and control; inspect and supervise dangerous goods, vehicles carrying dangerous goods in customs controlled areas according to regulations of law.
Article 30. The People’s Committees of provinces and central-affiliated cities
1. Manage transport of dangerous goods and issue licences to transport crop protection chemicals according to Clause 4 Article 17 of this Decree.
2. Cooperate with relevant ministries and central authorities in management, inspection and handling of violations concerning transport of dangerous goods within the Ministry's jurisdiction. Inspect and handle violations against regulations on training in transport of dangerous goods being crop protection chemicals. 
3. Direct the People’s Committees of second-level administrative divisions and third-level administrative divisions, in cases of occurrence of incidents during transport of dangerous goods in areas managed by the Committees, to:
a) assist drivers/operators and escorts (if any) in rescuing people, goods, and vehicles;
b) remove victims from incident areas and give first aid to victims; 
c) protect goods and vehicles for continued transport, storage, or transhipment according to instructions from competent authorities;
d) establish fenced-in areas and evacuate residents from dangerously affected areas, and report to the superior People's Committees and other relevant agencies to mobilize necessary forces to promptly handle the incidents.
Article 31. Consignors
A consignor shall:

1. Pack each class of dangerous goods in accordance with requirements for their sizes, weights and packaging materials stated in applicable technical standards.
2. Affix hazard placards, hazard signs and goods labels to outer packages and containers according to regulations of Article 7 herein.
3. Prepare 04 copies of a dossier on the dangerous goods to be transported, 03 of which shall be sent to the carrier, unloader and driver of vehicle/captain/operator of inland watercraft and 01 of which shall be retained by the consignor. The dossier shall consist of a consignment note that specifies name, code, class and division, total weight, type of packages, number of packages, manufacture date and location of the dangerous goods; and full names and addresses of the consignor and consignee.
4. Provide the carrier with transport requirements and emergency response guidelines, even when there are escorts, in writing.
5. Organize dangerous goods training or hire a unit in charge of dangerous goods training provision for escorts, loaders and warehouse-keepers according to regulations in Article 8 of this Decree. Assign escorts if required.
6. Fully equip escorts, warehouse-keepers, and loaders with protective gear according to regulations.
Article 32. Carriers shall:
A carrier shall:
1. Use a vehicle suitable to the class of dangerous goods to be transported.
2. Inspect goods and ensure safety before transport begins as per regulations.
3. Comply with all requirements from the consignor and regulations stated in the granted licence.
4. Affix hazard placard applicable to the class or division of dangerous goods being transported according to regulations.
5. Clean and remove all hazard placards from the vehicle carrying dangerous goods when unloading is completed and the vehicle no longer carry the same class of goods.
6. Adhere to regulations written in the granted licence and only transport the dangerous goods for which the licence, hazard placards and signs are required after the licence has been granted.
7. Only transport dangerous goods when all requirements concerning procedures, valid applications and packaging have been satisfied.
8. Follow instructions of supervisory authorities or construction units when transporting flammable substances, substances liable to spontaneous combustion or desensitized liquid or solid explosives through extremely important bridges or tunnels with a length of less than 100m or other works under construction with high temperature, welding sparks or electric sparks during the transport route.
9. Provide oil spill response plans when transporting oil and/or gasoline by inland waterways.
10. Organize dangerous goods training or hire a unit in charge of dangerous goods training provision for the vehicle’s driver/operator according to regulations in Article 8 of this Decree.
Article 33. Drivers/operators and escorts
A driver/operator or escort shall:

1. Adhere to regulations written in the granted licence and only transport the class or division or name of dangerous goods for which the licence is valid and required; all necessary hazard placards and signs have been affixed on the vehicle, packages and containers.
2. Follow instructions provided by the consignor and the carrier.
3. Follow instructions of supervisory authorities or construction units when transporting flammable substances, substances liable to spontaneous combustion or desensitized liquid or solid explosives through extremely important bridges or tunnels or other works under construction with high temperature, welding sparks or electric sparks during the transport route.
4. The driver/operator must bring the dangerous goods transport dossier provided by the consignor, valid licence for the class, division or name of dangerous goods which requires licensing, certificate of completion of dangerous goods training appropriate to the class or division of dangerous goods being transported, professional qualification (for captain or operator of inland watercraft) and other documents required by law; and preserve dangerous goods during transport if there is no escort.
5. Take measures to eliminate or mitigate dangers posed by dangerous goods; record and report to the local People's Committee of the nearest third-level administrative division and relevant agencies for timely handling of dangerous goods incidents, which may affect human lives, vehicles, the environment and other goods, or traffic accidents when transporting dangerous goods during transport. Notify the carrier and the consignor for cooperation in handling of incidents that are beyond the capacity of the driver/operator or escort.
6. The captain or operator of inland watercraft shall assign crew members to regularly instruct and supervise loading/unloading of dangerous goods into/from their watercraft.
7. Follow instructions of supervisory authorities or construction units when transporting flammable substances, substances liable to spontaneous combustion or desensitized liquid or solid explosives through extremely important bridges or tunnels with a length of less than 100m or other works under construction with high temperature, welding sparks or electric sparks during the transport route.
8. The escort must bring a certificate of completion of dangerous goods training appropriate to the class or division of dangerous goods being transported.
Chapter VI
IMPLEMENTATION PROVISIONS
Article 34. Entry into force
1. This Decree takes effect from May 15, 2024 and replaces Decree No. 42/2020/ND-CP.
2. Organizations and individuals granted licences prior to the effective date of this Decree may continue using such licences until they expire or are renewed.
Article 35. Implementation responsibilities
Ministers, Heads of ministerial-level agencies, Heads of Governmental agencies, Presidents of the People’s Committees of provinces and central-affiliated cities and relevant entities shall implement this Decree./.
	
	ON BEHALF OF GOVERNMENT OF VIETNAM
PP. PRIME MINISTER
DEPUTY PRIME MINISTER




Tran Hong Ha


APPENDIX I
LIST OF DANGEROUS GOODS 
(Enclosed with Decree No. 34/2024/ND-CP dated March 31, 2024 of the Government of Vietnam)
	No.
	Name and description
	UN Number
	Class or division
	Hazard placard or sign 
	Hazard identification number

	(1)
	(2)
	(3)
	(4)
	(5)
	(6)

	1
	AMMONIUM PICRATE dry or wetted with less than 10% water, by mass
	0004
	1
	1
	

	2
	CARTRIDGES FOR WEAPONS with bursting charge
	0005
	1
	1
	

	3
	CARTRIDGES FOR WEAPONS with bursting charge
	0006
	1
	1
	

	4
	CARTRIDGES FOR WEAPONS with bursting charge
	0007
	1
	1
	

	5
	AMMUNITION, INCENDIARY with or without burster, expelling charge or propelling charge
	0009
	1
	1
	

	6
	AMMUNITION, INCENDIARY with or without burster, expelling charge or propelling charge
	0010
	1
	1
	

	7
	CARTRIDGES FOR WEAPONS, INERT PROJECTILE or CARTRIDGES, SMALL ARMS
	0012
	1
	1.4
	

	8
	CARTRIDGES FOR WEAPONS, BLANK or CARTRIDGES, SMALL ARMS, BLANK or CARTRIDGE FOR TOOLS, BLANK
	0014
	1
	1.4
	

	9
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge
	0015
	1
	1
	

	10
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge, containing corrosive substances
	0015
	1
	1

+8
	

	11
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge, containing toxic by inhalation substances
	0015
	1
	1

+6.1
	

	12
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge
	0016
	1
	1
	

	13
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge, containing corrosive substances
	0016
	1
	1

+8
	

	14
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge, containing toxic by inhalation substances
	0016
	1
	1

+6.1
	

	15
	AMMUNITION, TEAR​PRODUCING with burster, expelling charge or propelling charge
	0018
	1
	1

+6.1

+8
	

	16
	AMMUNITION, TEAR​PRODUCING with burster, expelling charge or propelling charge
	0019
	1
	1+6.1+8
	

	17
	AMMUNITION, TOXIC with burster, expelling charge or propelling charge
	0020
	1
	
	

	18
	AMMUNITION, TOXIC with burster, expelling charge or propelling charge
	0021
	1
	
	

	19
	BLACK POWDER (GUNPOWDER), granular or as a meal
	0027
	1
	1
	

	20
	BLACK POWDER (GUNPOWDER), COMPRESSED or BLACK POWDER (GUNPOWDER), IN PELLETS
	0028
	1
	1
	

	21
	DETONATORS, NON-ELECTRIC for blasting
	0029
	1
	1
	

	22
	DETONATORS, ELECTRIC for blasting
	0030
	1
	1
	

	23
	BOMBS with bursting charge
	0033
	1
	1
	

	24
	BOMBS with bursting charge
	0034
	1
	1
	

	25
	BOMBS with bursting charge
	0035
	1
	1
	

	26
	BOMBS, PHOTO-FLASH
	0037
	1
	1
	

	27
	BOMBS, PHOTO-FLASH
	0038
	1
	1
	

	28
	BOMBS, PHOTO-FLASH
	0039
	1
	1
	

	29
	BOOSTERS without detonator
	0042
	1
	1
	

	32
	CHARGES, DEMOLITION
	0048
	1
	1
	

	33
	CARTRIDGES, FLASH
	0049
	1
	1
	

	34
	CARTRIDGES, FLASH
	0050
	1
	1
	

	35
	CARTRIDGES, SIGNAL
	0054
	1
	1
	

	36
	CASES, CARTRIDGE, EMPTY, WITH PRIMER
	0055
	1
	1.4
	

	37
	CHARGES, DEPTH
	0056
	1
	1
	

	38
	CHARGES, SHAPED without detonator
	0059
	1
	1
	

	39
	CHARGES, SUPPLEMENTARY, EXPLOSIVE
	0060
	1
	1
	

	41
	CORD, IGNITER
	0066
	1
	1.4
	

	42
	CUTTERS, CABLE, EXPLOSIVE
	0070
	1
	1.4
	

	43
	CYCLOTRIMETHYLENE​TRINITRAMINE (CYCLONITE; HEXOGEN; RDX), WETTED with not less than 15% water, by mass
	0072
	1
	1
	

	44
	DETONATORS FOR AMMUNITION
	0073
	1
	1
	

	45
	DIAZODINITROPHENOL, WETTED with not less than 40% water, or mixture of alcohol and water, by mass
	0074
	1
	1
	

	46
	DIETHYLENEGLYCOL DINITRATE, DESENSITIZED with not less than 25% non-volatile, water- insoluble phlegmatizer, by mass
	0075
	1
	1
	

	47
	DINITROPHENOL, dry or wetted with less than 15% water, by mass
	0076
	1
	1

+6.1
	

	48
	DINITROPHENOLATES, alkali metals, dry or wetted with less than 15% water, by mass
	0077
	1
	1

+6.1
	

	49
	DINITRORESORCINOL, dry or wetted with less than 15% water, by mass
	0078
	1
	1
	

	50
	HEXANITRODIPHENYL- AMINE (DIPICRYLAMINE; HEXYL)
	0079
	1
	1
	

	51
	EXPLOSIVE, BLASTING, TYPE A
	0081
	1
	1
	

	52
	EXPLOSIVE, BLASTING, TYPE B
	0082
	1
	1
	

	53
	EXPLOSIVE, BLASTING, TYPE C
	0083
	1
	1
	

	54
	EXPLOSIVE, BLASTING, TYPE D
	0084
	1
	1
	

	55
	FLARES, SURFACE
	0092
	1
	1
	

	56
	FLARES, AERIAL
	0093
	1
	1
	

	57
	FLASH POWDER
	0094
	1
	1
	

	58
	FRACTURING DEVICES, EXPLOSIVE without detonator, for oil wells
	0099
	1
	1
	

	59
	FUSE, NON-DETONATING
	0101
	1
	1
	

	61
	FUSE IGNITER, tubular, metal clad
	0103
	1
	1.4
	

	62
	CORD (FUSE), DETONATING, MILD EFFECT, metal clad
	0104
	1
	1.4
	

	63
	FUSE, SAFETY
	0105
	1
	1.4
	

	64
	FUZES, DETONATING
	0106
	1
	1
	

	65
	FUZES, DETONATING
	0107
	1
	1
	

	66
	GRENADES, PRACTICE, hand or rifle
	0110
	1
	1.4
	

	67
	GUANYLNITROSAMINO- GUANYLIDENE HYDRAZINE, WETTED with not less than 30% water, by mass
	0113
	1
	1
	

	68
	GUANYLNITROSAMINO​ GUANYLTETRAZENE (TETRAZENE), WETTED with not less than 30% water, or mixture of alcohol and water, by mass
	0114
	1
	1
	

	69
	HEXOLITE (HEXOTOL), dry or wetted with less than 15% water, by mass
	0118
	1
	1
	

	70
	IGNITERS
	0121
	1
	1
	

	71
	JET PERFORATING GUNS, CHARGED, oil well, without detonator
	0124
	1
	1
	

	72
	LEAD AZIDE, WETTED with not less than 20% water, or mixture of alcohol and water, by mass
	0129
	1
	1
	

	73
	LEAD STYPHNATE (LEAD TRINITRORESORCINATE), WETTED with not less than 20% water, or mixture of alcohol and water, by mass
	0130
	1
	1
	

	74
	LIGHTERS, FUSE
	0131
	1
	1.4
	

	75
	DEFLAGRATING METAL SALTS OF AROMATIC NITRODERIVATIVES, N.O.S.
	0132
	1
	1
	

	76
	MANNITOL HEXANITRATE (NITROMANNITE), WETTED with not less than 40% water, or mixture of alcohol and water, by mass
	0133
	1
	1
	

	77
	MERCURY FULMINATE, WETTED with not less than 20% water, or mixture of alcohol and water, by mass
	0135
	1
	1
	

	78
	MINES with bursting charge
	0136
	1
	1
	

	79
	MINES with bursting charge
	0137
	1
	1
	

	80
	MINES with bursting charge
	0138
	1
	1
	

	81
	NITROGLYCERIN, DESENSITIZED with not less than 40% non-volatile water-insoluble phlegmatizer, by mass
	0143
	1
	1

+6.1
	

	82
	NITROGLYCERIN SOLUTION IN ALCOHOL with more than 1% but not more than 10% nitroglycerin
	0144
	1
	1
	

	83
	NITROSTARCH, dry or wetted with less than 20% water, by mass
	0146
	1
	1
	

	84
	NITRO UREA
	0147
	1
	1
	

	85
	PENTAERYTHRITE TETRANITRATE (PENTAERYTHRITOL

TETRANITRATE; PETN), WETTED with not less than 25% water, by mass, or DESENSITIZED with not less than 15% phlegmatizer, by mass
	0150
	1
	1
	

	86
	PENTOLITE, dry or wetted with less than 15% water, by mass
	0151
	1
	1
	

	87
	TRINITROANILINE (PICRAMIDE)
	0153
	1
	1
	

	88
	TRINITROPHENOL (PICRIC ACID), dry or wetted with less than 30% water, by mass
	0154
	1
	1
	

	89
	TRINITROCHLORO-BENZENE (PICRYL CHLORIDE)
	0155
	1
	1
	

	90
	POWDER CAKE (POWDER PASTE), WETTED with not less than 25% water, by mass
	0159
	1
	1
	

	91
	POWDER, SMOKELESS
	0160
	1
	1
	

	92
	POWDER, SMOKELESS
	0161
	1
	1
	

	93
	PROJECTILES with bursting charge
	0167
	1
	1
	

	94
	PROJECTILES with bursting charge
	0168
	1
	1
	

	95
	PROJECTILES with bursting charge
	0169
	1
	1
	

	96
	AMMUNITION, ILLUMINATING with or without burster, expelling charge or propelling charge
	0171
	1
	1
	

	97
	RELEASE DEVICES, EXPLOSIVE
	0173
	1
	1.4
	

	98
	RIVETS, EXPLOSIVE
	0174
	1
	1.4
	

	99
	ROCKETS with bursting charge
	0180
	1
	1
	

	100
	ROCKETS with bursting charge
	0181
	1
	1
	

	101
	ROCKETS with bursting charge
	0182
	1
	1
	

	102
	ROCKETS with inert head
	0183
	1
	1
	

	103
	ROCKET MOTORS
	0186
	1
	1
	

	104
	SAMPLES, EXPLOSIVE, other than initiating explosive
	0190
	1
	
	

	105
	SIGNAL DEVICES, HAND
	0191
	1
	1.4
	

	106
	SIGNALS, RAILWAY TRACK, EXPLOSIVE
	0192
	1
	1
	

	107
	SIGNALS, RAILWAY TRACK, EXPLOSIVE
	0193
	1
	1.4
	

	108
	SIGNALS, DISTRESS, ship
	0194
	1
	1
	

	109
	SIGNALS, DISTRESS, ship
	0195
	1
	1
	

	110
	SIGNALS, SMOKE
	0196
	1
	1
	

	111
	SIGNALS, SMOKE
	0197
	1
	1.4
	

	112
	SOUNDING DEVICES, EXPLOSIVE
	0204
	1
	1
	

	113
	TETRANITROANILINE
	0207
	1
	1
	

	114
	TRINITROPHENYLMETHYL​

NITRAMINE (TETRYL)
	0208
	1
	1
	

	115
	TRINITROTOLUENE (TNT), dry or wetted with less than 30% water, by mass
	0209
	1
	1
	

	116
	TRACERS FOR AMMUNITION
	0212
	1
	1
	

	117
	TRINITROANISOLE
	0213
	1
	1
	

	118
	TRINITROBENZENE, dry or wetted with less than 30% water, by mass
	0214
	1
	1
	

	119
	TRINITROBENZOIC ACID, dry or wetted with less than 30% water, by mass
	0215
	1
	1
	

	120
	TRINITRO-m-CRESOL
	0216
	1
	1
	

	121
	TRINITRONAPHTHALENE
	0217
	1
	1
	

	122
	TRINITROPHENETOLE
	0218
	1
	1
	

	123
	TRINITRORESORCINOL (STYPHNIC ACID), dry or wetted with less than 20% water, or mixture of alcohol and water, by mass
	0219
	1
	1
	

	124
	UREA NITRATE, dry or wetted with less than 20% water, by mass
	0220
	1
	1
	

	125
	WARHEADS, TORPEDO with bursting charge
	0221
	1
	1
	

	127
	BARIUM AZIDE, dry or wetted with less than 50% water, by mass
	0224
	1
	1 +6.1
	

	128
	BOOSTERS WITH DETONATOR
	0225
	1
	1
	

	129
	CYCLOTETRAMETHYLENE​TETRANITRAMINE (HMX; OCTOGEN), WETTED with not less than 15% water, by mass
	0226
	1
	1
	

	130
	SODIUM DINITRO-o- CRESOLATE, dry or wetted with less than 15% water, by mass
	0234
	1
	1
	

	131
	SODIUM PICRAMATE, dry or wetted with less than 20% water, by mass
	0235
	1
	1
	

	132
	ZIRCONIUM PICRAMATE, dry or wetted with less than 20% water, by mass
	0236
	1
	1
	

	133
	CHARGES, SHAPED, FLEXIBLE, LINEAR
	0237
	1
	1.4
	

	134
	ROCKETS, LINE-THROWING
	0238
	1
	1
	

	135
	ROCKETS, LINE-THROWING
	0240
	1
	1
	

	137
	CHARGES, PROPELLING, FOR CANNON
	0242
	1
	1
	

	138
	AMMUNITION, INCENDIARY, WHITE PHOSPHORUS with burster, expelling charge or propelling charge
	0243
	1
	1
	

	139
	AMMUNITION, INCENDIARY, WHITE PHOSPHORUS with burster, expelling charge or propelling charge
	0244
	1
	1
	

	140
	AMMUNITION, SMOKE, WHITE PHOSPHORUS with burster, expelling charge or propelling charge
	0245
	1
	1
	

	141
	AMMUNITION, SMOKE, WHITE PHOSPHORUS with burster, expelling charge or propelling charge
	0246
	1
	1
	

	142
	AMMUNITION, INCENDIARY, liquid or gel, with burster, expelling charge or propelling charge
	0247
	1
	1
	

	143
	CONTRIVANCES, WATER- ACTIVATED with burster, expelling charge or propelling charge
	0248
	1
	1
	

	144
	CONTRIVANCES, WATER- ACTIVATED with burster, expelling charge or propelling charge
	0249
	1
	1
	

	145
	ROCKET MOTORS WITH HYPERGOLIC LIQUIDS with or without expelling charge
	0250
	1
	1
	

	146
	AMMUNITION, ILLUMINATING with or without burster, expelling charge or propelling charge
	0254
	1
	1
	

	149
	OCTOLITE (OCTOL), dry or wetted with less than 15% water, by mass
	0266
	1
	1
	

	150
	DETONATORS, NON-ELECTRIC for blasting
	0267
	1
	1.4
	

	151
	BOOSTERS WITH DETONATOR
	0268
	1
	1
	

	152
	CHARGES, PROPELLING
	0271
	1
	1
	

	153
	CHARGES, PROPELLING
	0272
	1
	1
	

	154
	CARTRIDGES, POWER DEVICE
	0275
	1
	1
	

	155
	CARTRIDGES POWER DEVICE
	0276
	1
	1.4
	

	156
	CARTRIDGES OIL WELL
	0277
	1
	1
	

	157
	CARTRIDGES OIL WELL
	0278
	1
	1.4
	

	158
	CHARGES, PROPELLING, FOR CANNON
	0279
	1
	1
	

	159
	ROCKET MOTORS
	0280
	1
	1
	

	160
	ROCKET MOTORS
	0281
	1
	1
	

	161
	NITROGUANIDINE (PICRITE), dry or wetted with less than 20% water, by mass
	0282
	1
	1
	

	162
	BOOSTERS without detonator
	0283
	1
	1
	

	163
	GRENADES, hand or rifle, with bursting charge
	0284
	1
	1
	

	164
	GRENADES, hand or rifle, with bursting charge
	0285
	1
	1
	

	165
	WARHEADS, ROCKET with bursting charge
	0286
	1
	1
	

	166
	WARHEADS, ROCKET with bursting charge
	0287
	1
	1
	

	167
	CHARGES, SHAPED, FLEXIBLE, LINEAR
	0288
	1
	1
	

	168
	CORD, DETONATING, flexible
	0289
	1
	1.4
	

	169
	CORD (FUSE), DETONATING, metal clad
	0290
	1
	1
	

	170
	BOMBS with bursting charge
	0291
	1
	1
	

	171
	GRENADES, hand or rifle, with bursting charge
	0292
	1
	1
	

	172
	GRENADES, hand or rifle, with bursting charge
	0293
	1
	1
	

	173
	MINES with bursting charge
	0294
	1
	1
	

	174
	ROCKETS with bursting charge
	0295
	1
	1
	

	175
	SOUNDING DEVICES, EXPLOSIVE
	0296
	1
	1
	

	176
	AMMUNITION, ILLUMINATING with or without burster, expelling charge or propelling charge
	0297
	1
	1.4
	

	177
	BOMBS, PHOTO-FLASH
	0299
	1
	1
	

	178
	AMMUNITION, INCENDIARY with or without burster, expelling charge or propelling charge
	0300
	1
	1.4
	

	179
	AMMUNITION, TEAR​PRODUCING with burster, expelling charge or propelling charge
	0301
	1
	1.4 

+6.1

+8
	

	180
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge
	0303
	1
	1.4
	

	181
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge, containing corrosive substances
	0303
	1
	1.4 

+8
	

	182
	AMMUNITION, SMOKE with or without burster, expelling charge or propelling charge, containing toxic by inhalation substances
	0303
	1
	1.4

+6.1
	

	183
	FLASH POWDER
	0305
	1
	1
	

	184
	TRACERS FOR AMMUNITION
	0306
	1
	1.4
	

	186
	SIGNALS, SMOKE
	0313
	1
	1
	

	187
	IGNITERS
	0314
	1
	1
	

	188
	IGNITERS
	0315
	1
	1
	

	189
	FUZES, IGNITING
	0316
	1
	1
	

	190
	FUZES, IGNITING
	0317
	1
	1.4
	

	191
	GRENADES, PRACTICE, hand or rifle
	0318
	1
	1
	

	194
	CARTRIDGES FOR WEAPONS with bursting charge
	0321
	1
	1
	

	195
	ROCKET MOTORS WITH HYPERGOLIC LIQUIDS with or without expelling charge
	0322
	1
	1
	

	196
	CARTRIDGES, POWER DEVICE
	0323
	1
	1.4
	

	197
	PROJECTILES with bursting charge
	0324
	1
	1
	

	198
	IGNITERS
	0325
	1
	1.4
	

	199
	CARTRIDGES FOR WEAPONS, BLANK
	0326
	1
	1
	

	200
	CARTRIDGES FOR WEAPONS, BLANK or CARTRIDGES, SMALL ARMS, BLANK
	0327
	1
	1
	

	201
	CARTRIDGES FOR WEAPONS, INERT PROJECTILE
	0328
	1
	1
	

	202
	TORPEDOES with bursting charge
	0329
	1
	1
	

	203
	TORPEDOES with bursting charge
	0330
	1
	1
	

	211
	CARTRIDGES FOR WEAPONS, BLANK or CARTRIDGES, SMALL ARMS, BLANK
	0338
	1
	1.4
	

	212
	CARTRIDGES FOR WEAPONS, INERT PROJECTILE or CARTRIDGES, SMALL ARMS
	0339
	1
	1.4
	

	213
	NITROCELLULOSE, dry or wetted with less than 25% water (or alcohol), by mass
	0340
	1
	1
	

	214
	NITROCELLULOSE, unmodified or plasticized with less than 18% plasticizing substance, by mass
	0341
	1
	1
	

	215
	NITROCELLULOSE, WETTED with not less than 25% alcohol, by mass
	0342
	1
	1
	

	216
	NITROCELLULOSE, PLASTICIZED with not less than 18% plasticizing substance, by mass
	0343
	1
	1
	

	217
	PROJECTILES with bursting charge
	0344
	1
	1.4
	

	218
	PROJECTILES, inert with tracer
	0345
	1
	1.4
	

	219
	PROJECTILES with burster or expelling charge
	0346
	1
	1
	

	220
	PROJECTILES with burster or expelling charge
	0347
	1
	1.4
	

	221
	CARTRIDGES FOR WEAPONS with bursting charge
	0348
	1
	1.4
	

	222
	ARTICLES, EXPLOSIVE, N.o.s.
	0349
	1
	1.4
	

	223
	ARTICLES, EXPLOSIVE, N.O.S.
	0350
	1
	1.4
	

	224
	ARTICLES, EXPLOSIVE, N.O.S.
	0351
	1
	1.4
	

	225
	ARTICLES, EXPLOSIVE, N.O.S.
	0352
	1
	1.4
	

	226
	ARTICLES, EXPLOSIVE, N.O.S.
	0353
	1
	1.4
	

	227
	ARTICLES, EXPLOSIVE, N.O.S.
	0354
	1
	1
	

	228
	ARTICLES, EXPLOSIVE, N.O.S.
	0355
	1
	1
	

	229
	ARTICLES, EXPLOSIVE, N.O.S.
	0356
	1
	1
	

	230
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0357
	1
	1
	

	231
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0358
	1
	1
	

	232
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0359
	1
	1
	

	233
	DETONATOR ASSEMBLIES, NON-ELECTRIG for blasting
	0360
	1
	1
	

	234
	DETONATOR ASSEMBLIES, NON-ELECTRIC for blasting
	0361
	1
	1.4
	

	235
	AMMUNITION, PRACTICE
	0362
	1
	1.4
	

	236
	AMMUNITION, PROOF
	0363
	1
	1.4
	

	237
	DETONATORS FOR AMMUNITION
	0364
	1
	1
	

	238
	DETONATORS FOR AMMUNITION
	0365
	1
	1.4
	

	239
	DETONATORS FOR AMMUNITION
	0366
	1
	1.4
	

	240
	FUZES, DETONATING
	0367
	1
	1.4
	

	241
	FUZES, IGNITING
	0368
	1
	1.4
	

	242
	WARHEADS, ROCKET with bursting charge
	0369
	1
	1
	

	243
	WARHEADS, ROCKET with burster or expelling charge
	0370
	1
	1.4
	

	244
	WARHEADS, ROCKET with burster or expelling charge
	0371
	1
	1.4
	

	245
	GRENADES, PRACTICE, hand or rifle
	0372
	1
	1
	

	246
	SIGNAL DEVICES, HAND
	0373
	1
	1.4
	

	247
	SOUNDING DEVICES, EXPLOSIVE
	0374
	1
	1
	

	248
	SOUNDING DEVICES, EXPLOSIVE
	0375
	1
	1
	

	252
	CASES, CARTRIDGE, EMPTY, WITH PRIMER
	0379
	1
	1.4
	

	253
	ARTICLES, PYROPHORIC
	0380
	1
	1
	

	254
	CARTRIDGES, POWER DEVICE
	0381
	1
	1
	

	255
	COMPONENTS, EXPLOSIVE TRAIN, N.O.S.
	0382
	1
	1
	

	256
	COMPONENTS, EXPLOSIVE TRAIN, N.O.S.
	0383
	1
	1.4
	

	257
	COMPONENTS, EXPLOSIVE TRAIN, N.O.S.
	0384
	1
	1.4
	

	258
	5-NITROBENZOTRIAZOL
	0385
	1
	1
	

	259
	TRINITROBENZENE- SULPHONIC ACID
	0386
	1
	1
	

	260
	TRINITROFLUORENONE
	0387
	1
	1
	

	261
	TRINITROTOLUENE (TNT) AND TRINITROBENZENE MIXTURE or TRINITROTOLUENE (TNT) AND HEXANITROSTILBENE MIXTURE
	0388
	1
	1
	

	262
	TRINITROTOLUENE (TNT) MIXTURE CONTAINING TRINITROBENZENE AND HEXANITROSTILBENE
	0389
	1
	1
	

	263
	TRITONAL
	0390
	1
	1
	

	264
	CYCLOTRIMETHYLENE​TRINITRAMINE (CYCLONITE; HEXOGEN; RDX) AND CYCLOTETRAMETHYLENE​TETRANITRAMINE (HMX; OCTOGEN) MIXTURE, WETTED with not less than 15% water, by mass or DESENSITIZED with not less than 10% phlegmatiser by mass
	0391
	1
	1
	

	265
	HEXANITROSTILBENE
	0392
	1
	1
	

	266
	HEXOTONAL
	0393
	1
	1
	

	267
	TRINITRORESORCINOL (STYPHNIC ACID), WETTED with not less than 20% water, or mixture of alcohol and water, by mass
	0394
	1
	1
	

	268
	ROCKET MOTORS, LIQUID FUELLED
	0395
	1
	1
	

	269
	ROCKET MOTORS, LIQUID FUELLED
	0396
	1
	1
	

	270
	ROCKETS, LIQUID FUELLED with bursting charge
	0397
	1
	1
	

	271
	ROCKETS, LIQUID FUELLED with bursting charge
	0398
	1
	1
	

	272
	BOMBS WITH FLAMMABLE LIQUID with bursting charge
	0399
	1
	1
	

	273
	BOMBS WITH FLAMMABLE LIQUID with bursting charge
	0400
	1
	1
	

	274
	DIPICRYL SULPHIDE, dry or wetted with less than 10% water, by mass
	0401
	1
	1
	

	276
	FLARES, AERIAL
	0403
	1
	1.4
	

	277
	FLARES, AERIAL
	0404
	1
	1.4
	

	278
	CARTRIDGES, SIGNAL
	0405
	1
	1.4
	

	279
	DINITROSOBENZENE
	0406
	1
	1
	

	280
	TETRAZOL-1 -ACETIC ACID
	0407
	1
	1.4
	

	281
	FUZES, DETONATING with protective features
	0408
	1
	1
	

	282
	FUZES, DETONATING with protective features
	0409
	1
	1
	

	283
	FUZES, DETONATING with protective features
	0410
	1
	1.4
	

	284
	PENTAERYTHRITE TETRANITRATE (PENTAERYTHRITOL TETRANITRATE; PETN) with not less than 7% wax, by mass
	0411
	1
	1
	

	285
	CARTRIDGES FOR WEAPONS with bursting charge
	0412
	1
	1.4
	

	286
	CARTRIDGES FOR WEAPONS, BLANK
	0413
	1
	1
	

	287
	CHARGES, PROPELLING, FOR CANNON
	0414
	1
	1
	

	288
	CHARGES, PROPELLING
	0415
	1
	1
	

	289
	CARTRIDGES FOR WEAPONS, INERT PROJECTILE or CARTRIDGES, SMALL ARMS
	0417
	1
	1
	

	290
	FLARES, SURFACE
	0418
	1
	1
	

	291
	FLARES, SURFACE
	0419
	1
	1
	

	292
	FLARES, AERIAL
	0420
	1
	1
	

	293
	FLARES, AERIAL
	0421
	1
	1
	

	294
	PROJECTILES, inert with tracer
	0424
	1
	1
	

	295
	PROJECTILES, inert with tracer
	0425
	1
	1.4
	

	296
	PROJECTILES with burster or expelling charge
	0426
	1
	1
	

	297
	PROJECTILES with burster or expelling charge
	0427
	1
	1.4
	

	298
	ARTICLES, PYROTECHNIC for technical purposes
	0428
	1
	1
	

	299
	ARTICLES, PYROTECHNIC for technical purposes
	0429
	1
	1
	

	300
	ARTICLES, PYROTECHNIC for technical purposes
	0430
	1
	1
	

	301
	ARTICLES, PYROTECHNIC for technical purposes
	0431
	1
	1.4
	

	302
	ARTICLES, PYROTECHNIC for technical purposes
	0432
	1
	1.4
	

	303
	POWDER CAKE (POWDER PASTE), WETTED with not less than 17% alcohol, by mass
	0433
	1
	1
	

	304
	PROJECTILES with burster or expelling charge
	0434
	1
	1
	

	305
	PROJECTILES with burster or expelling charge
	0435
	1
	1.4
	

	306
	ROCKETS with expelling charge
	0436
	1
	1
	

	307
	ROCKETS with expelling charge
	0437
	1
	1
	

	308
	ROCKETS with expelling charge
	0438
	1
	1.4
	

	309
	CHARGES, SHAPED, without detonator
	0439
	1
	1
	

	310
	CHARGES, SHAPED, without detonator
	0440
	1
	1.4
	

	311
	CHARGES, SHAPED, without detonator
	0441
	1
	1.4
	

	312
	CHARGES EXPLOSIVE, COMMERCIAL without detonator
	0442
	1
	1
	

	313
	CHARGES EXPLOSIVE, COMMERCIAL without detonator
	0443
	1
	1
	

	314
	CHARGES, EXPLOSIVE, COMMERCIAL without detonator
	0444
	1
	1.4
	

	315
	CHARGES EXPLOSIVE, COMMERCIAL without detonator
	0445
	1
	1.4
	

	316
	CASES, COMBUSTIBLE, EMPTY, WITHOUT PRIMER
	0446
	1
	1.4
	

	317
	CASES, COMBUSTIBLE, EMPTY, WITHOUT PRIMER
	0447
	1
	1
	

	318
	5-MERCAPTOTETRAZOL-1-ACETIC ACID
	0448
	1
	1.4
	

	319
	TORPEDOES, LIQUID FUELLED with or without bursting charge
	0449
	1
	1
	

	320
	TORPEDOES, LIQUID FUELLED with inert head
	0450
	1
	1
	

	321
	TORPEDOES with bursting charge
	0451
	1
	1
	

	322
	GRENADES, PRACTICE, hand or rifle
	0452
	1
	1.4
	

	323
	ROCKETS, LINE-THROWING
	0453
	1
	1.4
	

	324
	IGNITERS
	0454
	1
	1.4
	

	325
	DETONATORS, NON-ELECTRIC for blasting
	0455
	1
	1.4
	

	326
	DETONATORS, ELECTRIC for blasting
	0456
	1
	1.4
	

	327
	CHARGES, BURSTING, PLASTICS BONDED
	0457
	1
	1
	

	328
	CHARGES, BURSTING, PLASTICS BONDED
	0458
	1
	1
	

	329
	CHARGES, BURSTING, PLASTICS BONDED
	0459
	1
	1.4
	

	330
	CHARGES, BURSTING, PLASTICS BONDED
	0460
	1
	1.4
	

	331
	COMPONENTS, EXPLOSIVE TRAIN, N.O.S.
	0461
	1
	1
	

	332
	ARTICLES, EXPLOSIVE, N.O.S.
	0462
	1
	1
	

	333
	ARTICLES, EXPLOSIVE, N.O.S.
	0463
	1
	1
	

	334
	ARTICLES, EXPLOSIVE, N.O.S.
	0464
	1
	1
	

	335
	ARTICLES, EXPLOSIVE, N.O.S.
	0465
	1
	1
	

	336
	ARTICLES, EXPLOSIVE, N.O.S.
	0466
	1
	1
	

	337
	ARTICLES, EXPLOSIVE, N.O.S.
	0467
	1
	1
	

	338
	ARTICLES, EXPLOSIVE, N.O.S.
	0468
	1
	1
	

	339
	ARTICLES, EXPLOSIVE, N.O.S.
	0469
	1
	1
	

	340
	ARTICLES, EXPLOSIVE, N.O.S.
	0470
	1
	1
	

	341
	ARTICLES, EXPLOSIVE, N.O.S.
	0471
	1
	1.4
	

	342
	ARTICLES, EXPLOSIVE, N.O.S.
	0472
	1
	1.4
	

	343
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0473
	1
	1
	

	344
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0474
	1
	1
	

	345
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0475
	1
	1
	

	346
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0476
	1
	1
	

	347
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0477
	1
	1
	

	348
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0478
	1
	1
	

	349
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0479
	1
	1.4
	

	350
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0480
	1
	1.4
	

	351
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0481
	1
	1.4
	

	352
	SUBSTANCES, EXPLOSIVE, VERY INSENSITIVE (SUBSTANCES, EVI), N.O.S.
	0482
	1
	1.5
	

	353
	CYCLOTRIMETHYLENE​ TRINITRAMINE (CYCLONITE; HEXOGEN; RDX), DESENSITIZED
	0483
	1
	1
	

	354
	CYCLOTETRAMETHYLENE- TETRA-NITRAMINE (HMX; OCTOGEN), DESENSITIZED
	0484
	1
	1
	

	355
	SUBSTANCES, EXPLOSIVE, N.O.S.
	0485
	1
	1.4
	

	356
	ARTICLES, EXPLOSIVE, EXTREMELY INSENSITIVE (ARTICLES, EEI)
	0486
	1
	1.6
	

	357
	SIGNALS, SMOKE
	0487
	1
	1
	

	358
	AMMUNITION, PRACTICE
	0488
	1
	1
	

	359
	DINITROGLYCOLURIL (DINGU)
	0489
	1
	1
	

	360
	NITROTRIAZOLONE (NTO)
	0490
	1
	1
	

	361
	CHARGES, PROPELLING
	0491
	1
	1.4
	

	362
	SIGNALS, RAILWAY TRACK, EXPLOSIVE
	0492
	1
	1
	

	363
	SIGNALS, RAILWAY TRACK, EXPLOSIVE
	0493
	1
	1.4
	

	364
	JET PERFORATING GUNS, CHARGED, oil well, without detonator
	0494
	1
	1.4
	

	365
	PROPELLANT, LIQUID
	0495
	1
	1
	

	366
	OCTONAL
	0496
	1
	1
	

	367
	PROPELLANT, LIQUID
	0497
	1
	1
	

	368
	PROPELLANT, SOLID
	0498
	1
	1
	

	369
	PROPELLANT, SOLID
	0499
	1
	1
	

	370
	DETONATOR ASSEMBLIES, NON-ELECTRIC for blasting
	0500
	1
	1.4
	

	371
	PROPELLANT, SOLID
	0501
	1
	1.4
	

	372
	ROCKETS with inert head
	0502
	1
	1
	

	373
	SAFETY DEVICES, PYROTECHNIC
	0503
	1
	1.4
	

	374
	1H-TETRAZOLE
	0504
	1
	1
	

	375
	SIGNALS, DISTRESS, ship
	0505
	1
	1.4
	

	376
	SIGNALS, DISTRESS, ship
	0506
	1
	1.4
	

	377
	SIGNALS, SMOKE
	0507
	1
	1.4
	

	378
	1 -HYDROXY-BENZOTRI AZOLE, ANHYDROUS, dry or wetted with less than 20% water, by mass
	0508
	1
	1
	

	379
	POWDER, SMOKELESS
	0509
	1
	1.4
	

	380
	ROCKET MOTORS
	0510
	1
	1.4
	

	381
	ACETYLENE, DISSOLVED
	1001
	2
	2.1
	239

	382
	AIR, COMPRESSED
	1002
	2
	2.2
	20

	383
	AIR, REFRIGERATED LIQUID
	1003
	2
	2.2

+5.1
	225

	384
	AMMONIA, ANHYDROUS
	1005
	2
	2.3

+8
	268

	385
	ARGON, COMPRESSED
	1006
	2
	2.2
	20

	386
	BORON TRIFLUORIDE
	1008
	2
	2.3

+8
	268

	387
	BROMOTRIFLUORO-METHANE (REFRIGERANT GAS R 13B1)
	1009
	2
	2.2
	20

	388
	BUTADIENES, STABILIZED or BUTADIENES AND HYDROCARBON MIXTURE, STABILIZED, having a vapour pressure at 70 °C not exceeding 1.1 Mpa (11 bar) and a density at 50 °C not lower than 0.525 kg/l
	1010
	2
	2.1
	239

	389
	BUTANE
	1011
	2
	2.1
	23

	390
	BUTYLENES MIXTURE or 1- BUTYLENE or cis-2-BUTYLENE or trans-2-BUTYLENE
	1012
	2
	2.1
	23

	391
	CARBON DIOXIDE
	1013
	2
	2.2
	20

	392
	CARBON MONOXIDE, COMPRESSED
	1016
	2
	2.3

+2.1
	263

	393
	CHLORINE
	1017
	2
	2.3

+5.1

+8
	265

	394
	CHLORODIFLUORO-METHANE (REFRIGERANT GAS R 22)
	1018
	2
	2.2
	20

	395
	CHLOROPENTAFLUORO​ETHANE (REFRIGERANT GAS R 115)
	1020
	2
	2.2
	20

	396
	1-CHLORO-1,2,2,2-TETRAFLUOROETHANE (REFRIGERANT GAS R 124)
	1021
	2
	2.2
	20

	397
	CHLOROTRIFLUORO-METHANE (REFRIGERANT GAS R 13)
	1022
	2
	2.2
	20

	398
	COAL GAS, COMPRESSED
	1023
	2
	2.3

+2.1
	263

	399
	CYANOGEN
	1026
	2
	2.3

+2.1
	263

	400
	CYCLOPROPANE
	1027
	2
	2.1
	23

	401
	DICHLORODIFLUORO​-METHANE (REFRIGERANT GAS R 12)
	1028
	2
	2.2
	20

	402
	DICHLOROFLUORO-METHANE (REFRIGERANT GAS R 21)
	1029
	2
	2.2
	20

	403
	1,1-DIFLUOROETHANE

(REFRIGERANT GAS R 152a)
	1030
	2
	2.1
	23

	404
	DIMETHYLAMINE, ANHYDROUS
	1032
	2
	2.1
	23

	405
	DIMETHYL ETHER
	1033
	2
	2.1
	23

	406
	ETHANE
	1035
	2
	2.1
	23

	407
	ETHYLAMINE
	1036
	2
	2.1
	23

	408
	ETHYL CHLORIDE
	1037
	2
	2.1
	23

	409
	ETHYLENE, REFRIGERATED LIQUID
	1038
	2
	2.1
	223

	410
	ETHYL METHYL ETHER
	1039
	2
	2.1
	23

	411
	ETHYLENE OXIDE
	1040
	2
	2.3

+2.1
	263

	412
	ETHYLENE OXIDE WITH NITROGEN up to a total pressure of 1 MPa (10 bar) at 50 °C
	1040
	2
	2.3

+2.1
	263

	413
	ETHYLENE OXIDE AND CARBON DIOXIDE MIXTURE with more than 9% but not more than 87% ethylene oxide
	1041
	2
	2.1
	239

	414
	FERTILIZER AMMONIATING SOLUTION with free ammonia
	1043
	2
	2.2
	

	415
	FIRE EXTINGUISHERS with compressed or liquefied gas
	1044
	2
	2.2
	

	416
	FLUORINE, COMPRESSED
	1045
	2
	2.3

+5.1

+8
	

	417
	HELIUM, COMPRESSED
	1046
	2
	2.2
	20

	418
	HYDROGEN BROMIDE, ANHYDROUS
	1048
	2
	2.3

+8
	268

	419
	HYDROGEN, COMPRESSED
	1049
	2
	2.1
	23

	420
	HYDROGEN CHLORIDE, ANHYDROUS
	1050
	2
	2.3

+8
	268

	421
	HYDROGEN CYANIDE, STABILIZED containing less than 3% water
	1051
	6.1
	6.1

+3
	

	422
	HYDROGEN FLUORIDE, ANHYDROUS
	1052
	8
	8

+6.1
	886

	423
	HYDROGEN SULPHIDE
	1053
	2
	2.3

+2.1
	263

	424
	ISOBUTYLENE
	1055
	2
	2.1
	23

	425
	KRYPTON, COMPRESSED
	1056
	2
	2.2
	20

	426
	LIGHTERS or LIGHTER REFILLS containing flammable gas
	1057
	2
	2.1
	

	427
	LIQUEFIED GASES, non​flammable, charged with nitrogen, carbon dioxide or air
	1058
	2
	2.2
	20

	428
	METHYLACETYLENE AND PROPADIENE MIXTURE, STABILIZED such as mixture P1 or mixture P2
	1060
	2
	2.1
	239

	429
	METHYLAMINE, ANHYDROUS
	1061
	2
	2.1
	23

	430
	METHYL BROMIDE with not more than 2% chloropicrin
	1062
	2
	2.3
	26

	431
	METHYL CHLORIDE (REFRIGERANT GAS R 40)
	1063
	2
	2.1
	23

	432
	METHYL MERCAPTAN
	1064
	2
	2.3

+2.1
	263

	433
	NEON, COMPRESSED
	1065
	2
	2.2
	20

	434
	NITROGEN, COMPRESSED
	1066
	2
	2.2
	20

	435
	DINITROGEN TETROXIDE (NITROGEN DIOXIDE)
	1067
	2
	2.3

+5.1

+8
	265

	436
	NITROSYL CHLORIDE
	1069
	2
	2.3

+8
	

	437
	NITROUS OXIDE
	1070
	2
	2.2

+5.1
	25

	438
	OILGAS, COMPRESSED
	1071
	2
	2.3

+2.1
	263

	439
	OXYGEN, COMPRESSED
	1072
	2
	2.2

+5.1
	25

	440
	OXYGEN, REFRIGERATED LIQUID
	1073
	2
	2.2

+5.1
	225

	441
	PETROLEUM GASES, LIQUEFIED
	1075
	2
	2.1
	23

	442
	PHOSGENE
	1076
	2
	2.3

+8
	268

	443
	PROPYLENE
	1077
	2
	2.1
	23

	444
	REFRIGERANT GAS, N.O.S., such as mixture F1, mixture F2 or mixture F3
	1078
	2
	2.2
	20

	445
	SULPHUR DIOXIDE
	1079
	2
	2.3

+8
	268

	446
	SULPHUR HEXAFLUORIDE
	1080
	2
	2.2
	20

	447
	TETRAFLUOROETHYLENE, STABILIZED
	1081
	2
	2.1
	239

	448
	TRIFLUOROCHLORO​ETHYLENE, STABILIZED (REFRIGERANT GAS R 1113)
	1082
	2
	2.3

+2.1
	263

	449
	TRIMETHYLAMINE, ANHYDROUS
	1083
	2
	2.1
	23

	450
	VINYL BROMIDE, STABILIZED
	1085
	2
	2.1
	239

	451
	VINYL CHLORIDE, STABILIZED
	1086
	2
	2.1
	239

	452
	VINYL METHYL ETHER, STABILIZED
	1087
	2
	2.1
	239

	453
	ACETAL
	1088
	3
	3
	33

	454
	ACETALDEHYDE
	1089
	3
	3
	33

	455
	ACETONE
	1090
	3
	3
	33

	456
	ACETONE OILS
	1091
	3
	3
	33

	457
	ACROLEIN, STABILIZED
	1092
	6.1
	6.1

+3
	663

	458
	ACRYLONITRILE, STABILIZED
	1093
	3
	3

+6.1
	336

	459
	ALLYL ALCOHOL
	1098
	6.1
	6.1

+3
	663

	460
	ALLYL BROMIDE
	1099
	3
	3

+6.1
	336

	461
	ALLYL CHLORIDE
	1100
	3
	3

+6.1
	336

	462
	AMYL ACETATES
	1104
	3
	3
	30

	463
	PENTANOLS
	1105
	3
	3
	33

	464
	PENTANOLS
	1105
	3
	3
	30

	465
	AMYLAMINE
	1106
	3
	3

+8
	338

	466
	AMYLAMINE
	1106
	3
	3

+8
	38

	467
	AMYL CHLORIDE
	1107
	3
	3
	33

	468
	1-PENTENE (n-AMYLENE)
	1108
	3
	3
	33

	469
	AMYL FORMATES
	1109
	3
	3
	30

	470
	n-AMYL METHYL KETONE
	1110
	3
	3
	30

	471
	AMYL MERCAPTAN
	1111
	3
	3
	33

	472
	AMYL NITRATE
	1112
	3
	3
	30

	473
	AMYL NITRITE
	1113
	3
	3
	33

	474
	BENZENE
	1114
	3
	3
	33

	475
	BUTANOLS
	1120
	3
	3
	33

	476
	BUTANOLS
	1120
	3
	3
	30

	477
	BUTYL ACETATES
	1123
	3
	3
	33

	478
	BUTYL ACETATES
	1123
	3
	3
	30

	479
	n-BUTYLAMINE
	1125
	3
	3

+8
	338

	480
	1-BROMOBUTANE
	1126
	3
	3
	33

	481
	CHLOROBUTANES
	1127
	3
	3
	33

	482
	n-BUTYL FORMATE
	1128
	3
	3
	33

	483
	BUTYRALDEHYDE
	1129
	3
	3
	33

	484
	CAMPHOROIL
	1130
	3
	3
	30

	485
	CARBON DISULPHIDE
	1131
	3
	3

+6.1
	336

	486
	ADHESIVES containing flammable liquid
	1133
	3
	3
	33

	487
	ADHESIVES containing flammable liquid (vapour pressure at 50 °C more than 110 kPa)
	1133
	3
	3
	33

	488
	ADHESIVES containing flammable liquid (vapour pressure at 50 °C not more than 110 kPa)
	1133
	3
	3
	33

	489
	ADHESIVES containing flammable liquid
	1133
	3
	3
	30

	490
	ADHESIVES containing flammable liquid (having a flash-point below 23°c and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1133
	3
	3
	

	491
	ADHESIVES containing flammable liquid (having a flash-point below 23°c and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1133
	3
	3
	

	492
	CHLOROBENZENE
	1134
	3
	3
	30

	493
	ETHYLENE CHLOROHYDRIN
	1135
	6.1
	6.1

+3
	663

	494
	COALTAR DISTILLATES, FLAMMABLE
	1136
	3
	3
	33

	495
	COAL TAR DISTILLATES, FLAMMABLE
	1136
	3
	3
	30

	496
	COATING SOLUTION (includes surface treatments or coatings used for industrial or other purposes such as vehicle under coating, drum or barrel lining)
	1139
	3
	3
	33

	497
	COATING SOLUTION (includes surface treatments or coatings used for industrial or other purposes such as vehicle under coating, drum or barrel lining) (vapour pressure at 50 °C more than 110 kPa)
	1139
	3
	3
	33

	498
	COATING SOLUTION (includes surface treatments or coatings used for industrial or other purposes such as vehicle under coating, drum or barrel lining) (vapour pressure at 50 °C not more than 110 kPa)
	1139
	3
	3
	33

	499
	COATING SOLUTION (includes surface treatments or coatings used for industrial or other purposes such as vehicle under coating, drum or barrel lining)
	1139
	3
	3
	30

	500
	COATING SOLUTION (includes surface treatments or coatings used for industrial or other purposes such as vehicle under coating, drum or barrel lining) (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1139
	3
	3
	

	501
	COATING SOLUTION (includes surface treatments or coatings used for industrial or other purposes such as vehicle under coating, drum or barrel lining) (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1139
	3
	3
	

	502
	CROTONALDEHYDE or CROTONALDEHYDE, STABILIZED
	1143
	6.1
	6.1

+3
	663

	503
	CROTONYLENE
	1144
	3
	3
	339

	504
	CYCLOHEXANE
	1145
	3
	3
	33

	505
	CYCLOPENTANE
	1146
	3
	3
	33

	506
	DECAHYDRO-NAPHTHALENE
	1147
	3
	3
	30

	507
	DIACETONE ALCOHOL
	1148
	3
	3
	33

	508
	DIACETONE ALCOHOL
	1148
	3
	3
	30

	509
	DIBUTYL ETHERS
	1149
	3
	3
	30

	510
	1,2-DICHLOROETHYLENE
	1150
	3
	3
	33

	511
	DICHLOROPENTANES
	1152
	3
	3
	30

	512
	ETHYLENE GLYCOL DIETHYL ETHER
	1153
	3
	3
	33

	513
	ETHYLENE GLYCOL DIETHYL ETHER
	1153
	3
	3
	30

	514
	DIETHYLAMINE
	1154
	3
	3

+8
	338

	515
	DIETHYL ETHER (ETHYL ETHER)
	1155
	3
	3
	33

	516
	DIETHYL KETONE
	1156
	3
	3
	33

	517
	DIISOBUTYL KETONE
	1157
	3
	3
	30

	518
	DIISOPROPYLAMINE
	1158
	3
	3

+8
	338

	519
	DIISOPROPYL ETHER
	1159
	3
	3
	33

	520
	DIMETHYLAMINE AQUEOUS SOLUTION
	1160
	3
	3

+8
	338

	521
	DIMETHYL CARBONATE
	1161
	3
	3
	33

	522
	DIMETHYLDICHLORO-SILANE
	1162
	3
	3

+8
	X338

	523
	DIMETHYLHYDRAZINE, UNSYMMETRICAL
	1163
	6.1
	6.1

+3

+8
	663

	524
	DIMETHYL SULPHIDE
	1164
	3
	3
	33

	525
	DIOXANE
	1165
	3
	3
	33

	526
	DIOXOLANE
	1166
	3
	3
	33

	527
	DIVINYL ETHER, STABILIZED
	1167
	3
	3
	339

	528
	EXTRACTS, AROMATIC, LIQUID (vapour pressure at 50 °C more than 110 kPa)
	1169
	3
	3
	33

	529
	EXTRACTS, AROMATIC, LIQUID (vapour pressure at 50 °C not more than 110 kPa)
	1169
	3
	3
	33

	530
	EXTRACTS, AROMATIC, LIQUID
	1169
	3
	3
	30

	531
	EXTRACTS, AROMATIC, LIQUID (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1169
	3
	3
	

	532
	EXTRACTS, AROMATIC, LIQUID (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1169
	3
	3
	

	533
	ETHANOL (ETHYL ALCOHOL) or ETHANOL SOLUTION (ETHYL ALCOHOL SOLUTION)
	1170
	3
	3
	33

	534
	ETHANOL SOLUTION (ETHYL ALCOHOL SOLUTION)
	1170
	3
	3
	30

	535
	ETHYLENEGLYCOL MONOETHYL ETHER
	1171
	3
	3
	30

	536
	ETHYLENEGLYCOL MONOETHYL ETHER ACETATE
	1172
	3
	3
	30

	537
	ETHYL ACETATE
	1173
	3
	3
	33

	538
	ETHYLBENZENE
	1175
	3
	3
	33

	539
	ETHYL BORATE
	1176
	3
	3
	33

	540
	2-ETHYLBUTYL ACETATE
	1177
	3
	3
	30

	541
	2-ETHYLBUTYRALDEHYDE
	1178
	3
	3
	33

	542
	ETHYL BUTYL ETHER
	1179
	3
	3
	33

	543
	ETHYL BUTYRATE
	1180
	3
	3
	30

	544
	ETHYL CHLOROACETATE
	1181
	6.1
	6.1

+3
	63

	545
	ETHYL CHLOROFORMATE
	1182
	6.1
	6.1

+3

+8
	663

	546
	ETHYLDICHLOROSILANE
	1183
	4.3
	4.3

+3

+8
	X338

	547
	ETHYLENE DICHLORIDE
	1184
	3
	3

+6.1
	336

	548
	ETHYLENEIMINE, STABILIZED
	1185
	6.1
	6.1

+3
	663

	549
	ETHYLENE GLYCOL MONOMETHYL ETHER
	1188
	3
	3
	30

	550
	ETHYLENE GLYCOL MONOMETHYL ETHER ACETATE
	1189
	3
	3
	30

	551
	ETHYL FORMATE
	1190
	3
	3
	33

	552
	OCTYL ALDEHYDES
	1191
	3
	3
	30

	553
	ETHYL LACTATE
	1192
	3
	3
	30

	554
	ETHYL METHYL KETONE (METHYL ETHYL KETONE)
	1193
	3
	3
	33

	555
	ETHYL NITRITE SOLUTION
	1194
	3
	3

+6.1
	336

	556
	ETHYL PROPIONATE
	1195
	3
	3
	33

	557
	ETHYLTRICHLOROSILANE
	1196
	3
	3

+8
	X338

	558
	EXTRACTS, FLAVOURING, LIQUID (vapour pressure at 50 °C more than 110 kPa)
	1197
	3
	3
	33

	559
	EXTRACTS, FLAVOURING, LIQUID (vapour pressure at 50 °C not more than 110 kPa)
	1197
	3
	3
	33

	560
	EXTRACTS, FLAVOURING, LIQUID
	1197
	3
	3
	30

	561
	EXTRACTS, FLAVOURING, LIQUID (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1197
	3
	3
	

	562
	EXTRACTS, FLAVOURING, LIQUID (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1197
	3
	3
	

	563
	FORMALDEHYDE SOLUTION, FLAMMABLE
	1198
	3
	3

+8
	38

	564
	FURALDEHYDES
	1199
	6.1
	6.1

+3
	63

	565
	FUSEL OIL
	1201
	3
	3
	33

	566
	FUSEL OIL
	1201
	3
	3
	30

	567
	GAS OIL or DIESEL FUEL or HEATING OIL, LIGHT (flash-point not more than 60 °C)
	1202
	3
	3
	30

	568
	DIESEL FUEL complying with standard EN 590:2013 + AC:2014 or GAS OIL or HEATING OIL, LIGHT with a flash-point as specified in EN 590:2013 + AC:2014
	1202
	3
	3
	30

	569
	GAS OIL or DIESEL FUEL or HEATING OIL, LIGHT (flash-point more than 60 °C and not more than 100 °C)
	1202
	3
	3
	30

	570
	MOTOR SPIRIT or GASOLINE or PETROL
	1203
	3
	3
	33

	571
	NITROGLYCERIN SOLUTION IN ALCOHOL with not more than 1% nitroglycerin
	1204
	3
	3
	

	572
	HEPTANES
	1206
	3
	3
	33

	573
	HEXALDEHYDE
	1207
	3
	3
	30

	574
	HEXANES
	1208
	3
	3
	33

	575
	PRINTING INK, flammable or

PRINTING INK RELATED MATERIAL (including printing ink thinning or reducing compound), flammable
	1210
	3
	3
	33

	576
	PRINTING INK, flammable or PRINTING INK RELATED MATERIAL (including printing ink thinning or reducing compound), flammable (vapour pressure at 50 °C more than 110 kPa)
	1210
	3
	3
	33

	577
	PRINTING INK, flammable or PRINTING INK RELATED MATERIAL (including printing ink thinning or reducing compound), flammable (vapour pressure at 50 °C not more than 110 kPa)
	1210
	3
	3
	33

	578
	PRINTING INK, flammable or PRINTING INK RELATED MATERIAL (including printing ink thinning or reducing compound), flammable
	1210
	3
	3
	30

	579
	PRINTING INK, flammable or

PRINTING INK RELATED MATERIAL (including printing ink thinning or reducing compound), flammable (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1210
	3
	3
	

	580
	PRINTING INK, flammable or PRINTING INK RELATED MATERIAL (including printing ink thinning or reducing compound), flammable (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1210
	3
	3
	

	581
	ISOBUTANOL (ISOBUTYL ALCOHOL)
	1212
	3
	3
	30

	582
	ISOBUTYL ACETATE
	1213
	3
	3
	33

	583
	ISOBUTYLAMINE
	1214
	3
	3

+8
	338

	584
	ISOOCTENES
	1216
	3
	3
	33

	585
	ISOPRENE, STABILIZED
	1218
	3
	3
	339

	586
	ISOPROPANOL (ISOPROPYL ALCOHOL)
	1219
	3
	3
	33

	587
	ISOPROPYL ACETATE
	1220
	3
	3
	33

	588
	ISOPROPYLAMINE
	1221
	3
	3 +8
	338

	589
	ISOPROPYL NITRATE
	1222
	3
	3
	

	590
	KEROSENE
	1223
	3
	3
	30

	591
	KETONES, LIQUID, N.O.S. (vapour pressure at 50 °C more than 110 kPa)
	1224
	3
	3
	33

	592
	KETONES, LIQUID, N.O.S. (vapour pressure at 50 °C not more than 110 kPa)
	1224
	3
	3
	33

	593
	KETONES, LIQUID, N.O.S.
	1224
	3
	3
	30

	594
	MERCAPTANS, LIQUID, FLAMMABLE, TOXIC, N.O.S. or MERCAPTAN MIXTURE, LIQUID, FLAMMABLE, TOXIC, N.O.S.
	1228
	3
	3

+6.1
	336

	595
	MERCAPTANS, LIQUID, FLAMMABLE, TOXIC, N.O.S. or MERCAPTAN MIXTURE, LIQUID, FLAMMABLE, TOXIC, N.O.S.
	1228
	3
	3

+6.1
	36

	596
	MESITYL OXIDE
	1229
	3
	3
	30

	597
	METHANOL
	1230
	3
	3

+6.1
	336

	598
	METHYL ACETATE
	1231
	3
	3
	33

	599
	METHYLAMYL ACETATE
	1233
	3
	3
	30

	600
	METHYLAL
	1234
	3
	3
	33

	601
	METHYLAMINE, AQUEOUS SOLUTION
	1235
	3
	3

+8
	338

	602
	METHYL BUTYRATE
	1237
	3
	3
	33

	603
	METHYL CHLOROFORMATE
	1238
	6.1
	6.1

+3

+8
	663

	604
	METHYL CHLORO-METHYL ETHER
	1239
	6.1
	6.1

+3
	663

	605
	METHYLDICHLOROSILANE
	1242
	4.3
	4.3

+3

+8
	X338

	606
	METHYL FORMATE
	1243
	3
	3
	33

	607
	METHYLHYDRAZINE
	1244
	6.1
	6.1

+3

+8
	663

	608
	METHYL ISOBUTYL KETONE
	1245
	3
	3
	33

	609
	METHYL ISOPROPENYL KETONE, STABILIZED
	1246
	3
	3
	339

	610
	METHYL METHACRYLATE MONOMER, STABILIZED
	1247
	3
	3
	339

	611
	METHYL PROPIONATE
	1248
	3
	3
	33

	612
	METHYL PROPYL KETONE
	1249
	3
	3
	33

	613
	METHYLTRICHLORO-SILANE
	1250
	3
	3 +8
	X338

	614
	METHYL VINYL KETONE, STABILIZED
	1251
	6.1
	6.1

+3

+8
	639

	615
	NICKEL CARBONYL
	1259
	6.1
	6.1

+3
	663

	616
	NITROMETHANE
	1261
	3
	3
	

	617
	OCTANES
	1262
	3
	3
	33

	618
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound)
	1263
	3
	3
	33

	619
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound) (vapour pressure at 50 °C more than 110 kPa)
	1263
	3
	3
	33

	620
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound) (vapour pressure at 50 °C not more than 110 kPa)
	1263
	3
	3
	33

	621
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound)
	1263
	3
	3
	30

	622
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound) (having a flash- point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1263
	3
	3
	

	623
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound) (having a flash- point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1263
	3
	3
	

	624
	PARALDEHYDE
	1264
	3
	3
	30

	625
	PENTANES, liquid
	1265
	3
	3
	33

	626
	PENTANES liquid
	1265
	3
	3
	33

	627
	PERFUMERY PRODUCTS with flammable solvents (vapour pressure at 50 °C more than 110 kPa)
	1266
	3
	3
	33

	628
	PERFUMERY PRODUCTS with flammable solvents (vapour pressure at 50 °C not more than 110 kPa)
	1266
	3
	3
	33

	629
	PERFUMERY PRODUCTS with flammable solvents
	1266
	3
	3
	30

	630
	PERFUMERY PRODUCTS with flammable solvents (having a flash​point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1266
	3
	3
	

	631
	PERFUMERY PRODUCTS with flammable solvents (having a flash​point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1266
	3
	3
	

	632
	PETROLEUM CRUDE OIL
	1267
	3
	3
	33

	633
	PETROLEUM CRUDE OIL (vapour pressure at 50 °C more than 110 kPa)
	1267
	3
	3
	33

	634
	PETROLEUM CRUDE OIL (vapour pressure at 50 °C not more than 110 kPa)
	1267
	3
	3
	33

	635
	PETROLEUM CRUDE OIL
	1267
	3
	3
	30

	636
	PETROLEUM DISTILLATES,

N.O.S. or PETROLEUM

PRODUCTS, N.O.S.
	1268
	3
	3
	33

	637
	PETROLEUM DISTILLATES, N.O.S. or PETROLEUM PRODUCTS, N.O.S. (vapour pressure at 50 °C more than 110 kPa)
	1268
	3
	3
	33

	638
	PETROLEUM DISTILLATES, N.O.S. or PETROLEUM PRODUCTS, N.O.S. (vapour pressure at 50 °C not more than 110 kPa)
	1268
	3
	3
	33

	639
	PETROLEUM DISTILLATES,

N.O.S. or PETROLEUM

PRODUCTS, N.O.S.
	1268
	3
	3
	30

	640
	PINE OIL
	1272
	3
	3
	30

	641
	n-PROPANOL (PROPYL ALCOHOL, NORMAL)
	1274
	3
	3
	33

	642
	n-PROPANOL (PROPYL ALCOHOL, NORMAL)
	1274
	3
	3
	30

	643
	PROPIONALDEHYDE
	1275
	3
	3
	33

	644
	n-PROPYL ACETATE
	1276
	3
	3
	33

	645
	PROPYLAMINE
	1277
	3
	3

+8
	338

	646
	1-CHLOROPROPANE
	1278
	3
	3
	33

	647
	1,2-DICHLOROPROPANE
	1279
	3
	3
	33

	648
	PROPYLENE OXIDE
	1280
	3
	3
	33

	649
	PROPYL FORMATES
	1281
	3
	3
	33

	650
	PYRIDINE
	1282
	3
	3
	33

	651
	ROSIN OIL (vapour pressure at 50 °C more than 110 kPa)
	1286
	3
	3
	33

	652
	ROSIN OIL (vapour pressure at 50 °C not more than 110 kPa)
	1286
	3
	3
	33

	653
	ROSIN OIL
	1286
	3
	3
	30

	654
	ROSIN OIL (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1286
	3
	3
	

	655
	ROSIN OIL (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1286
	3
	3
	

	656
	RUBBER SOLUTION (vapour pressure at 50 °C more than 110 kPa)
	1287
	3
	3
	33

	657
	RUBBER SOLUTION (vapour pressure at 50 °C not more than 110 kPa)
	1287
	3
	3
	33

	658
	RUBBER SOLUTION
	1287
	3
	3
	30

	659
	RUBBER SOLUTION (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1287
	3
	3
	

	660
	RUBBER SOLUTION (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1287
	3
	3
	

	661
	SHALE OIL
	1288
	3
	3
	33

	662
	SHALE OIL
	1288
	3
	3
	30

	663
	SODIUM METHYLATE SOLUTION in alcohol
	1289
	3
	3

+8
	338

	664
	SODIUM METHYLATE SOLUTION in alcohol
	1289
	3
	3

+8
	38

	665
	TETRAETHYL SILICATE
	1292
	3
	3
	30

	666
	TINCTURES, MEDICINAL
	1293
	3
	3
	33

	667
	TINCTURES, MEDICINAL
	1293
	3
	3
	30

	668
	TOLUENE
	1294
	3
	3
	33

	669
	TRICHLOROSILANE
	1295
	4.3
	4.3

+3

+8
	X338

	670
	TRIETHYLAMINE
	1296
	3
	3

+8
	338

	671
	TRIMETHYLAMINE, AQUEOUS SOLUTION, not more than 50% trimethylamine, by mass
	1297
	3
	3

+8
	338

	672
	TRIMETHYLAMINE, AQUEOUS SOLUTION, not more than 50% trimethylamine, by mass
	1297
	3
	3+8
	338

	673
	TRIMETHYLAMINE, AQUEOUS SOLUTION, not more than 50% trimethylamine, by mass
	1297
	3
	3 

+8
	38

	674
	TRIMETHYLCHLORO-SILANE
	1298
	3
	3 

+8
	X338

	675
	TURPENTINE
	1299
	3
	3
	30

	676
	TURPENTINE SUBSTITUTE
	1300
	3
	3
	33

	677
	TURPENTINE SUBSTITUTE
	1300
	3
	3
	30

	678
	VINYL ACETATE, STABILIZED
	1301
	3
	3
	339

	679
	VINYL ETHYL ETHER, STABILIZED
	1302
	3
	3
	339

	680
	VINYLIDENE CHLORIDE, STABILIZED
	1303
	3
	3
	339

	681
	VINYL ISOBUTYL ETHER, STABILIZED
	1304
	3
	3
	339

	682
	VINYLTRICHLOROSILANE
	1305
	3
	3

+8
	X338

	683
	WOOD PRESERVATIVES,

LIQUID (vapour pressure at 50 °C more than 110 kPa)
	1306
	3
	3
	33

	684
	WOOD PRESERVATIVES, LIQUID (vapour pressure at 50 °C not more than 110 kPa)
	1306
	3
	3
	33

	685
	WOOD PRESERVATIVES, LIQUID
	1306
	3
	3
	30

	686
	WOOD PRESERVATIVES, LIQUID (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1306
	3
	3
	

	687
	WOOD PRESERVATIVES, LIQUID (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1306
	3
	3
	

	688
	XYLENES
	1307
	3
	3
	33

	689
	XYLENES
	1307
	3
	3
	30

	690
	ZIRCONIUM SUSPENDED IN A FLAMMABLE LIQUID
	1308
	3
	3
	33

	691
	ZIRCONIUM SUSPENDED IN A FLAMMABLE LIQUID (vapour pressure at 50 °C more than 110 kPa)
	1308
	3
	3
	33

	692
	ZIRCONIUM SUSPENDED IN A FLAMMABLE LIQUID (vapour pressure at 50 °C not more than 110 kPa)
	1308
	3
	3
	33

	693
	ZIRCONIUM SUSPENDED IN A FLAMMABLE LIQUID
	1308
	3
	3
	30

	694
	ALUMINIUM POWDER, COATED
	1309
	4.1
	4.1
	40

	695
	ALUMINIUM POWDER, COATED
	1309
	4.1
	4.1
	40

	696
	AMMONIUM PICRATE, WETTED with not less than 10% water, by mass
	1310
	4.1
	4.1
	

	697
	BORNEOL
	1312
	4.1
	4.1
	40

	698
	CALCIUM RESINATE
	1313
	4.1
	4.1
	40

	699
	CALCIUM RESINATE, FUSED
	1314
	4.1
	4.1
	40

	700
	COBALT RESINATE, PRECIPITATED
	1318
	4.1
	4.1
	40

	701
	DINITROPHENOL, WETTED with not less than 15% water, by mass
	1320
	4.1
	4.1

+6.1
	

	702
	DINITROPHENOLATES, WETTED with not less than 15% water, by mass
	1321
	4.1
	4.1

+6.1
	

	703
	DINITRORESORCINOL, WETTED with not less than 15% water, by mass
	1322
	4.1
	4.1
	

	704
	FERROCERIUM
	1323
	4.1
	4.1
	40

	705
	FILMS, NITROCELLULOSE BASE, gelatin coated, except scrap
	1324
	4.1
	4.1
	

	706
	FLAMMABLE SOLID, ORGANIC, N.O.S.
	1325
	4.1
	4.1
	40

	707
	FLAMMABLE SOLID, ORGANIC, N.O.S.
	1325
	4.1
	4.1
	40

	708
	HAFNIUM POWDER, WETTED with not less than 25% water
	1326
	4.1
	4.1
	40

	709
	Hay, Straw or Bhusa
	1327
	4.1
	
	

	710
	HEXAM ETHYLENETE-TRAMINE
	1328
	4.1
	4.1
	40

	711
	MANGANESE RESINATE
	1330
	4.1
	4.1
	40

	712
	MATCHES, ‘STRIKE ANYWHERE’
	1331
	4.1
	4.1
	

	713
	METALDEHYDE
	1332
	4.1
	4.1
	40

	714
	CERIUM, slabs, ingots or rods
	1333
	4.1
	4.1
	

	715
	NAPHTHALENE, CRUDE or NAPHTHALENE, REFINED
	1334
	4.1
	4.1
	40

	716
	NITROGUANIDINE (PICRITE), WETTED with not less than 20% water, by mass
	1336
	4.1
	4.1
	

	717
	NITROSTARCH, WETTED with not less than 20% water, by mass
	1337
	4.1
	4.1
	

	718
	PHOSPHORUS, AMORPHOUS
	1338
	4.1
	4.1
	40

	719
	PHOSPHORUS HEPTASULPHIDE, free from yellow and white phosphorus
	1339
	4.1
	4.1
	40

	720
	PHOSPHORUS PENTASULPHIDE, free from yellow and white phosphorus
	1340
	4.3
	4.3

+4.1
	423

	721
	PHOSPHORUS SESQUISULPHIDE, free from yellow and white phosphorus
	1341
	4.1
	4.1
	40

	722
	PHOSPHORUS TRISULPHIDE, free from yellow and white phosphorus
	1343
	4.1
	4.1
	40

	723
	TRINITROPHENOL (PICRIC ACID), WETTED with not less than 30% water, by mass
	1344
	4.1
	4.1
	

	724
	RUBBER SCRAP or RUBBER SHODDY, powdered or granulated
	1345
	4.1
	4.1
	40

	725
	SILICON POWDER, AMORPHOUS
	1346
	4.1
	4.1
	40

	726
	SILVER PICRATE, WETTED with not less than 30% water, by mass
	1347
	4.1
	4.1
	

	727
	SODIUM DINITRO-o- CRESOLATE, WETTED with not less than 15% water, by mass
	1348
	4.1
	4.1

+6.1
	

	728
	SODIUM PICRAMATE, WETTED with not less than 20% water, by mass
	1349
	4.1
	4.1
	

	729
	SULPHUR
	1350
	4.1
	4.1
	40

	730
	TITANIUM POWDER, WETTED with not less than 25% water
	1352
	4.1
	4.1
	40

	731
	FIBRES or FABRICS IMPREGNATED WITH WEAKLY NITRATED NITROCELLULOSE, N.O.S.
	1353
	4.1
	4.1
	

	732
	TRINITROBENZENE, WETTED with not less than 30% water, by mass
	1354
	4.1
	4.1
	

	733
	TRINITROBENZOIC ACID, WETTED with not less than 30% water, by mass
	1355
	4.1
	4.1
	

	734
	TRINITROTOLUENE (TNT), WETTED with not less than 30% water, by mass
	1356
	4.1
	4.1
	

	735
	UREA NITRATE, WETTED with not less than 20% water, by mass
	1357
	4.1
	4.1
	

	736
	ZIRCONIUM POWDER, WETTED with not less than 25% water
	1358
	4.1
	4.1
	40

	737
	CALCIUM PHOSPHIDE
	1360
	4.3
	4.3

+6.1
	

	738
	CARBON, animal or vegetable origin
	1361
	4.2
	4.2
	40

	739
	CARBON, animal or vegetable origin
	1361
	4.2
	4.2
	40

	740
	CARBON, ACTIVATED
	1362
	4.2
	4.2
	40

	741
	COPRA
	1363
	4.2
	4.2
	40

	742
	COTTON WASTE, OILY
	1364
	4.2
	4.2
	40

	743
	COTTON, WET
	1365
	4.2
	4.2
	40

	744
	P-NITROSODIMETHYL-ANILINE
	1369
	4.2
	4.2
	40

	745
	Fibres, animal or fibres, vegetable burnt, wet or damp
	1372
	4.2
	
	

	746
	FIBRES or FABRICS, ANIMAL or VEGETABLE or SYNTHETIC, N.O.S. with oil
	1373
	4.2
	4.2
	40

	747
	FISH MEAL (FISH SCRAP), UNSTABILIZED
	1374
	4.2
	4.2
	40

	748
	IRON OXIDE, SPENT or IRON SPONGE, SPENT obtained from coal gas purification
	1376
	4.2
	4.2
	40

	749
	METAL CATALYST, WETTED with a visible excess of liquid
	1378
	4.2
	4.2
	40

	750
	PAPER, UNSATURATED OIL TREATED, incompletely dried (including carbon paper)
	1379
	4.2
	4.2
	40

	751
	PENTABORANE
	1380
	4.2
	4.2

+6.1
	333

	752
	PHOSPHORUS, WHITE or YELLOW, UNDER WATER or IN SOLUTION
	1381
	4.2
	4.2 

+6.1
	46

	753
	PHOSPHORUS, WHITE or YELLOW, DRY
	1381
	4.2
	4.2 

+6.1
	46

	754
	POTASSIUM SULPHIDE, ANHYDROUS or POTASSIUM SULPHIDE with less than 30% water of crystallization
	1382
	4.2
	4.2
	40

	755
	PYROPHORIC METAL, N.O.S. or PYROPHORIC ALLOY, N.O.S.
	1383
	4.2
	4.2
	43

	756
	SODIUM DITHIONITE (SODIUM HYDROSULPHITE)
	1384
	4.2
	4.2
	40

	757
	SODIUM SULPHIDE, ANHYDROUS or SODIUM SULPHIDE with less than 30% water of crystallization
	1385
	4.2
	4.2
	40

	758
	SEED CAKE with more than 1.5% oil and not more than 11 % moisture
	1386
	4.2
	4.2
	40

	759
	Wool waste, wet
	1387
	4.2
	
	

	760
	ALKALI METAL AMALGAM, LIQUID
	1389
	4.3
	4.3
	X323

	761
	ALKALI METAL AMIDES
	1390
	4.3
	4.3
	423

	762
	ALKALI METAL DISPERSION or ALKALINE EARTH METAL DISPERSION
	1391
	4.3
	4.3
	X323

	763
	ALKALINE EARTH METAL AMALGAM, LIQUID
	1392
	4.3
	4.3
	X323

	764
	ALKALINE EARTH METAL ALLOY, N.O.S.
	1393
	4.3
	4.3
	423

	765
	ALUMINIUM CARBIDE
	1394
	4.3
	4.3
	423

	766
	ALUMINIUM FERROSILICON POWDER
	1395
	4.3
	4.3

+6.1
	462

	767
	ALUMINIUM POWDER, UNCOATED
	1396
	4.3
	4.3
	423

	768
	ALUMINIUM POWDER, UNCOATED
	1396
	4.3
	4.3
	423

	769
	ALUMINIUM PHOSPHIDE
	1397
	4.3
	4.3

+6.1
	

	770
	ALUMINIUM SILICON POWDER, UNCOATED
	1398
	4.3
	4.3
	423

	771
	BARIUM
	1400
	4.3
	4.3
	423

	772
	CALCIUM
	1401
	4.3
	4.3
	423

	773
	CALCIUM CARBIDE
	1402
	4.3
	4.3
	X423

	774
	CALCIUM CARBIDE
	1402
	4.3
	4.3
	423

	775
	CALCIUM CYANAMIDE with more than 0.1% calcium carbide
	1403
	4.3
	4.3
	423

	776
	CALCIUM HYDRIDE
	1404
	4.3
	4.3
	

	777
	CALCIUM SILICIDE
	1405
	4.3
	4.3
	423

	778
	CALCIUM SILICIDE
	1405
	4.3
	4.3
	423

	779
	CAESIUM
	1407
	4.3
	4.3
	X423

	780
	FERROSILICON with 30% or more but less than 90% silicon
	1408
	4.3
	4.3

+6.1
	462

	781
	METAL HYDRIDES, WATER- REACTIVE, N.O.S.
	1409
	4.3
	4.3
	

	782
	METAL HYDRIDES, WATER- REACTIVE, N.O.S.
	1409
	4.3
	4.3
	423

	783
	LITHIUM ALUMINIUM HYDRIDE
	1410
	4.3
	4.3
	

	784
	LITHIUM ALUMINIUM HYDRIDE, ETHEREAL
	1411
	4.3
	4.3

+3
	

	785
	LITHIUM BOROHYDRIDE
	1413
	4.3
	4.3
	

	786
	LITHIUM HYDRIDE
	1414
	4.3
	4.3
	

	787
	LITHIUM
	1415
	4.3
	4.3
	X423

	788
	LITHIUM SILICON
	1417
	4.3
	4.3
	423

	789
	MAGNESIUM POWDER or MAGNESIUM ALLOYS POWDER
	1418
	4.3
	4.3

+4.2
	

	790
	MAGNESIUM POWDER or MAGNESIUM ALLOYS POWDER
	1418
	4.3
	4.3

+4.2
	423

	791
	MAGNESIUM POWDER or MAGNESIUM ALLOYS POWDER
	1418
	4.3
	4.3

+4.2
	423

	792
	MAGNESIUM ALUMINIUM PHOSPHIDE
	1419
	4.3
	4.3 +6.1
	

	793
	POTASSIUM METAL ALLOYS, LIQUID
	1420
	4.3
	4.3
	X323

	794
	ALKALI METAL ALLOY, LIQUID, N.O.S.
	1421
	4.3
	4.3
	X323

	795
	POTASSIUM SODIUM ALLOYS, LIQUID
	1422
	4.3
	4.3
	X323

	796
	RUBIDIUM
	1423
	4.3
	4.3
	X423

	797
	SODIUM BOROHYDRIDE
	1426
	4.3
	4.3
	

	798
	SODIUM HYDRIDE
	1427
	4.3
	4.3
	

	799
	SODIUM
	1428
	4.3
	4.3
	X423

	800
	SODIUM METHYLATE
	1431
	4.2
	4.2

+8
	48

	801
	SODIUM PHOSPHIDE
	1432
	4.3
	4.3

+6.1
	

	802
	STANNIC PHOSPHIDES
	1433
	4.3
	4.3

+6.1
	

	803
	ZINC ASHES
	1435
	4.3
	4.3
	423

	804
	ZINC POWDER or ZINC DUST
	1436
	4.3
	4.3+4.2
	

	805
	ZINC POWDER or ZINC DUST
	1436
	4.3
	4.3

+4.2
	423

	806
	ZINC POWDER or ZINC DUST
	1436
	4.3
	4.3

+4.2
	423

	807
	ZIRCONIUM HYDRIDE
	1437
	4.1
	4.1
	40

	808
	ALUMINIUM NITRATE
	1438
	5.1
	5.1
	50

	809
	AMMONIUM DICHROMATE
	1439
	5.1
	5.1
	50

	810
	AMMONIUM PERCHLORATE
	1442
	5.1
	5.1
	50

	811
	AMMONIUM PERSULPHATE
	1444
	5.1
	5.1
	50

	812
	BARIUM CHLORATE, SOLID
	1445
	5.1
	5.1

+6.1
	56

	813
	BARIUM NITRATE
	1446
	5.1
	5.1

+6.1
	56

	814
	BARIUM PERCHLORATE, SOLID
	1447
	5.1
	5.1

+6.1
	56

	815
	BARIUM PERMANGANATE
	1448
	5.1
	5.1

+6.1
	56

	816
	BARIUM PEROXIDE
	1449
	5.1
	5.1

+6.1
	56

	817
	BROMATES, INORGANIC, N.O.S.
	1450
	5.1
	5.1
	50

	818
	CAESIUM NITRATE
	1451
	5.1
	5.1
	50

	819
	CALCIUM CHLORATE
	1452
	5.1
	5.1
	50

	820
	CALCIUM CHLORITE
	1453
	5.1
	5.1
	50

	821
	CALCIUM NITRATE
	1454
	5.1
	5.1
	50

	822
	CALCIUM PERCHLORATE
	1455
	5.1
	5.1
	50

	823
	CALCIUM PERMANGANATE
	1456
	5.1
	5.1
	50

	824
	CALCIUM PEROXIDE
	1457
	5.1
	5.1
	50

	825
	CHLORATE AND BORATE MIXTURE
	1458
	5.1
	5.1
	50

	826
	CHLORATE AND BORATE MIXTURE
	1458
	5.1
	5.1
	50

	827
	CHLORATE AND MAGNESIUM CHLORIDE MIXTURE, SOLID
	1459
	5.1
	5.1
	50

	828
	CHLORATE AND MAGNESIUM CHLORIDE MIXTURE, SOLID
	1459
	5.1
	5.1
	50

	829
	CHLORATES, INORGANIC, N.O.S.
	1461
	5.1
	5.1
	50

	830
	CHLORITES, INORGANIC, N.O.S.
	1462
	5.1
	5.1
	50

	831
	CHROMIUM TRIOXIDE, ANHYDROUS
	1463
	5.1
	5.1 

+6.1

+8
	568

	832
	DIDYMIUM NITRATE
	1465
	5.1
	5.1
	50

	833
	FERRIC NITRATE
	1466
	5.1
	5.1
	50

	834
	GUANIDINE NITRATE
	1467
	5.1
	5.1
	50

	835
	LEAD NITRATE
	1469
	5.1
	5.1

+6.1
	56

	836
	LEAD PERCHLORATE, SOLID
	1470
	5.1
	5.1

+6.1
	56

	837
	LITHIUM HYPOCHLORITE, DRY or LITHIUM HYPOCHLORITE MIXTURE
	1471
	5.1
	5.1
	50

	838
	LITHIUM HYPOCHLORITE, DRY or LITHIUM HYPOCHLORITE MIXTURE
	1471
	5.1
	5.1
	50

	839
	LITHIUM PEROXIDE
	1472
	5.1
	5.1
	50

	840
	MAGNESIUM BROMATE
	1473
	5.1
	5.1
	50

	841
	MAGNESIUM NITRATE
	1474
	5.1
	5.1
	50

	842
	MAGNESIUM PERCHLORATE
	1475
	5.1
	5.1
	50

	843
	MAGNESIUM PEROXIDE
	1476
	5.1
	5.1
	50

	844
	NITRATES, INORGANIC, N.O.S.
	1477
	5.1
	5.1
	50

	845
	NITRATES, INORGANIC, N.O.S.
	1477
	5.1
	5.1
	50

	846
	OXID-1IZING SOLID, N.O.S.
	1479
	5.1
	5.1
	

	847
	OXIDIZING SOLID, N.O.S.
	1479
	5.1
	5.1
	50

	848
	OXIDIZING SOLID, N.O.S.
	1479
	5.1
	5.1
	50

	849
	PERCHLORATES, INORGANIC, N.O.S.
	1481
	5.1
	5.1
	50

	850
	PERCHLORATES, INORGANIC, N.O.S.
	1481
	5.1
	5.1
	50

	851
	PERMANGANATES, INORGANIC, N.O.S.
	1482
	5.1
	5.1
	50

	852
	PERMANGANATES, INORGANIC, N.O.S.
	1482
	5.1
	5.1
	50

	853
	PEROXIDES, INORGANIC, N.O.S.
	1483
	5.1
	5.1
	50

	854
	PEROXIDES, INORGANIC, N.O.S.
	1483
	5.1
	5.1
	50

	855
	POTASSIUM BROMATE
	1484
	5.1
	5.1
	50

	856
	POTASSIUM CHLORATE
	1485
	5.1
	5.1
	50

	857
	POTASSIUM NITRATE
	1486
	5.1
	5.1
	50

	858
	POTASSIUM NITRATE AND SODIUM NITRITE MIXTURE
	1487
	5.1
	5.1
	50

	859
	POTASSIUM NITRITE
	1488
	5.1
	5.1
	50

	860
	POTASSIUM PERCHLORATE
	1489
	5.1
	5.1
	50

	861
	POTASSIUM PERMANGANATE
	1490
	5.1
	5.1
	50

	862
	POTASSIUM PEROXIDE
	1491
	5.1
	5.1
	

	863
	POTASSIUM PERSULPHATE
	1492
	5.1
	5.1
	50

	864
	SILVER NITRATE
	1493
	5.1
	5.1
	50

	865
	SODIUM BROMATE
	1494
	5.1
	5.1
	50

	866
	SODIUM CHLORATE
	1495
	5.1
	5.1
	50

	867
	SODIUM CHLORITE
	1496
	5.1
	5.1
	50

	868
	SODIUM NITRATE
	1498
	5.1
	5.1
	50

	869
	SODIUM NITRATE AND POTASSIUM NITRATE MIXTURE
	1499
	5.1
	5.1
	50

	870
	SODIUM NITRITE
	1500
	5.1
	5.1

+6.1
	56

	871
	SODIUM PERCHLORATE
	1502
	5.1
	5.1
	50

	872
	SODIUM PERMANGANATE
	1503
	5.1
	5.1
	50

	873
	SODIUM PEROXIDE
	1504
	5.1
	5.1
	

	874
	SODIUM PERSULPHATE
	1505
	5.1
	5.1
	50

	875
	STRONTIUM CHLORATE
	1506
	5.1
	5.1
	50

	876
	STRONTIUM NITRATE
	1507
	5.1
	5.1
	50

	877
	STRONTIUM PERCHLORATE
	1508
	5.1
	5.1
	50

	878
	STRONTIUM PEROXIDE
	1509
	5.1
	5.1
	50

	879
	TETRANITROMETHANE
	1510
	6.1
	6.1

+5.1
	665

	880
	UREA HYDROGEN PEROXIDE
	1511
	5.1
	5.1

+8
	58

	881
	ZINC AMMONIUM NITRITE
	1512
	5.1
	5.1
	50

	882
	ZINC CHLORATE
	1513
	5.1
	5.1
	50

	883
	ZINC NITRATE
	1514
	5.1
	5.1
	50

	884
	ZINC PERMANGANATE
	1515
	5.1
	5.1
	50

	885
	ZINC PEROXIDE
	1516
	5.1
	5.1
	50

	886
	ZIRCONIUM PICRAMATE, WETTED with not less than 20% water, by mass
	1517
	4.1
	4.1
	

	887
	ACETONE CYANOHYDRIN, STABILIZED
	1541
	6.1
	6.1
	669

	888
	ALKALOIDS, SOLID, N.O.S. or ALKALOID SALTS, SOLID, N.O.S.
	1544
	6.1
	6.1
	66

	889
	ALKALOIDS, SOLID, N.O.S. or ALKALOID SALTS, SOLID, N.O.S.
	1544
	6.1
	6.1
	60

	890
	ALKALOIDS, SOLID, N.O.S. or ALKALOID SALTS, SOLID, N.O.S.
	1544
	6.1
	6.1
	60

	891
	ALLYL ISOTHIOCYANATE, STABILIZED
	1545
	6.1
	6.1

+3
	639

	892
	AMMONIUM ARSENATE
	1546
	6.1
	6.1
	60

	893
	ANILINE
	1547
	6.1
	6.1
	60

	894
	ANILINE HYDROCHLORIDE
	1548
	6.1
	6.1
	60

	895
	ANTIMONY COMPOUND, INORGANIC, SOLID, N.O.S.
	1549
	6.1
	6.1
	60

	896
	ANTIMONY LACTATE
	1550
	6.1
	6.1
	60

	897
	ANTIMONY POTASSIUM TARTRATE
	1551
	6.1
	6.1
	60

	898
	ARSENIC ACID, LIQUID
	1553
	6.1
	6.1
	66

	899
	ARSENIC ACID, SOLID
	1554
	6.1
	6.1
	60

	900
	ARSENIC BROMIDE
	1555
	6.1
	6.1
	60

	901
	ARSENIC COMPOUND, LIQUID, N.O.S., inorganic, including: Arsenates, n.o.s., Arsenites, n.o.s.; and Arsenic sulphides, n.o.s.
	1556
	6.1
	6.1
	66

	902
	ARSENIC COMPOUND, LIQUID, N.O.S., inorganic, including: Arsenates, n.o.s., Arsenites, n.o.s.; and Arsenic sulphides, n.o.s.
	1556
	6.1
	6.1
	60

	903
	ARSENIC COMPOUND, LIQUID, N.O.S., inorganic, including: Arsenates, n.o.s., Arsenites, n.o.s.; and Arsenic sulphides, n.o.s.
	1556
	6.1
	6.1
	60

	904
	ARSENIC COMPOUND, SOLID, N.O.S., inorganic, including: Arsenates, n.o.s.; Arsenites, n.o.s.; and Arsenic sulphides, n.o.s.
	1557
	6.1
	6.1
	66

	905
	ARSENIC COMPOUND, SOLID, N.O.S., inorganic, including: Arsenates, n.o.s.; Arsenites, n.o.s.; and Arsenic sulphides, n.o.s.
	1557
	6.1
	6.1
	60

	906
	ARSENIC COMPOUND, SOLID, N.O.S., inorganic, including: Arsenates, n.o.s.; Arsenites, n.o.s.; and Arsenic sulphides, n.o.s.
	1557
	6.1
	6.1
	60

	907
	ARSENIC
	1558
	6.1
	6.1
	60

	908
	ARSENIC PENTOXIDE
	1559
	6.1
	6.1
	60

	909
	ARSENIC TRICHLORIDE
	1560
	6.1
	6.1
	66

	910
	ARSENIC TRIOXIDE
	1561
	6.1
	6.1
	60

	911
	ARSENICAL DUST
	1562
	6.1
	6.1
	60

	912
	BARIUM COMPOUND, N.O.S.
	1564
	6.1
	6.1
	60

	913
	BARIUM COMPOUND, N.O.S.
	1564
	6.1
	6.1
	60

	914
	BARIUM CYANIDE
	1565
	6.1
	6.1
	66

	915
	BERYLLIUM COMPOUND, N.O.S.
	1566
	6.1
	6.1
	60

	916
	BERYLLIUM COMPOUND, N.O.S.
	1566
	6.1
	6.1
	60

	917
	BERYLLIUM POWDER
	1567
	6.1
	6.1

+4.1
	64

	918
	BROMOACETONE
	1569
	6.1
	6.1

+3
	63

	919
	BRUCINE
	1570
	6.1
	6.1
	66

	920
	BARIUM AZIDE, WETTED with not less than 50% water, by mass
	1571
	4.1
	4.1

+6.1
	

	921
	CACODYLIC ACID
	1572
	6.1
	6.1
	60

	922
	CALCIUM ARSENATE
	1573
	6.1
	6.1
	60

	923
	CALCIUM ARSENATE AND CALCIUM ARSENITE MIXTURE, SOLID
	1574
	6.1
	6.1
	60

	924
	CALCIUM CYANIDE
	1575
	6.1
	6.1
	66

	925
	CHLORODINITRO-BENZENES, LIQUID
	1577
	6.1
	6.1
	60

	926
	CHLORONITROBENZENES, SOLID
	1578
	6.1
	6.1
	60

	927
	4-CHLORO-o-TOLUIDINE
	1579
	6.1
	6.1
	60

	
	HYDROCHLORIDE, SOLID
	
	
	
	

	928
	CHLOROPICRIN
	1580
	6.1
	6.1
	66

	929
	CHLOROPICRIN AND METHYL BROMIDE MIXTURE with more than 2% chloropicrin
	1581
	2
	2.3
	26

	930
	CHLOROPICRIN AND METHYL CHLORIDE MIXTURE
	1582
	2
	2.3
	26

	931
	CHLOROPICRIN MIXTURE, N.O.S.
	1583
	6.1
	6.1
	66

	932
	CHLOROPICRIN MIXTURE, N.O.S.
	1583
	6.1
	6.1
	60

	933
	CHLOROPICRIN MIXTURE, N.O.S.
	1583
	6.1
	6.1
	60

	934
	COPPER ACETOARSENITE
	1585
	6.1
	6.1
	60

	935
	COPPER ARSENITE
	1586
	6.1
	6.1
	60

	936
	COPPER CYANIDE
	1587
	6.1
	6.1
	60

	937
	CYANIDES, INORGANIC, SOLID, N.O.S.
	1588
	6.1
	6.1
	66

	938
	CYANIDES, INORGANIC, SOLID, N.O.S.
	1588
	6.1
	6.1
	60

	939
	CYANIDES, INORGANIC, SOLID, N.O.S.
	1588
	6.1
	6.1
	60

	940
	CYANIDES, INORGANIC, SOLID, N.O.S.
	1589
	2
	2.3

+8
	

	941
	DICHLOROANILINES, LIQUID
	1590
	6.1
	6.1
	60

	942
	o-DICHLOROBENZENE
	1591
	6.1
	6.1
	60

	943
	DICHLOROMETHANE
	1593
	6.1
	6.1
	60

	944
	DIETHYL SULPHATE
	1594
	6.1
	6.1
	60

	945
	DIMETHYL SULPHATE
	1595
	6.1
	6.1+8
	668

	946
	DINITROANILINES
	1596
	6.1
	6.1
	60

	947
	DINITROBENZENES, LIQUID
	1597
	6.1
	6.1
	60

	948
	DINITROBENZENES, LIQUID
	1597
	6.1
	6.1
	60

	949
	DINITRO-o-CRESOL
	1598
	6.1
	6.1
	60

	950
	DINITROPHENOL SOLUTION
	1599
	6.1
	6.1
	60

	951
	DINITROPHENOL SOLUTION
	1599
	6.1
	6.1
	60

	952
	DINITROTOLUENES, MOLTEN
	1600
	6.1
	6.1
	60

	953
	DISINFECTANT, SOLID, TOXIC, N.O.S.
	1601
	6.1
	6.1
	66

	954
	DISINFECTANT, SOLID, TOXIC, N.O.S.
	1601
	6.1
	6.1
	60

	955
	DISINFECTANT, SOLID, TOXIC, N.O.S.
	1601
	6.1
	6.1
	60

	956
	DYE, LIQUID, TOXIC, N.O.S. or DYE INTERMEDIATE, LIQUID, TOXIC, N.O.S.
	1602
	6.1
	6.1
	66

	957
	DYE, LIQUID, TOXIC, N.O.S. or DYE INTERMEDIATE, LIQUID, TOXIC, N.O.S.
	1602
	6.1
	6.1
	60

	958
	DYE, LIQUID, TOXIC, N.O.S. or DYE INTERMEDIATE, LIQUID, TOXIC, N.O.S.
	1602
	6.1
	6.1
	60

	959
	ETHYL BROMOACETATE
	1603
	6.1
	6.1

+3
	63

	960
	ETHYLENEDIAMINE
	1604
	8
	8

+3
	83

	961
	ETHYLENE DIBROMIDE
	1605
	6.1
	6.1
	66

	962
	FERRIC ARSENATE
	1606
	6.1
	6.1
	60

	963
	FERRIC ARSENITE
	1607
	6.1
	6.1
	60

	964
	FERROUS ARSENATE
	1608
	6.1
	6.1
	60

	965
	HEXAETHYL TETRAPHOSPHATE
	1611
	6.1
	6.1
	60

	966
	HEXAETHYL TETRAPHOSPHATE AND COMPRESSED GAS MIXTURE
	1612
	2
	2.3
	26

	967
	HYDROCYANIC ACID, AQUEOUS SOLUTION (HYDROGEN CYANIDE, AQUEOUS SOLUTION) with not more than 20% hydrogen cyanide
	1613
	6.1
	6.1

+3
	663

	968
	HYDROGEN CYANIDE, STABILIZED, containing less than 3% water and absorbed in a porous inert material
	1614
	6.1
	6.1

+3
	

	969
	LEAD ACETATE
	1616
	6.1
	6.1
	60

	970
	LEAD ARSENATES
	1617
	6.1
	6.1
	60

	971
	LEAD ARSENITES
	1618
	6.1
	6.1
	60

	972
	LEAD CYANIDE
	1620
	6.1
	6.1
	60

	973
	LONDON PURPLE
	1621
	6.1
	6.1
	60

	974
	MAGNESIUM ARSENATE
	1622
	6.1
	6.1
	60

	975
	MERCURIC ARSENATE
	1623
	6.1
	6.1
	60

	976
	MERCURIC CHLORIDE
	1624
	6.1
	6.1
	60

	977
	MERCURIC NITRATE
	1625
	6.1
	6.1
	60

	978
	MERCURIC POTASSIUM CYANIDE
	1626
	6.1
	6.1
	66

	979
	MERCUROUS NITRATE
	1627
	6.1
	6.1
	60

	980
	MERCURY ACETATE
	1629
	6.1
	6.1
	60

	981
	MERCURY AMMONIUM CHLORIDE
	1630
	6.1
	6.1
	60

	982
	MERCURY BENZOATE
	1631
	6.1
	6.1
	60

	983
	MERCURY BROMIDES
	1634
	6.1
	6.1
	60

	984
	MERCURY CYANIDE
	1636
	6.1
	6.1
	60

	985
	MERCURY GLUCONATE
	1637
	6.1
	6.1
	60

	986
	MERCURY IODIDE
	1638
	6.1
	6.1
	60

	987
	MERCURY NUCLEATE
	1639
	6.1
	6.1
	60

	988
	MERCURY OLEATE
	1640
	6.1
	6.1
	60

	989
	MERCURY OXIDE
	1641
	6.1
	6.1
	60

	990
	MERCURY OXYCYANIDE, DESENSITIZED
	1642
	6.1
	6.1
	60

	991
	MERCURY POTASSIUM IODIDE
	1643
	6.1
	6.1
	60

	992
	MERCURY SALICYLATE
	1644
	6.1
	6.1
	60

	993
	MERCURY SULPHATE
	1645
	6.1
	6.1
	60

	994
	MERCURY THIOCYANATE
	1646
	6.1
	6.1
	60

	995
	METHYL BROMIDE AND ETHYLENE DIBROMIDE MIXTURE, LIQUID
	1647
	6.1
	6.1
	66

	996
	ACETONITRILE
	1648
	3
	3
	33

	997
	MOTOR FUEL ANTI-KNOCK MIXTURE
	1649
	6.1
	6.1
	66

	998
	beta-NAPHTHYLAMINE, SOLID
	1650
	6.1
	6.1
	60

	999
	NAPHTHYLTHIOUREA
	1651
	6.1
	6.1
	60

	1000
	NAPHTHYLUREA
	1652
	6.1
	6.1
	60

	1001
	NICKEL CYANIDE
	1653
	6.1
	6.1
	60

	1002
	NICOTINE
	1654
	6.1
	6.1
	60

	1003
	NICOTINE COMPOUND, SOLID, N.O.S. or NICOTINE PREPARATION, SOLID, N.O.S.
	1655
	6.1
	6.1
	66

	1004
	NICOTINE COMPOUND, SOLID, N.O.S. or NICOTINE

PREPARATION, SOLID, N.O.S.
	1655
	6.1
	6.1
	60

	1005
	NICOTINE COMPOUND, SOLID, N.O.S. or NICOTINE PREPARATION, SOLID, N.O.S.
	1655
	6.1
	6.1
	60

	1006
	NICOTINE HYDROCHLORIDE, LIQUID or SOLUTION
	1656
	6.1
	6.1
	60

	1007
	NICOTINE HYDROCHLORIDE, LIQUID or SOLUTION
	1656
	6.1
	6.1
	60

	1008
	NICOTINE SALICYLATE
	1657
	6.1
	6.1
	60

	1009
	NICOTINE SULPHATE, SOLUTION
	1658
	6.1
	6.1
	60

	1010
	NICOTINE SULPHATE, SOLUTION
	1658
	6.1
	6.1
	60

	1011
	NICOTINE TARTRATE
	1659
	6.1
	6.1
	60

	1012
	NITRIC OXIDE, COMPRESSED
	1660
	2
	2.3

+5.1 

+8
	

	1013
	NITROANILINES (o-, m-, p-)
	1661
	6.1
	6.1
	60

	1014
	NITROBENZENE
	1662
	6.1
	6.1
	60

	1015
	NITROPHENOLS (o-, m-, p-)
	1663
	6.1
	6.1
	60

	1016
	NITROTOLUENES, LIQUID
	1664
	6.1
	6.1
	60

	1017
	NITROXYLENES, LIQUID
	1665
	6.1
	6.1
	60

	1018
	PENTACHLOROETHANE
	1669
	6.1
	6.1
	60

	1019
	PERCHLOROMETHYL MERCAPTAN
	1670
	6.1
	6.1
	66

	1020
	PHENOL, SOLID
	1671
	6.1
	6.1
	60

	1021
	PHENYLCARBYLAMINE CHLORIDE
	1672
	6.1
	6.1
	66

	1022
	PHENYLENEDIAMINES (o-, m-, p-)
	1673
	6.1
	6.1
	60

	1023
	PHENYLMERCURIC ACETATE
	1674
	6.1
	6.1
	60

	1024
	POTASSIUM ARSENATE
	1677
	6.1
	6.1
	60

	1025
	POTASSIUM ARSENITE
	1678
	6.1
	6.1
	60

	1026
	POTASSIUM CUPROCYANIDE
	1679
	6.1
	6.1
	60

	1027
	POTASSIUM CYANIDE, SOLID
	1680
	6.1
	6.1
	66

	1028
	SILVER ARSENITE
	1683
	6.1
	6.1
	60

	1029
	SILVER CYANIDE
	1684
	6.1
	6.1
	60

	1030
	SODIUM ARSENATE
	1685
	6.1
	6.1
	60

	1031
	SODIUM ARSENITE, AQUEOUS SOLUTION
	1686
	6.1
	6.1
	60

	1032
	SODIUM ARSENITE, AQUEOUS SOLUTION
	1686
	6.1
	6.1
	60

	1033
	SODIUM AZIDE
	1687
	6.1
	6.1
	

	1034
	SODIUM CACODYLATE
	1688
	6.1
	6.1
	60

	1035
	SODIUM CYANIDE, SOLID
	1689
	6.1
	6.1
	66

	1036
	SODIUM FLUORIDE, SOLID
	1690
	6.1
	6.1
	60

	1037
	STRONTIUM ARSENITE
	1691
	6.1
	6.1
	60

	1038
	STRYCHNINE or STRYCHNINE SALTS
	1692
	6.1
	6.1
	66

	1039
	TEAR GAS SUBSTANCE, LIQUID, N.O.S.
	1693
	6.1
	6.1
	66

	1040
	TEAR GAS SUBSTANCE, LIQUID, N.O.S.
	1693
	6.1
	6.1
	60

	1041
	BROMOBENZYL CYANIDES, LIQUID
	1694
	6.1
	6.1
	66

	1042
	CHLOROACETONE, STABILIZED
	1695
	6.1
	6.1

+3

+8
	663

	1043
	CHLOROACETOPHENONE, SOLID
	1697
	6.1
	6.1
	60

	1044
	DIPHENYLAMINE CHLOROARSINE
	1698
	6.1
	6.1
	66

	1045
	DIPHENYLCHLORO-ARSINE, LIQUID
	1699
	6.1
	6.1
	66

	1046
	TEAR GAS CANDLES
	1700
	6.1
	6.1

+4.1
	

	1047
	XYLYL BROMIDE, LIQUID
	1701
	6.1
	6.1
	60

	1048
	1,1,2,2-TETRACHLOROETHANE
	1702
	6.1
	6.1
	60

	1049
	TETRAETHYL DITHIOPYROPHOSPHATE
	1704
	6.1
	6.1
	60

	1050
	THALLIUM COMPOUND, N.O.S.
	1707
	6.1
	6.1
	60

	1051
	TOLUIDINES, LIQUID
	1708
	6.1
	6.1
	60

	1052
	2,4-TOLUYLENEDIAMINE, SOLID
	1709
	6.1
	6.1
	60

	1053
	TRICHLOROETHYLENE
	1710
	6.1
	6.1
	60

	1054
	XYLIDINES, LIQUID
	1711
	6.1
	6.1
	60

	1055
	ZINC ARSENATE, ZINC ARSENITE or ZINC ARSENATE AND ZINC ARSENITE MIXTURE
	1712
	6.1
	6.1
	60

	1056
	ZINC CYANIDE
	1713
	6.1
	6.1
	66

	1057
	ZINC PHOSPHIDE
	1714
	4.3
	4.3

+6.1
	

	1058
	ACETIC ANHYDRIDE
	1715
	8
	8

+3
	83

	1059
	ACETYL BROMIDE
	1716
	8
	8
	80

	1060
	ACETYL CHLORIDE
	1717
	3
	3

+8
	X338

	1061
	BUTYL ACID PHOSPHATE
	1718
	8
	8
	80

	1062
	CAUSTIC ALKALI LIQUID, N.O.S.
	1719
	8
	8
	80

	1063
	CAUSTIC ALKALI LIQUID, N.O.S.
	1719
	8
	8
	80

	1064
	ALLYL CHLOROFORMATE
	1722
	6.1
	6.1

+3

+8
	668

	1065
	ALLYL IODIDE
	1723
	3
	3 +8
	338

	1066
	ALLYLTRICHLOROSILANE, STABILIZED
	1724
	8
	8 

+3
	X839

	1067
	ALUMINIUM BROMIDE, ANHYDROUS
	1725
	8
	8
	80

	1068
	ALUMINIUM CHLORIDE, ANHYDROUS
	1726
	8
	8
	80

	1069
	AMMONIUM HYDROGENDIFLUORIDE, SOLID
	1727
	8
	8
	80

	1070
	AMYLTRICHLOROSILANE
	1728
	8
	8
	X80

	1071
	ANISOYL CHLORIDE
	1729
	8
	8
	80

	1072
	ANTIMONY PENTACHLORIDE, LIQUID
	1730
	8
	8
	X80

	1073
	ANTIMONY PENTACHLORIDE SOLUTION
	1731
	8
	8
	80

	1074
	ANTIMONY PENTACHLORIDE SOLUTION
	1731
	8
	8
	80

	1075
	ANTIMONY PENTAFLUORIDE
	1732
	8
	8

+6.1
	86

	1076
	ANTIMONY TRICHLORIDE
	1733
	8
	8
	80

	1077
	BENZOYL CHLORIDE
	1736
	8
	8
	80

	1078
	BENZYL BROMIDE
	1737
	6.1
	6.1

+8
	68

	1079
	BENZYL CHLORIDE
	1738
	6.1
	6.1

+8
	68

	1080
	BENZYL CHLOROFORMATE
	1739
	8
	8
	88

	1081
	HYDROGENDIFLUORIDES, SOLID, N.O.S.
	1740
	8
	8
	80

	1082
	HYDROGENDIFLUORIDES, SOLID, N.O.S.
	1740
	8
	8
	80

	1083
	BORON TRICHLORIDE
	1741
	2
	2.3

+8
	268

	1084
	BORON TRIFLUORIDE ACETIC ACID COMPLEX, LIQUID
	1742
	8
	8
	80

	1085
	BORON TRIFLUORIDE PROPIONIC ACID COMPLEX, LIQUID
	1743
	8
	8
	80

	1086
	BROMINE or BROMINE SOLUTION
	1744
	8
	8

+6.1
	886

	1087
	BROMINE PENTAFLUORIDE
	1745
	5.1
	5.1

+6.1

+8
	568

	1088
	BROMINE TRIFLUORIDE
	1746
	5.1
	5.1

+6.1

+8
	568

	1089
	BUTYLTRICHLOROSILANE
	1747
	8
	8

+3
	X83

	1090
	CALCIUM HYPOCHLORITE, DRY or CALCIUM HYPOCHLORITE MIXTURE, DRY with more than 39% available chlorine (8.8% available oxygen)
	1748
	5.1
	5.1
	50

	1091
	CALCIUM HYPOCHLORITE, DRY or CALCIUM HYPOCHLORITE MIXTURE, DRY with more than 39% available chlorine (8.8% available oxygen)
	1748
	5.1
	5.1
	50

	1092
	CHLORINE TRIFLUORIDE
	1749
	2
	2.3

+5.1

+8
	265

	1093
	CHLOROACETIC ACID SOLUTION
	1750
	6.1
	6.1

+8
	68

	1094
	CHLOROACETIC ACID, SOLID
	1751
	6.1
	6.1

+8
	68

	1095
	CHLOROACETYL CHLORIDE
	1752
	6.1
	6.1

+8
	668

	1096
	CHLOROPHENYL​ - TRICHLOROSILANE
	1753
	8
	8
	X80

	1097
	CHLOROSULPHONIC ACID (with or without sulphur trioxide)
	1754
	8
	8
	X88

	1098
	CHROMIC ACID SOLUTION
	1755
	8
	8
	80

	1099
	CHROMIC ACID SOLUTION
	1755
	8
	8
	80

	1100
	CHROMIC FLUORIDE, SOLID
	1756
	8
	8
	80

	1101
	CHROMIC FLUORIDE SOLUTION
	1757
	8
	8
	80

	1102
	CHROMIC FLUORIDE SOLUTION
	1757
	8
	8
	80

	1103
	CHROMIUM OXYCHLORIDE
	1758
	8
	8
	X88

	1104
	CORROSIVE SOLID, N.O.S.
	1759
	8
	8
	88

	1105
	CORROSIVE SOLID, N.O.S.
	1759
	8
	8
	80

	1106
	CORROSIVE SOLID, N.O.S.
	1759
	8
	8
	80

	1107
	CORROSIVE LIQUID, N.O.S.
	1760
	8
	8
	88

	1108
	CORROSIVE LIQUID, N.O.S.
	1760
	8
	8
	80

	1109
	CORROSIVE LIQUID, N.O.S.
	1760
	8
	8
	80

	1110
	CUPRIETHYLENEDIAMINE SOLUTION
	1761
	8
	8

+6.1
	86

	1111
	CUPRIETHYLENEDIAMINE SOLUTION
	1761
	8
	8

+6.1
	86

	1112
	CYCLOHEXENYLTRICHLORO-SILANE
	1762
	8
	8
	X80

	1113
	CYCLOHEXENYLTRICHLORO-SILANE
	1763
	8
	8
	X80

	1114
	DICHLOROACETIC ACID
	1764
	8
	8
	80

	1115
	DICHLOROACETYL CHLORIDE
	1765
	8
	8
	X80

	1116
	DICHLOROPHENYL- TRICHLOROSILANE
	1766
	8
	8
	X80

	1117
	DIETHYLDICHLORO-SILANE
	1767
	8
	8

+3
	X83

	1118
	DIFLUOROPHOSPHORIC ACID, ANHYDROUS
	1768
	8
	8
	80

	1119
	DIPHENYLDICHLORO-SILANE
	1769
	8
	8
	X80

	1120
	DIPHENYLMETHYL BROMIDE
	1770
	8
	8
	80

	1121
	DODECYLTRICHLORO-SILANE
	1771
	8
	8
	X80

	1122
	FERRIC CHLORIDE, ANHYDROUS
	1773
	8
	8
	80

	1123
	FIRE EXTINGUISHER CHARGES, corrosive liquid
	1774
	8
	8
	

	1124
	FLUOROBORIC ACID
	1775
	8
	8
	80

	1125
	FLUOROPHOSPHORIC ACID, ANHYDROUS
	1776
	8
	8
	80

	1126
	FLUOROSULPHONIC ACID
	1777
	8
	8
	88

	1127
	FLUOROSILICIC ACID
	1778
	8
	8
	80

	1128
	FORMIC ACID with more than 85% acid by mass
	1779
	8
	8

+3
	83

	1129
	FUMARYL CHLORIDE
	1780
	8
	8
	80

	1130
	HEXADECYLTRICHLORO​ SILANE
	1781
	8
	8
	X80

	1131
	HEXAFLUORO-PHOSPHORIC ACID
	1782
	8
	8
	80

	1132
	HEXAMETHYLENE-DIAMINE SOLUTION
	1783
	8
	8
	80

	1133
	HEXAM ETHYLENE-DIAMINE SOLUTION
	1783
	8
	8
	80

	1134
	HEXYLTRICHLOROSILANE
	1784
	8
	8
	X80

	1135
	HYDROFLUORIC ACID AND SULPHURIC ACID MIXTURE
	1786
	8
	8

+6.1
	886

	1136
	HYDRIODIC ACID
	1787
	8
	8
	80

	1137
	HYDRIODIC ACID
	1787
	8
	8
	80

	1138
	HYDROBROMIC ACID
	1788
	8
	8
	80

	1139
	HYDROBROMIC ACID
	1788
	8
	8
	80

	1140
	HYDROCHLORIC ACID
	1789
	8
	8
	80

	1141
	HYDROCHLORIC ACID
	1789
	8
	8
	80

	1142
	HYDROFLUORIC ACID with more than 85% hydrogen fluoride
	1790
	8
	8

+6.1
	886

	1143
	HYDROFLUORIC ACID with more than 60% but not more than 85% hydrogen fluoride
	1790
	8
	8

+6.1
	886

	1144
	HYDROFLUORIC ACID with not more than 60% hydrogen fluoride
	1790
	8
	8

+6.1
	86

	1145
	HYPOCHLORITE SOLUTION
	1791
	8
	8
	80

	1146
	HYPOCHLORITE SOLUTION
	1791
	8
	8
	80

	1147
	IODINE MONOCHLORIDE, SOLID
	1792
	8
	8
	80

	1148
	ISOPROPYL ACID PHOSPHATE
	1793
	8
	8
	80

	1149
	LEAD SULPHATE with more than 3% free acid
	1794
	8
	8
	80

	1150
	NITRATING ACID MIXTURE with more than 50% nitric acid
	1796
	8
	8+5.1
	885

	1151
	NITRATING ACID MIXTURE with not more than 50% nitric acid
	1796
	8
	8
	80

	1152
	NITROHYDROCHLORIC ACID
	1798
	8
	
	

	1153
	NONYLTRICHLOROSILANE
	1799
	8
	8
	X80

	1154
	OCTADECYLTRICHLORO- SILANE
	1800
	8
	8
	X80

	1155
	OCTYLTRICHLOROSILANE
	1801
	8
	8
	X80

	1156
	PERCHLORIC ACID with not more than 50% acid, by mass
	1802
	8
	8

+5.1
	85

	1157
	PHENOLSULPHONIC ACID, LIQUID
	1803
	8
	8
	80

	1158
	PHENYLTRICHLORO-SILANE
	1804
	8
	8
	X80

	1159
	PHOSPHORIC ACID, SOLUTION
	1805
	8
	8
	80

	1160
	PHOSPHORUS PENTACHLORIDE
	1806
	8
	8
	80

	1161
	PHOSPHORUS PENTOXIDE
	1807
	8
	8
	80

	1162
	PHOSPHORUS TRIBROMIDE
	1808
	8
	8
	X80

	1163
	PHOSPHORUS TRICHLORIDE
	1809
	6.1
	6.1

+8
	668

	1164
	PHOSPHORUS OXYCHLORIDE
	1810
	6.1
	6.1

+8
	X668

	1165
	POTASSIUM HYDROGENDIFLUORIDE, SOLID
	1811
	8
	8

+6.1
	86

	1166
	POTASSIUM FLUORIDE, SOLID
	1812
	6.1
	6.1
	60

	1167
	POTASSIUM HYDROXIDE, SOLID
	1813
	8
	8
	80

	1168
	POTASSIUM HYDROXIDE SOLUTION
	1814
	8
	8
	80

	1169
	POTASSIUM HYDROXIDE SOLUTION
	1814
	8
	8
	80

	1170
	PROPIONYL CHLORIDE
	1815
	3
	3

+8
	338

	1171
	PROPYLTRICHLORO-SILANE
	1816
	8
	8

+3
	X83

	1172
	PYROSULPHURYL CHLORIDE
	1817
	8
	8
	X80

	1173
	SILICON TETRACHLORIDE
	1818
	8
	8
	X80

	1174
	SODIUM ALUMINATE SOLUTION
	1819
	8
	8
	80

	1175
	SODIUM ALUMINATE SOLUTION
	1819
	8
	8
	80

	1176
	SODIUM HYDROXIDE, SOLID
	1823
	8
	8
	80

	1177
	SODIUM HYDROXIDE SOLUTION
	1824
	8
	8
	80

	1178
	SODIUM HYDROXIDE SOLUTION
	1824
	8
	8
	80

	1179
	SODIUM MONOXIDE
	1825
	8
	8
	80

	1180
	NITRATING ACID MIXTURE, SPENT, with more than 50% nitric acid
	1826
	8
	8

+5.1
	885

	1181
	NITRATING ACID MIXTURE, SPENT, with not more than 50% nitric acid
	1826
	8
	8
	80

	1182
	STANNIC CHLORIDE, ANHYDROUS
	1827
	8
	8
	X80

	1183
	SULPHUR CHLORIDES
	1828
	8
	8
	X88

	1184
	SULPHUR TRIOXIDE, STABILIZED
	1829
	8
	8
	X88

	1185
	SULPHURIC ACID with more than 51% acid
	1830
	8
	8
	80

	1186
	SULPHURIC ACID, FUMING
	1831
	8
	8

+6.1
	X886

	1187
	SULPHURIC ACID, SPENT
	1832
	8
	8
	80

	1188
	SULPHUROUS ACID
	1833
	8
	8
	80

	1189
	SULPHURYL CHLORIDE
	1834
	6.1
	6.1

+8
	X668

	1190
	TETRAMETHYL-AMMONIUM HYDROXIDE SOLUTION
	1835
	8
	8
	80

	1191
	TETRAMETHYL-AMMONIUM HYDROXIDE SOLUTION
	1835
	8
	8
	80

	1192
	THIONYL CHLORIDE
	1836
	8
	8
	X88

	1193
	THIOPHOSPHORYL CHLORIDE
	1837
	8
	8
	X80

	1194
	TITANIUM TETRACHLORIDE
	1838
	6.1
	6.1

+8
	X668

	1195
	TRICHLOROACETIC ACID
	1839
	8
	8
	80

	1196
	ZINC CHLORIDE SOLUTION
	1840
	8
	8
	80

	1197
	ACETALDEHYDE AMMONIA
	1841
	9
	9
	90

	1198
	AMMONIUM DINITRO-o- CRESOLATE, SOLID
	1843
	6.1
	6.1
	60

	1199
	Carbon dioxide, solid (Dry ice)
	1845
	9
	
	

	1200
	CARBON TETRACHLORIDE
	1846
	6.1
	6.1
	60

	1201
	POTASSIUM SULPHIDE, HYDRATED with not less than 30% water of crystallization
	1847
	8
	8
	80

	1202
	PROPIONIC ACID with not less than 10% and less than 90% acid by mass
	1848
	8
	8
	80

	1203
	SODIUM SULPHIDE, HYDRATED with not less than 30% water
	1849
	8
	8
	80

	1204
	MEDICINE, LIQUID, TOXIC, N.O.S.
	1851
	6.1
	6.1
	60

	1205
	MEDICINE, LIQUID, TOXIC, N.O.S.
	1851
	6.1
	6.1
	60

	1206
	BARIUM ALLOYS, PYROPHORIC
	1854
	4.2
	4.2
	43

	1207
	CALCIUM, PYROPHORIC or CALCIUM ALLOYS, PYROPHORIC
	1855
	4.2
	4.2
	

	1208
	Rags, oily
	1856
	4.2
	
	

	1209
	Textile waste, wet
	1857
	4.2
	
	

	1210
	HEXAFLUOROPROPYLENE (REFRIGERANT GAS R 1216)
	1858
	2
	2.2
	20

	1211
	SILICON TETRAFLUORIDE
	1859
	2
	2.3

+8
	268

	1212
	VINYL FLUORIDE, STABILIZED
	1860
	2
	2.1
	239

	1213
	ETHYL CROTONATE
	1862
	3
	3
	33

	1214
	FUEL, AVIATION, TURBINE ENGINE
	1863
	3
	3
	33

	1215
	FUEL, AVIATION, TURBINE ENGINE (vapour pressure at 50 °C more than 110 kPa)
	1863
	3
	3
	33

	1216
	FUEL, AVIATION, TURBINE ENGINE (vapour pressure at50 °C not more than 110 kPa)
	1863
	3
	3
	33

	1217
	FUEL, AVIATION, TURBINE ENGINE
	1863
	3
	3
	30

	1218
	n-PROPYL NITRATE
	1865
	3
	3
	

	1219
	RESIN SOLUTION, flammable
	1866
	3
	3
	33

	1220
	RESIN SOLUTION, flammable (vapour pressure at 50 °C more than 110 kPa)
	1866
	3
	3
	33

	1221
	RESIN SOLUTION, flammable (vapour pressure at 50 °C not more than 110 kPa)
	1866
	3
	3
	33

	1222
	RESIN SOLUTION, flammable
	1866
	3
	3
	30

	1223
	RESIN SOLUTION, flammable (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1866
	3
	3
	

	1224
	RESIN SOLUTION, flammable (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1866
	3
	3
	

	1225
	DECABORANE
	1868
	4.1
	4.1

+6.1
	46

	1226
	MAGNESIUM or MAGNESIUM ALLOYS with more than 50% magnesium in pellets, turnings or ribbons
	1869
	4.1
	4.1
	40

	1227
	POTASSIUM BOROHYDRIDE
	1870
	4.3
	4.3
	

	1228
	TITANIUM HYDRIDE
	1871
	4.1
	4.1
	40

	1229
	LEAD DIOXIDE
	1872
	5.1
	5.1

+6.1
	56

	1230
	PERCHLORIC ACID with more than 50% but not more than 72% acid, by mass
	1873
	5.1
	5.1

+8
	558

	1231
	BARIUM OXIDE
	1884
	6.1
	6.1
	60

	1232
	BENZIDINE
	1885
	6.1
	6.1
	60

	1233
	BENZYLIDENE CHLORIDE
	1886
	6.1
	6.1
	60

	1234
	BROMOCHLOROMETHANE
	1887
	6.1
	6.1
	60

	1235
	CHLOROFORM
	1888
	6.1
	6.1
	60

	1236
	CYANOGEN BROMIDE
	1889
	6.1
	6.1

+8
	668

	1237
	ETHYL BROMIDE
	1891
	6.1
	6.1
	60

	1238
	ETHYLDICHLOROARSINE
	1892
	6.1
	6.1
	66

	1239
	PHENYLMERCURIC
	1894
	6.1
	6.1
	60

	
	HYDROXIDE
	
	
	
	

	1240
	PHENYLMERCURIC NITRATE
	1895
	6.1
	6.1
	60

	1241
	TETRACHLOROETHYLENE
	1897
	6.1
	6.1
	60

	1242
	ACETYL IODIDE
	1898
	8
	8
	80

	1243
	DIISOOCTYL ACID PHOSPHATE
	1902
	8
	8
	80

	1244
	DISINFECTANT, LIQUID, CORROSIVE, N.O.S.
	1903
	8
	8
	88

	1245
	DISINFECTANT, LIQUID, CORROSIVE, N.O.S.
	1903
	8
	8
	80

	1246
	DISINFECTANT, LIQUID, CORROSIVE, N.O.S.
	1903
	8
	8
	80

	1247
	SELENIC ACID
	1905
	8
	8
	88

	1248
	SLUDGE ACID
	1906
	8
	8
	80

	1249
	SODA LIME with more than 4% sodium hydroxide
	1907
	8
	8
	80

	1250
	CHLORITE SOLUTION
	1908
	8
	8
	80

	1251
	CHLORITE SOLUTION
	1908
	8
	8
	80

	1252
	Calcium oxide
	1910
	8
	
	

	1253
	DIBORANE
	1911
	2
	2.3 

+2.1
	

	1254
	METHYL CHLORIDE AND METHYLENE CHLORIDE MIXTURE
	1912
	2
	2.1
	23

	1255
	NEON, REFRIGERATED LIQUID
	1913
	2
	2.2
	22

	1256
	BUTYL PROPIONATES
	1914
	3
	3
	30

	1257
	CYCLOHEXANONE
	1915
	3
	3
	30

	1258
	2,2'-DICHLORODIETHYL ETHER
	1916
	6.1
	6.1

+3
	63

	1259
	ETHYL ACRYLATE, STABILIZED
	1917
	3
	3
	339

	1260
	ISOPROPYLBENZENE
	1918
	3
	3
	30

	1261
	METHYL ACRYLATE, STABILIZED
	1919
	3
	3
	339

	1262
	NONANES
	1920
	3
	3
	30

	1263
	PROPYLENEIMINE, STABILIZED
	1921
	3
	3

+6.1
	336

	1264
	PYRROLIDINE
	1922
	3
	3

+8
	338

	1265
	CALCIUM DITHIONITE (CALCIUM HYDROSULPHITE)
	1923
	4.2
	4.2
	40

	1266
	METHYL MAGNESIUM BROMIDE IN ETHYL ETHER
	1928
	4.3
	4.3

+3
	X323

	1267
	POTASSIUM DITHIONITE (POTASSIUM HYDROSULPHITE)
	1929
	4.2
	4.2
	40

	1268
	ZINC DITHIONITE (ZINC HYDROSULPHITE)
	1931
	9
	9
	90

	1269
	ZIRCONIUM SCRAP
	1932
	4.2
	4.2
	40

	1270
	CYANIDE SOLUTION, N.O.S.
	1935
	6.1
	6.1
	66

	1271
	CYANIDE SOLUTION, N.O.S.
	1935
	6.1
	6.1
	60

	1272
	CYANIDE SOLUTION, N.O.S.
	1935
	6.1
	6.1
	60

	1273
	BROMOACETIC ACID SOLUTION
	1938
	8
	8
	80

	1274
	BROMOACETIC ACID SOLUTION
	1938
	8
	8
	80

	1275
	PHOSPHORUS OXYBROMIDE
	1939
	8
	8
	80

	1276
	THIOGLYCOLIC ACID
	1940
	8
	8
	80

	1277
	DIBROMODIFLUORO-METHANE
	1941
	9
	9
	90

	1278
	AMMONIUM NITRATE with not more than 0.2% combustible substances, including any organic substance calculated as carbon, to the exclusion of any other added substance
	1942
	5.1
	5.1
	50

	1279
	MATCHES, SAFETY (book, card or strike on box)
	1944
	4.1
	4.1
	

	1280
	MATCHES, WAX ‘VESTA’
	1945
	4.1
	4.1
	

	1281
	AEROSOLS, asphyxiant
	1950
	2
	2.2
	

	1282
	AEROSOLS, corrosive
	1950
	2
	2.2

+8
	

	1283
	AEROSOLS, corrosive, oxidizing
	1950
	2
	2.2

+5.1

+8
	

	1284
	AEROSOLS, flammable
	1950
	2
	2.1
	

	1285
	AEROSOLS, flammable, corrosive
	1950
	2
	2.1

+8
	

	1286
	AEROSOLS, oxidizing
	1950
	2
	2.2

+5.1
	

	1287
	AEROSOLS, toxic
	1950
	2
	2.2

+6.1
	

	1288
	AEROSOLS, toxic, corrosive
	1950
	2
	2.2

+6.1

+8
	

	1289
	AEROSOLS, toxic, flammable
	1950
	2
	2.1

+6.1
	

	1290
	AEROSOLS, toxic, flammable, corrosive
	1950
	2
	2.1 

+6.1

+8
	

	1291
	AEROSOLS, toxic, oxidizing
	1950
	2
	2.2

+5.1

+6.1
	

	1292
	AEROSOLS, toxic, oxidizing, corrosive
	1950
	2
	2.2

+5.1

+6.1 

+8
	

	1293
	ARGON, REFRIGERATED LIQUID
	1951
	2
	2.2
	22

	1294
	ETHYLENE OXIDE AND CARBON DIOXIDE MIXTURE with not more than 9% ethylene oxide
	1952
	2
	2.2
	20

	1295
	COMPRESSED GAS, TOXIC, FLAMMABLE, N.O.S.
	1953
	2
	2.3

+2.1
	263

	1296
	COMPRESSED GAS, FLAMMABLE, N.O.S.
	1954
	2
	2.1
	23

	1297
	COMPRESSED GAS, TOXIC, N.O.S.
	1955
	2
	2.3
	26

	1298
	COMPRESSED GAS, N.O.S.
	1956
	2
	2.2
	20

	1299
	DEUTERIUM, COMPRESSED
	1957
	2
	2.1
	23

	1300
	1.2-DICHLORO-1,1,2,2- TETRAFLUOROETHANE (REFRIGERANT GAS R 114)
	1958
	2
	2.2
	20

	1301
	1.1-DIFLUOROETHYLENE (REFRIGERANT GAS R 1132a)
	1959
	2
	2.1
	239

	1302
	ETHANE, REFRIGERATED LIQUID
	1961
	2
	2.1
	223

	1303
	ETHYLENE
	1962
	2
	2.1
	23

	1304
	HELIUM, REFRIGERATED LIQUID
	1963
	2
	2.2
	22

	1305
	HYDROCARBON GAS MIXTURE, COMPRESSED, N.O.S.
	1964
	2
	2.1
	23

	1306
	HYDROCARBON GAS MIXTURE, LIQUEFIED, N.O.S. such as mixtures A, A01, A02, A0, A1, B1, B2, B or C
	1965
	2
	2.1
	23

	1307
	HYDROGEN, REFRIGERATED LIQUID
	1966
	2
	2.1
	223

	1308
	INSECTICIDE GAS, TOXIC, N.O.S.
	1967
	2
	2.3
	26

	1309
	INSECTICIDE GAS, N.O.S.
	1968
	2
	2.2
	20

	1310
	ISOBUTANE
	1969
	2
	2.1
	23

	1311
	KRYPTON, REFRIGERATED LIQUID
	1970
	2
	2.2
	22

	1312
	METHANE, COMPRESSED or NATURAL GAS, COMPRESSED with high methane content
	1971
	2
	2.1
	23

	1313
	METHANE, REFRIGERATED LIQUID or NATURAL GAS, REFRIGERATED LIQUID with high methane content
	1972
	2
	2.1
	223

	1314
	CHLORODIFLUORO-M ETHANE AND CHLOROPENTAFLUORO​ETHANE MIXTURE with fixed boiling point, with approximately 49% chlorodifluoromethane (REFRIGERANT GAS R 502)
	1973
	2
	2.2
	20

	1315
	CHLORODIFLUOROBROMO- METHANE (REFRIGERANT GAS R12B1)
	1974
	2
	2.2
	20

	1316
	NITRIC OXIDE AND DINITROGEN TETROXIDE MIXTURE (NITRIC OXIDE AND NITROGEN DIOXIDE MIXTURE)
	1975
	2
	2.3

+5.1 

+8
	

	1317
	OCTAFLUOROCYCLO-BUTANE (REFRIGERANT GAS RC 318)
	1976
	2
	2.2
	20

	1318
	NITROGEN, REFRIGERATED LIQUID
	1977
	2
	2.2
	22

	1319
	PROPANE
	1978
	2
	2.1
	23

	1320
	TETRAFLUOROMETHANE (REFRIGERANT GAS R 14)
	1982
	2
	2.2
	20

	1321
	1-CHLORO-2,2,2- TRIFLUOROETHANE (REFRIGERANT GAS R 133a)
	1983
	2
	2.2
	20

	1322
	TRIFLUOROMETHANE (REFRIGERANT GAS R 23)
	1984
	2
	2.2
	20

	1323
	ALCOHOLS, FLAMMABLE, TOXIC, N.O.S.
	1986
	3
	3

+6.1
	336

	1324
	ALCOHOLS, FLAMMABLE, TOXIC, N.O.S.
	1986
	3
	3

+6.1
	336

	1325
	ALCOHOLS, FLAMMABLE, TOXIC, N.O.S.
	1986
	3
	3+6.1
	36

	1326
	ALCOHOLS, N.O.S. (vapour pressure at 50 °C more than 110 kPa)
	1987
	3
	3
	33

	1327
	ALCOHOLS, N.O.S. (vapour pressure at 50 °C not more than 110 kPa)
	1987
	3
	3
	33

	1328
	ALCOHOLS, N.O.S.
	1987
	3
	3
	30

	1329
	ALDEHYDES, FLAMMABLE, TOXIC, N.O.S.
	1988
	3
	3

+6.1
	336

	1330
	ALDEHYDES, FLAMMABLE, TOXIC, N.O.S.
	1988
	3
	3

+6.1
	336

	1331
	ALDEHYDES, FLAMMABLE, TOXIC, N.O.S.
	1988
	3
	3

+6.1
	36

	1332
	ALDEHYDES, N.O.S.
	1989
	3
	3
	33

	1333
	ALDEHYDES, N.O.S. (vapour pressure at 50 °C more than 110 kPa)
	1989
	3
	3
	33

	1334
	ALDEHYDES, N.O.S. (vapour pressure at 50 °C not more than 110 kPa)
	1989
	3
	3
	33

	1335
	ALDEHYDES, N.O.S.
	1989
	3
	3
	30

	1336
	BENZALDEHYDE
	1990
	9
	9
	90

	1337
	CHLOROPRENE, STABILIZED
	1991
	3
	3

+6.1
	336

	1338
	FLAMMABLE LIQUID, TOXIC, N.O.S.
	1992
	3
	3

+6.1
	336

	1339
	FLAMMABLE LIQUID, TOXIC, N.O.S.
	1992
	3
	3

+6.1
	336

	1340
	FLAMMABLE LIQUID, TOXIC, N.O.S.
	1992
	3
	3

+6.1
	36

	1341
	FLAMMABLE LIQUID, N.O.S.
	1993
	3
	3
	33

	1342
	FLAMMABLE LIQUID N.O.S. (vapour pressure at 50 °C more than 110 kPa)
	1993
	3
	3
	33

	1343
	FLAMMABLE LIQUID, N.O.S. (vapour pressure at 50 °C not more than 110 kPa)
	1993
	3
	3
	33

	1344
	FLAMMABLE LIQUID, N.O.S.
	1993
	3
	3
	30

	1345
	FLAMMABLE LIQUID N.O.S. (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1993
	3
	3
	

	1346
	FLAMMABLE LIQUID, N.O.S. (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1993
	3
	3
	

	1347
	IRON PENTACARBONYL
	1994
	6.1
	6.1

+3
	663

	1348
	TARS, LIQUID, including road oils, and cutback bitumens (vapour pressure at 50 °C more than 110 kPa)
	1999
	3
	3
	33

	1349
	TARS, LIQUID, including road oils, and cutback bitumens (vapour pressure at 50 °C not more than 110 kPa)
	1999
	3
	3
	33

	1350
	TARS, LIQUID, including road oils, and cutback bitumens
	1999
	3
	3
	30

	1351
	TARS, LIQUID, including road oils, and cutback bitumens (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C more than 110 kPa)
	1999
	3
	3
	

	1352
	TARS, LIQUID, including road oils, and cutback bitumens (having a flash-point below 23 °C and viscous according to 2.2.3.1.4) (vapour pressure at 50 °C not more than 110 kPa)
	1999
	3
	3
	

	1353
	CELLULOID in block, rods, rolls, sheets, tubes, etc., except scrap
	2000
	4.1
	4.1
	

	1354
	COBALT NAPHTHENATES, POWDER
	2001
	4.1
	4.1
	40

	1355
	CELLULOID, SCRAP
	2002
	4.2
	4.2
	

	1356
	MAGNESIUM DIAMIDE
	2004
	4.2
	4.2
	40

	1357
	PLASTICS, NITROCELLULOSE- BASED, SELF-HEATING, N.O.S.
	2006
	4.2
	4.2
	

	1358
	ZIRCONIUM POWDER, DRY
	2008
	4.2
	4.2
	43

	1359
	ZIRCONIUM POWDER, DRY
	2008
	4.2
	4.2
	40

	1360
	ZIRCONIUM POWDER, DRY
	2008
	4.2
	4.2
	40

	1361
	ZIRCONIUM, DRY, finished sheets, strip or coiled wire
	2009
	4.2
	4.2
	40

	1362
	MAGNESIUM HYDRIDE
	2010
	4.3
	4.3
	

	1363
	MAGNESIUM PHOSPHIDE
	2011
	4.3
	4.3

+6.1
	

	1364
	POTASSIUM PHOSPHIDE
	2012
	4.3
	4.3 +6.1
	

	1365
	STRONTIUM PHOSPHIDE
	2013
	4.3
	4.3

+6.1
	

	1366
	HYDROGEN PEROXIDE, AQUEOUS SOLUTION with not less than 20% but not more than 60% hydrogen peroxide (stabilized as necessary)
	2014
	5.1
	5.1

+8
	58

	1367
	HYDROGEN PEROXIDE, AQUEOUS SOLUTION, STABILIZED with more than 70% hydrogen peroxide
	2015
	5.1
	5.1

+8
	559

	1368
	HYDROGEN PEROXIDE, AQUEOUS SOLUTION, STABILIZED with more than 60% hydrogen peroxide and not more than 70% hydrogen peroxide
	2015
	5.1
	5.1

+8
	559

	1369
	AMMUNITION, TOXIC, NON​EXPLOSIVE without burster or expelling charge, non-fuzed
	2016
	6.1
	6.1
	

	1370
	AMMUNITION, TEAR​PRODUCING, NON-EXPLOSIVE without burster or expelling charge, non-fuzed
	2017
	6.1
	6.1+8
	

	1371
	CHLOROANILINES, SOLID
	2018
	6.1
	6.1
	60

	1372
	CHLOROANILINES, LIQUID
	2019
	6.1
	6.1
	60

	1373
	CHLOROPHENOLS, SOLID
	2020
	6.1
	6.1
	60

	1374
	CHLOROPHENOLS, LIQUID
	2021
	6.1
	6.1
	60

	1375
	CRESYLIC ACID
	2022
	6.1
	6.1

+8
	68

	1376
	EPICHLOROHYDRIN
	2023
	6.1
	6.1

+3
	63

	1377
	MERCURY COMPOUND, LIQUID, N.O.S.
	2024
	6.1
	6.1
	66

	1378
	MERCURY COMPOUND, LIQUID, N.O.S.
	2024
	6.1
	6.1
	60

	1379
	MERCURY COMPOUND, LIQUID, N.O.S.
	2024
	6.1
	6.1
	60

	1380
	MERCURY COMPOUND, SOLID, N.O.S.
	2025
	6.1
	6.1
	66

	1381
	MERCURY COMPOUND, SOLID, N.O.S.
	2025
	6.1
	6.1
	60

	1382
	MERCURY COMPOUND, SOLID, N.O.S.
	2025
	6.1
	6.1
	60

	1383
	PHENYLMERCURIC COMPOUND, N.O.S.
	2026
	6.1
	6.1
	66

	1384
	PHENYLMERCURIC COMPOUND, N.O.S.
	2026
	6.1
	6.1
	60

	1385
	PHENYLMERCURIC COMPOUND, N.O.S.
	2026
	6.1
	6.1
	60

	1386
	SODIUM ARSENITE, SOLID
	2027
	6.1
	6.1
	60

	1387
	BOMBS, SMOKE, NON​EXPLOSIVE with corrosive liquid, without initiating device
	2028
	8
	8
	

	1388
	HYDRAZINE, ANHYDROUS
	2029
	8
	8 

+3
	

	1389
	HYDRAZINE AQUEOUS SOLUTION, with more than 37% hydrazine by mass
	2030
	8
	8

+6.1
	886

	1390
	HYDRAZINE AQUEOUS SOLUTION, with more than 37% hydrazine by mass
	2030
	8
	8

+6.1
	86

	1391
	HYDRAZINE AQUEOUS SOLUTION, with more than 37% hydrazine by mass
	2030
	8
	8

+6.1
	86

	1392
	NITRIC ACID, other than red fuming, with more than 70% nitric acid
	2031
	8
	8

+5.1
	885

	1393
	NITRIC ACID, other than red fuming, with at least 65%, but not more than 70% nitric acid
	2031
	8
	8

+5.1
	85

	1394
	NITRIC ACID, other than red fuming, with less than 65% nitric acid
	2031
	8
	8
	80

	1395
	NITRIC ACID, RED FUMING
	2032
	8
	8

+5.1

+6.1
	856

	1396
	POTASSIUM MONOXIDE
	2033
	8
	8
	80

	1397
	HYDROGEN AND METHANE MIXTURE, COMPRESSED
	2034
	2
	2.1
	23

	1398
	1,1,1-TRIFLUOROETHANE (REFRIGERANT GAS R 143a)
	2035
	2
	2.1
	23

	1399
	XENON
	2036
	2
	2.2
	20

	1400
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.2
	

	1401
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.1
	

	1402
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.2

+5.1
	

	1403
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.3
	

	1404
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.3

+8
	

	1405
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.3

+2.1
	

	1406
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.3

+2.1

+8
	

	1407
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.3

+5.1
	

	1408
	RECEPTACLES, SMALL, CONTAINING GAS (GAS CARTRIDGES) without a release device, non-refillable
	2037
	2
	2.3

+5.1

+8
	

	1409
	DINITROTOLUENES, LIQUID
	2038
	6.1
	6.1
	60

	1410
	2,2-DIMETHYLPROPANE
	2044
	2
	2.1
	23

	1411
	ISOBUTYRALDEHYDE (ISOBUTYL ALDEHYDE)
	2045
	3
	3
	33

	1412
	CYMENES
	2046
	3
	3
	30

	1413
	DICHLOROPROPENES
	2047
	3
	3
	33

	1414
	DICHLOROPROPENES
	2047
	3
	3
	30

	1415
	DICYCLOPENTADIENE
	2048
	3
	3
	30

	1416
	DIETHYLBENZENE
	2049
	3
	3
	30

	1417
	DIISOBUTYLENE, ISOMERIC COMPOUNDS
	2050
	3
	3
	33

	1418
	2-DIMETHYLAMINO- ETHANOL
	2051
	8
	8

+3
	83

	1419
	DIPENTENE
	2052
	3
	3
	30

	1420
	METHYL ISOBUTYL CARBINOL
	2053
	3
	3
	30

	1421
	MORPHOLINE
	2054
	8
	8+3
	883

	1422
	STYRENE MONOMER, STABILIZED
	2055
	3
	3
	39

	1423
	TETRAHYDROFURAN
	2056
	3
	3
	33

	1424
	TRIPROPYLENE
	2057
	3
	3
	33

	1425
	TRIPROPYLENE
	2057
	3
	3
	30

	1426
	VALERALDEHYDE
	2058
	3
	3
	33

	1427
	NITROCELLULOSE SOLUTION, FLAMMABLE with not more than 12.6% nitrogen, by dry mass, and not more than 55% nitrocellulose
	2059
	3
	3
	33

	1428
	NITROCELLULOSE SOLUTION, FLAMMABLE with not more than 12.6% nitrogen, by dry mass, and not more than 55% nitrocellulose (vapour pressure at 50 °C more than 110 kPa)
	2059
	3
	3
	33

	1429
	NITROCELLULOSE SOLUTION, FLAMMABLE with not more than 12.6% nitrogen, by dry mass, and not more than 55% nitrocellulose (vapour pressure at 50 °C not more than 110 kPa)
	2059
	3
	3
	33

	1430
	NITROCELLULOSE SOLUTION, FLAMMABLE with not more than 12.6% nitrogen, by dry mass, and not more than 55% nitrocellulose
	2059
	3
	3
	30

	1431
	AMMONIUM NITRATE BASED FERTILIZER
	2067
	5.1
	5.1
	50

	1432
	Ammonium nitrate based fertilizer, uniform mixtures of the nitrogen/phosphate, nitrogen/potash or nitrogen/phosphate/potash type, containing not more than 70% ammonium nitrate and not more than 0.4% total combustible/organic material calculated as carbon or with not more than 45% ammonium nitrate and unrestricted combustible material
	2071
	9
	
	

	1433
	AMMONIA SOLUTION, relative density less than 0.880 at 15 °C in water, with more than 35% but not more than 50% ammonia
	2073
	2
	2.2
	20

	1434
	ACRYLAMIDE, SOLID
	2074
	6.1
	6.1
	60

	1435
	CHLORAL, ANHYDROUS, STABILIZED
	2075
	6.1
	6.1
	69

	1436
	CRESOLS, LIQUID
	2076
	6.1
	6.1

+8
	68

	1437
	alpha-NAPHTHYLAMINE
	2077
	6.1
	6.1
	60

	1438
	TOLUENE DIISOCYANATE
	2078
	6.1
	6.1
	60

	1439
	DIETHYLENETRIAMINE
	2079
	8
	8
	80

	1440
	HYDROGEN CHLORIDE, REFRIGERATED LIQUID
	2186
	2
	
	

	1441
	CARBON DIOXIDE, REFRIGERATED LIQUID
	2187
	2
	2.2
	22

	1442
	ARSINE
	2188
	2
	2.3

+2.1
	

	1443
	DICHLOROSILANE
	2189
	2
	2.3

+2.1

+8
	263

	1444
	OXYGEN DIFLUORIDE, COMPRESSED
	2190
	2
	2.3

+5.1

+8
	

	1445
	SULPHURYL FLUORIDE
	2191
	2
	2.3
	26

	1446
	GERMANE
	2192
	2
	2.3

+2.1
	263

	1447
	HEXAFLUOROETHANE (REFRIGERANT GAS R 116)
	2193
	2
	2.2
	20

	1448
	SELENIUM HEXAFLUORIDE
	2194
	2
	2.3

+8
	

	1449
	TELLURIUM HEXAFLUORIDE
	2195
	2
	2.3

+8
	

	1450
	TUNGSTEN HEXAFLUORIDE
	2196
	2
	2.3

+8
	

	1451
	HYDROGEN IODIDE, ANHYDROUS
	2197
	2
	2.3

+8
	268

	1452
	PHOSPHORUS PENTAFLUORIDE
	2198
	2
	2.3

+8
	

	1453
	PHOSPHINE
	2199
	2
	2.3

+2.1
	

	1454
	PROPADIENE, STABILIZED
	2200
	2
	2.1
	239

	1455
	NITROUS OXIDE,

REFRIGERATED LIQUID
	2201
	2
	2.2

+5.1
	225

	1456
	HYDROGEN SELENIDE, ANHYDROUS
	2202
	2
	2.3

+2.1
	

	1457
	SILANE
	2203
	2
	2.1
	23

	1458
	CARBONYL SULPHIDE
	2204
	2
	2.3 

+2.1
	263

	1459
	ADIPONITRILE
	2205
	6.1
	6.1
	60

	1460
	ISOCYANATES, TOXIC, N.O.S. or ISOCYANATE SOLUTION, TOXIC, N.O.S.
	2206
	6.1
	6.1
	60

	1461
	ISOCYANATES, TOXIC, N.O.S. or ISOCYANATE SOLUTION, TOXIC, N.O.S.
	2206
	6.1
	6.1
	60

	1462
	CALCIUM HYPOCHLORITE MIXTURE, DRY with more than 10% but not more than 39% available chlorine z
	2208
	5.1
	5.1
	50

	1463
	FORMALDEHYDE SOLUTION with not less than 25% formaldehyde
	2209
	8
	8
	80

	1464
	MANEB or MANEB PREPARATION with not less than 60% maneb
	2210
	4.2
	4.2

+4.3
	40

	1465
	POLYMERIC BEADS, EXPANDABLE, evolving flammable vapour
	2211
	9
	None
	90

	1466
	ASBESTOS, AMPHIBOLE (amosite, tremolite, actinolite, anthophyllite, crocidolite)
	2212
	9
	9
	90

	1467
	PARAFORMALDEHYDE
	2213
	4.1
	4.1
	40

	1468
	PHTHALIC ANHYDRIDE with more than 0.05% of maleic anhydride
	2214
	8
	8
	80

	1469
	MALEIC ANHYDRIDE, MOLTEN
	2215
	8
	8
	80

	1470
	MALEIC ANHYDRIDE
	2215
	8
	8
	80

	1471
	Fish meal (Fish scrap), stabilized
	2216
	9
	
	

	1472
	SEED CAKE with not more than 1.5% oil and not more than 11% moisture
	2217
	4.2
	4.2
	40

	1473
	ACRYLIC ACID, STABILIZED
	2218
	8
	8

+3
	839

	1474
	ALLYL GLYCIDYL ETHER
	2219
	3
	3
	30

	1475
	ANISOLE
	2222
	3
	3
	30

	1476
	BENZONITRILE
	2224
	6.1
	6.1
	60

	1477
	BENZENESULPHONYL CHLORIDE
	2225
	8
	8
	80

	1478
	BENZOTRICHLORIDE
	2226
	8
	8
	80

	1479
	n-BUTYL METHACRYLATE, STABILIZED
	2227
	3
	3
	39

	1480
	2-CHLOROETHANAL
	2232
	6.1
	6.1
	66

	1481
	CHLOROANISIDINES
	2233
	6.1
	6.1
	60

	1482
	CHLOROBENZOTRI-FLUORIDES
	2234
	3
	3
	30

	1483
	CHLOROBENZYL CHLORIDES, LIQUID
	2235
	6.1
	6.1
	60

	1484
	3-CHLORO-4-METHYLPHENYL ISOCYANATE, LIQUID
	2236
	6.1
	6.1
	60

	1485
	CHLORONITROANILINES
	2237
	6.1
	6.1
	60

	1486
	CHLOROTOLUENES
	2238
	3
	3
	30

	1487
	CHLOROTOLUIDINES, SOLID
	2239
	6.1
	6.1
	60

	1488
	CHROMOSULPHURIC ACID
	2240
	8
	8
	88

	1489
	CYCLOHEPTANE
	2241
	3
	3
	33

	1490
	CYCLOHEPTENE
	2242
	3
	3
	33

	1491
	CYCLOHEXYL ACETATE
	2243
	3
	3
	30

	1492
	CYCLOPENTANOL
	2244
	3
	3
	30

	1493
	CYCLOPENTANONE
	2245
	3
	3
	30

	1494
	CYCLOPENTENE
	2246
	3
	3
	33

	1495
	n-DECANE
	2247
	3
	3
	30

	1496
	DI-n-BUTYLAMINE
	2248
	8
	8

+3
	83

	1497
	DICHLORODIMETHYL ETHER, SYMMETRICAL
	2249
	6.1
	
	

	1498
	DICHLOROPHENYL ISOCYANATES
	2250
	6.1
	6.1
	60

	1499
	BICYCLO[2.2.1]HEPTA-2,5- DIENE, STABILIZED (2,5- NORBORNADIENE, STABILIZED)
	2251
	3
	3
	339

	1500
	1,2-DIMETHOXYETHANE
	2252
	3
	3
	33

	1501
	N,N-DIMETHYLANILINE
	2253
	6.1
	6.1
	60

	1502
	MATCHES, FUSEE
	2254
	4.1
	4.1
	

	1503
	CYCLOHEXENE
	2256
	3
	3
	33

	1504
	POTASSIUM
	2257
	4.3
	4.3
	X423

	1505
	1,2-PROPYLENEDIAMINE
	2258
	8
	8

+3
	83

	1506
	TRIETHYLENETETRAMINE
	2259
	8
	8
	80

	1507
	TRIPROPYLAMINE
	2260
	3
	3+8
	38

	1508
	XYLENOLS, SOLID
	2261
	6.1
	6.1
	60

	1509
	DIMETHYLCARBAMOYL CHLORIDE
	2262
	8
	8
	80

	1510
	DIMETHYL-CYCLOHEXANES
	2263
	3
	3
	33

	1511
	N,N-DIMETHYL- CYCLOHEXYLAMINE
	2264
	8
	8

+3
	83

	1512
	N,N-DIMETHYL-FORMAMIDE
	2265
	3
	3
	30

	1513
	DIMETHYL-N-PROPYLAMINE
	2266
	3
	3

+8
	338

	1514
	DIMETHYL THIOPHOSPHORYL CHLORIDE
	2267
	6.1
	6.1

+8
	68

	1515
	3,3'-IMINODIPROPYLAMINE
	2269
	8
	8
	80

	1516
	ETHYLAMINE, AQUEOUS SOLUTION with not less than 50% but not more than 70% ethylamine
	2270
	3
	3

+8
	338

	1517
	ETHYL AMYL KETONE
	2271
	3
	3
	30

	1518
	N-ETHYLANILINE
	2272
	6.1
	6.1
	60

	1519
	2-ETHYLANILINE
	2273
	6.1
	6.1
	60

	1520
	N-ETHYL-N-BENZYLANILINE
	2274
	6.1
	6.1
	60

	1521
	2-ETHYLBUTANOL
	2275
	3
	3
	30

	1522
	2-ETHYLHEXYLAMINE
	2276
	3
	3

+8
	38

	1523
	ETHYL METHACRYLATE, STABILIZED
	2277
	3
	3
	339

	1524
	n-HEPTENE
	2278
	3
	3
	33

	1525
	HEXACHLOROBUTADIENE
	2279
	6.1
	6.1
	60

	1526
	HEXAMETHYLENE-DIAMINE, SOLID
	2280
	8
	8
	80

	1527
	HEXAMETHYLENE DIISOCYANATE
	2281
	6.1
	6.1
	60

	1528
	HEXANOLS
	2282
	3
	3
	30

	1529
	ISOBUTYL METHACRYLATE, STABILIZED
	2283
	3
	3
	39

	1530
	ISOBUTYRONITRILE
	2284
	3
	3

+6.1
	336

	1531
	ISOCYANATOBENZO-TRIFLUORIDES
	2285
	6.1
	6.1

+3
	63

	1532
	PENTAM ETHYLHEPTAN E
	2286
	3
	3
	30

	1533
	ISOHEPTENE
	2287
	3
	3
	33

	1534
	ISOHEXENE
	2288
	3
	3
	33

	1535
	ISOPHORONEDIAMINE
	2289
	8
	8
	80

	1536
	ISOPHORONE DIISOCYANATE
	2290
	6.1
	6.1
	60

	1537
	LEAD COMPOUND, SOLUBLE, N.O.S.
	2291
	6.1
	6.1
	60

	1538
	4-METHOXY-4-METHYLPENTAN-2-ONE
	2293
	3
	3
	30

	1539
	N-METHYLANILINE
	2294
	6.1
	6.1
	60

	1540
	METHYL CHLOROACETATE
	2295
	6.1
	6.1

+3
	663

	1541
	METHYLCYCLOHEXANE
	2296
	3
	3
	33

	1542
	METHYLCYCLO-HEXANONE
	2297
	3
	3
	30

	1543
	METHYLCYCLOPENTANE
	2298
	3
	3
	33

	1544
	METHYL DICHLOROACETATE
	2299
	6.1
	6.1
	60

	1545
	2-METHYL-5-ETHYLPYRIDINE
	2300
	6.1
	6.1
	60

	1546
	2-METHYLFURAN
	2301
	3
	3
	33

	1547
	5-METHYLHEXAN-2-ONE
	2302
	3
	3
	30

	1548
	ISOPROPENYLBENZENE
	2303
	3
	3
	30

	1549
	NAPHTHALENE, MOLTEN
	2304
	4.1
	4.1
	44

	1550
	NITROBENZENE-SULPHONIC ACID
	2305
	8
	8
	80

	1551
	NITROBENZOTRI-FLUORIDES, LIQUID
	2306
	6.1
	6.1
	60

	1552
	3-NITRO-4-CHLORO- BENZOTRIFLUORIDE
	2307
	6.1
	6.1
	60

	1553
	NITROSYLSULPHURIC ACID, LIQUID
	2308
	8
	8
	X80

	1554
	OCTADIENES
	2309
	3
	3
	33

	1555
	PENTANE-2,4-DIONE
	2310
	3
	3

+6.1
	36

	1556
	PHENETIDINES
	2311
	6.1
	6.1
	60

	1557
	PHENOL, MOLTEN
	2312
	6.1
	6.1
	60

	1558
	PICOLINES
	2313
	3
	3
	30

	1559
	POLYCHLORINATED BIPHENYLS, LIQUID
	2315
	9
	9
	90

	1560
	SODIUM CUPROCYANIDE, SOLID
	2316
	6.1
	6.1
	66

	1561
	SODIUM CUPROCYANIDE SOLUTION
	2317
	6.1
	6.1
	66

	1562
	SODIUM HYDROSULPHIDE with less than 25% water of crystallization
	2318
	4.2
	4.2
	40

	1563
	TERPENE HYDROCARBONS, N.O.S.
	2319
	3
	3
	30

	1564
	TETRAETHYLENE-PENTAMINE
	2320
	8
	8
	80

	1565
	TRICHLOROBENZENES, LIQUID
	2321
	6.1
	6.1
	60

	1566
	TRICHLOROBUTENE
	2322
	6.1
	6.1
	60

	1567
	TRIETHYL PHOSPHITE
	2323
	3
	3
	30

	1568
	TRIISOBUTYLENE
	2324
	3
	3
	30

	1569
	1,3,5-TRIMETHYLBENZENE
	2325
	3
	3
	30

	1570
	TRIMETHYLCYCLO​ EXYLAMINE
	2326
	8
	8
	80

	1571
	TRIMETHYLHEXA​ METHYLENEDIAMINES
	2327
	8
	8
	80

	1572
	TRIMETHYLHEXA-METHYLENE DIISOCYANATE
	2328
	6.1
	6.1
	60

	1573
	TRIMETHYL PHOSPHITE
	2329
	3
	3
	30

	1574
	UNDECANE
	2330
	3
	3
	30

	1575
	ZINC CHLORIDE, ANHYDROUS
	2331
	8
	8
	80

	1576
	ACETALDEHYDE OXIME
	2332
	3
	3
	30

	1577
	ALLYL ACETATE
	2333
	3
	3

+6.1
	336

	1578
	ALLYLAMINE
	2334
	6.1
	6.1

+3
	663

	1579
	ALLYL ETHYL ETHER
	2335
	3
	3

+6.1
	336

	1580
	ALLYL FORMATE
	2336
	3
	3

+6.1
	336

	1581
	PHENYL MERCAPTAN
	2337
	6.1
	6.1

+3
	663

	1582
	BENZOTRIFLUORIDE
	2338
	3
	3
	33

	1583
	2-BROMOBUTANE
	2339
	3
	3
	33

	1584
	2-BROMOETHYL ETHYL ETHER
	2340
	3
	3
	33

	1585
	1-BROMO-3-METHYLBUTANE
	2341
	3
	3
	30

	1586
	BROMOMETHYL-PROPANES
	2342
	3
	3
	33

	1587
	2-BROMOPENTANE
	2343
	3
	3
	33

	1588
	BROMOPROPANES
	2344
	3
	3
	33

	1589
	BROMOPROPANES
	2344
	3
	3
	30

	1590
	3-BROMOPROPYNE
	2345
	3
	3
	33

	1591
	BUTANEDIONE
	2346
	3
	3
	33

	1592
	BUTYL MERCAPTAN
	2347
	3
	3
	33

	1593
	BUTYL ACRYLATES, STABILIZED
	2348
	3
	3
	39

	1594
	BUTYL METHYL ETHER
	2350
	3
	3
	33

	1595
	BUTYL NITRITES
	2351
	3
	3
	33

	1596
	BUTYL NITRITES
	2351
	3
	3
	30

	1597
	BUTYL VINYL ETHER, STABILIZED
	2352
	3
	3
	339

	1598
	BUTYRYL CHLORIDE
	2353
	3
	3

+8
	338

	1599
	CHLOROMETHYL ETHYL ETHER
	2354
	3
	3

+6.1
	336

	1600
	2-CHLOROPROPANE
	2356
	3
	3
	33

	1601
	CYCLOHEXYLAMINE
	2357
	8
	8

+3
	83

	1602
	CYCLOOCTATETRAE N E
	2358
	3
	3
	33

	1603
	DIALLYLAMINE
	2359
	3
	3

+6.1

+8
	338

	1604
	DIALLYL ETHER
	2360
	3
	3

+6.1
	336

	1605
	DIISOBUTYLAMINE
	2361
	3
	3

+8
	38

	1606
	1,1-DICHLOROETHANE
	2362
	3
	3
	33

	1607
	ETHYL MERCAPTAN
	2363
	3
	3
	33

	1608
	n-PROPYLBENZENE
	2364
	3
	3
	30

	1609
	DIETHYL CARBONATE
	2366
	3
	3
	30

	1610
	alpha-METHYL- VALERALDEHYDE
	2367
	3
	3
	33

	1611
	alpha-PINENE
	2368
	3
	3
	30

	1612
	1-HEXENE
	2370
	3
	3
	33

	1613
	ISOPENTENES
	2371
	3
	3
	33

	1614
	1,2-DI-(DIMETHYLAMINO) ETHANE
	2372
	3
	3
	33

	1615
	DIETHOXYMETHANE
	2373
	3
	3
	33

	1616
	3,3-DIETHOXYPROPENE
	2374
	3
	3
	33

	1617
	DIETHYL SULPHIDE
	2375
	3
	3
	33

	1618
	2,3-DIHYDROPYRAN
	2376
	3
	3
	33

	1619
	1,1-DIMETHOXYETHANE
	2377
	3
	3
	33

	1620
	2-DIMETHYLAMINO- ACETONITRILE
	2378
	3
	3

+6.1
	336

	1621
	1,3-DIMETHYLBUTYLAMINE
	2379
	3
	3

+8
	338

	1622
	DIMETHYLDIETHOXY-SILANE
	2380
	3
	3
	33

	1623
	DIMETHYL DISULPHIDE
	2381
	3
	3

+6.1
	336

	1624
	DIMETHYLHYDRAZINE, SYMMETRICAL
	2382
	6.1
	6.1

+3
	663

	1625
	DIPROPYLAMINE
	2383
	3
	3

+8
	338

	1626
	DI-n-PROPYL ETHER
	2384
	3
	3
	33

	1627
	ETHYL ISOBUTYRATE
	2385
	3
	3
	33

	1628
	1-ETHYLPIPERIDINE
	2386
	3
	3+8
	338

	1629
	FLUOROBENZENE
	2387
	3
	3
	33

	1630
	FLUOROTOLUENES
	2388
	3
	3
	33

	1631
	FURAN
	2389
	3
	3
	33

	1632
	2-IODOBUTANE
	2390
	3
	3
	33

	1633
	IODOMETHYLPROPANES
	2391
	3
	3
	33

	1634
	IODOPROPANES
	2392
	3
	3
	30

	1635
	ISOBUTYL FORMATE
	2393
	3
	3
	33

	1636
	ISOBUTYL PROPIONATE
	2394
	3
	3
	30

	1637
	ISOBUTYRYL CHLORIDE
	2395
	3
	3

+8
	338

	1638
	METHACRYLALDEHYDE, STABILIZED
	2396
	3
	3

+6.1
	336

	1639
	3-METHYLBUTAN-2-ONE
	2397
	3
	3
	33

	1640
	METHYL tert-BUTYL ETHER
	2398
	3
	3
	33

	1641
	1-METHYLPIPERIDINE
	2399
	3
	3

+8
	338

	1642
	METHYL ISOVALERATE
	2400
	3
	3
	33

	1643
	PIPERIDINE
	2401
	8
	8

+3
	883

	1644
	PROPANETHIOLS
	2402
	3
	3
	33

	1645
	ISOPROPENYL ACETATE
	2403
	3
	3
	33

	1646
	PROPIONITRILE
	2404
	3
	3

+6.1
	336

	1647
	ISOPROPYL BUTYRATE
	2405
	3
	3
	30

	1648
	ISOPROPYL ISOBUTYRATE
	2406
	3
	3
	33

	1649
	ISOPROPYL CHLOROFORMATE
	2407
	6.1
	6.1

+3

+8
	

	1650
	ISOPROPYL PROPIONATE
	2409
	3
	3
	33

	1651
	1,2,3,6-TETRAHYDROPYRIDINE
	2410
	3
	3
	33

	1652
	BUTYRONITRILE
	2411
	3
	3

+6.1
	336

	1653
	TETRAHYDROTHIOPHENE
	2412
	3
	3
	33

	1654
	TETRAPROPYL ORTHOTITANATE
	2413
	3
	3
	30

	1655
	THIOPHENE
	2414
	3
	3
	33

	1656
	TRIMETHYL BORATE
	2416
	3
	3
	33

	1657
	CARBONYL FLUORIDE
	2417
	2
	2.3

+8
	268

	1658
	SULPHUR TETRAFLUORIDE
	2418
	2
	2.3

+8
	

	1659
	BROMOTRIFLUORO-ETHYLENE
	2419
	2
	2.1
	23

	1660
	HEXAFLUOROACETONE
	2420
	2
	2.3

+8
	268

	1661
	NITROGEN TRIOXIDE
	2421
	2
	
	

	1662
	OCTAFLUOROBUT-2-ENE (REFRIGERANT GAS R 1318)
	2422
	2
	2.2
	20

	1663
	OCTAFLUOROPROPANE (REFRIGERANT GAS R 218)
	2424
	2
	2.2
	20

	1664
	AMMONIUM NITRATE, LIQUID, hot concentrated solution, in a concentration of more than 80% but not more than 93%
	2426
	5.1
	5.1
	59

	1665
	POTASSIUM CHLORATE, AQUEOUS SOLUTION
	2427
	5.1
	5.1
	50

	1666
	POTASSIUM CHLORATE, AQUEOUS SOLUTION
	2427
	5.1
	5.1
	50

	1667
	SODIUM CHLORATE, AQUEOUS SOLUTION
	2428
	5.1
	5.1
	50

	1668
	SODIUM CHLORATE, AQUEOUS SOLUTION
	2428
	5.1
	5.1
	50

	1669
	CALCIUM CHLORATE, AQUEOUS SOLUTION
	2429
	5.1
	5.1
	50

	1670
	CALCIUM CHLORATE, AQUEOUS SOLUTION
	2429
	5.1
	5.1
	50

	1671
	ALKYLPHENOLS, SOLID, N.O.S. (including C2-C12 homologues)
	2430
	8
	8
	88

	1672
	ALKYLPHENOLS, SOLID, N.O.S. (including C2-C12 homologues)
	2430
	8
	8
	80

	1673
	ALKYLPHENOLS, SOLID, N.O.S. (including C2-C12 homologues)
	2430
	8
	8
	80

	1674
	ANISIDINES
	2431
	6.1
	6.1
	60

	1675
	N,N-DIETHYLANILINE
	2432
	6.1
	6.1
	60

	1676
	CHLORONITROTOLUENES. LIQUID
	2433
	6.1
	6.1
	60

	1677
	DIBENZYL-DICHLOROSILANE
	2434
	8
	8
	X80

	1678
	ETHYLPHENYL​DICHLOROSILANE
	2435
	8
	8
	X80

	1679
	THIOACETIC ACID
	2436
	3
	3
	33

	1680
	METHYLPHENYL​ DICHLOROSILANE
	2437
	8
	8
	X80

	1681
	TRIMETHYLACETYL CHLORIDE
	2438
	6.1
	6.1

+3

+8
	663

	1682
	SODIUM HYDROGENDIFLUORIDE
	2439
	8
	8
	80

	1683
	STANNIC CHLORIDE PENTAHYDRATE
	2440
	8
	8
	80

	1684
	TITANIUM TRICHLORIDE, PYROPHORIC or TITANIUM TRICHLORIDE MIXTURE. PYROPHORIC
	2441
	4.2
	4.2

+8
	

	1685
	TRICHLOROACETYL CHLORIDE
	2442
	8
	8
	X80

	1686
	VANADIUM OXYTRICHLORIDE
	2443
	8
	8
	80

	1687
	VANADIUM TETRACHLORIDE
	2444
	8
	8
	X88

	1688
	NITROCRESOLS, SOLID
	2446
	6.1
	6.1
	60

	1689
	PHOSPHORUS, WHITE, MOLTEN
	2447
	4.2
	4.2

+6.1
	446

	1690
	SULPHUR, MOLTEN
	2448
	4.1
	4.1
	44

	1691
	NITROGEN TRIFLUORIDE
	2451
	2
	2.2

+5.1
	25

	1692
	ETHYLACETYLENE, STABILIZED
	2452
	2
	2.1
	239

	1693
	ETHYL FLUORIDE (REFRIGERANT GAS R 161)
	2453
	2
	2.1
	23

	1694
	METHYL FLUORIDE (REFRIGERANT GAS R 41)
	2454
	2
	2.1
	23

	1695
	METHYL NITRITE
	2455
	2
	
	

	1696
	2-CHLOROPROPENE
	2456
	3
	3
	33

	1697
	2,3-DIMETHYLBUTANE
	2457
	3
	3
	33

	1698
	HEXADIENES
	2458
	3
	3
	33

	1699
	2-METHYL-1-BUTENE
	2459
	3
	3
	33

	1700
	2-METHYL-2-BUTENE
	2460
	3
	3
	33

	1701
	METHYLPENTADIENE
	2461
	3
	3
	33

	1702
	ALUMINIUM HYDRIDE
	2463
	4.3
	4.3
	

	1703
	BERYLLIUM NITRATE
	2464
	5.1
	5.1

+6.1
	56

	1704
	DICHLOROISOCYANURIC ACID, DRY or DICHLOROISOCYANURIC ACID SALTS
	2465
	5.1
	5.1
	50

	1705
	POTASSIUM SUPEROXIDE
	2466
	5.1
	5.1
	

	1706
	TRICHLOROISOCYANURIC ACID, DRY
	2468
	5.1
	5.1
	50

	1707
	ZINC BROMATE
	2469
	5.1
	5.1
	50

	1708
	PHENYLACETONITRILE, LIQUID
	2470
	6.1
	6.1
	60

	1709
	OSMIUM TETROXIDE
	2471
	6.1
	6.1
	66

	1710
	SODIUM ARSANILATE
	2473
	6.1
	6.1
	60

	1711
	THIOPHOSGENE
	2474
	6.1
	6.1
	66

	1712
	VANADIUM TRICHLORIDE
	2475
	8
	8
	80

	1713
	METHYL ISOTHIOCYANATE
	2477
	6.1
	6.1

+3
	663

	1714
	ISOCYANATES, FLAMMABLE, TOXIC, N.O.S. or ISOCYANATE SOLUTION, FLAMMABLE, TOXIC, N.O.S.
	2478
	3
	3

+6.1
	336

	1715
	ISOCYANATES, FLAMMABLE, TOXIC, N.O.S. or ISOCYANATE SOLUTION, FLAMMABLE, TOXIC, N.O.S.
	2478
	3
	3

+6.1
	36

	1716
	METHYL ISOCYANATE
	2480
	6.1
	6.1

+3
	663

	1717
	ETHYL ISOCYANATE
	2481
	6.1
	6.1 

+3
	663

	1718
	n-PROPYL ISOCYANATE
	2482
	6.1
	6.1

+3
	663

	1719
	ISOPROPYL ISOCYANATE
	2483
	6.1
	6.1

+3
	663

	1720
	tert-BUTYL ISOCYANATE
	2484
	6.1
	6.1

+3
	663

	1721
	n-BUTYL ISOCYANATE
	2485
	6.1
	6.1

+3
	663

	1722
	ISOBUTYL ISOCYANATE
	2486
	6.1
	6.1

+3
	663

	1723
	PHENYL ISOCYANATE
	2487
	6.1
	6.1

+3
	663

	1724
	CYCLOHEXYL ISOCYANATE
	2488
	6.1
	6.1

+3
	663

	1725
	DICHLOROISOPROPYL ETHER
	2490
	6.1
	6.1
	60

	1726
	ETHANOLAMINE or ETHANOLAMINE SOLUTION
	2491
	8
	8
	80

	1727
	HEXAMETHYLENEIMINE
	2493
	3
	3

+8
	338

	1728
	IODINE PENTAFLUORIDE
	2495
	5.1
	5.1+6.1+8
	568

	1729
	PROPIONIC ANHYDRIDE
	2496
	8
	8
	80

	1730
	1,2,3,6-TETRAHYDROBENZAL- DEHYDE
	2498
	3
	3
	30

	1731
	TRIS-(I-AZIRIDINYL) PHOSPHINE OXIDE SOLUTION
	2501
	6.1
	6.1
	60

	1732
	TRIS-(I-AZIRIDINYL) PHOSPHINE OXIDE SOLUTION
	2501
	6.1
	6.1
	60

	1733
	VALERYL CHLORIDE
	2502
	8
	8

+3
	83

	1734
	ZIRCONIUM TETRACHLORIDE
	2503
	8
	8
	80

	1735
	TETRABROMOETHANE
	2504
	6.1
	6.1
	60

	1736
	AMMONIUM FLUORIDE
	2505
	6.1
	6.1
	60

	1737
	AMMONIUM HYDROGEN SULPHATE
	2506
	8
	8
	80

	1738
	CHLOROPLATINIC ACID, SOLID
	2507
	8
	8
	80

	1739
	MOLYBDENUM PENTACHLORIDE
	2508
	8
	8
	80

	1740
	POTASSIUM HYDROGEN SULPHATE
	2509
	8
	8
	80

	1741
	2-CHLOROPROPIONIC ACID
	2511
	8
	8
	80

	1742
	AMINOPHENOLS (o-, m-, p-)
	2512
	6.1
	6.1
	60

	1743
	BROMOACETYL BROMIDE
	2513
	8
	8
	X80

	1744
	BROMOBENZENE
	2514
	3
	3
	30

	1745
	BROMOFORM
	2515
	6.1
	6.1
	60

	1746
	CARBON TETRABROMIDE
	2516
	6.1
	6.1
	60

	1747
	1-CHLORO-1,1- DIFLUOROETHANE (REFRIGERANT GAS R 142b)
	2517
	2
	2.1
	23

	1748
	1,5,9-CYCLODODECATRIENE
	2518
	6.1
	6.1
	60

	1749
	CYCLOOCTADIENES
	2520
	3
	3
	30

	1750
	DIKETENE, STABILIZED
	2521
	6.1
	6.1

+3
	663

	1751
	2-DIMETHYLAMINOETHYL METHACRYLATE
	2522
	6.1
	6.1
	69

	1752
	ETHYL ORTHOFORMATE
	2524
	3
	3
	30

	1753
	ETHYL OXALATE
	2525
	6.1
	6.1
	60

	1754
	FURFURYLAMINE
	2526
	3
	3

+8
	38

	1755
	ISOBUTYL ACRYLATE, STABILIZED
	2527
	3
	3
	39

	1756
	ISOBUTYL ISOBUTYRATE
	2528
	3
	3
	30

	1757
	ISOBUTYRIC ACID
	2529
	3
	3

+8
	38

	1758
	METHACRYLIC ACID, STABILIZED
	2531
	8
	8
	89

	1759
	METHYL TRICHLOROACETATE
	2533
	6.1
	6.1
	60

	1760
	METHYLCHLOROSILANE
	2534
	2
	2.3

+2.1

+8
	263

	1761
	4-METHYLMORPHOLINE (N-METHYLMORPHOLINE)
	2535
	3
	3

+8
	338

	1762
	METHYLTETRAHYDRO-FURAN
	2536
	3
	3
	33

	1763
	NITRONAPHTHALENE
	2538
	4.1
	4.1
	40

	1764
	TERPINOLENE
	2541
	3
	3
	30

	1765
	TRIBUTYLAMINE
	2542
	6.1
	6.1
	60

	1766
	HAFNIUM POWDER, DRY
	2545
	4.2
	4.2
	

	1767
	HAFNIUM POWDER, DRY
	2545
	4.2
	4.2
	40

	1768
	HAFNIUM POWDER, DRY
	2545
	4.2
	4.2
	40

	1769
	TITANIUM POWDER, DRY
	2546
	4.2
	4.2
	

	1770
	TITANIUM POWDER, DRY
	2546
	4.2
	4.2
	40

	1771
	TITANIUM POWDER, DRY
	2546
	4.2
	4.2
	40

	1772
	SODIUM SUPEROXIDE
	2547
	5.1
	5.1
	

	1773
	CHLORINE PENTAFLUORIDE
	2548
	2
	2.3

+5.1

+8
	

	1774
	HEXAFLUOROACETONE HYDRATE, LIQUID
	2552
	6.1
	6.1
	60

	1775
	METHYLALLYL CHLORIDE
	2554
	3
	3
	33

	1776
	NITROCELLULOSE WITH WATER (not less than 25% water, by mass)
	2555
	4.1
	4.1
	

	1777
	NITROCELLULOSE WITH ALCOHOL (not less than 25% alcohol, by mass, and not more than 12.6% nitrogen, by dry mass)
	2556
	4.1
	4.1
	

	1778
	NITROCELLULOSE, with not more than 12.6% nitrogen, by dry mass, MIXTURE WITH or WITHOUT PLASTICIZER, WITH or WITHOUT PIGMENT
	2557
	4.1
	4.1
	

	1779
	EPIBROMOHYDRIN
	2558
	6.1
	6.1

+3
	663

	1780
	2-METHYLPENTAN-2-OL
	2560
	3
	3
	30

	1781
	3-METHYL-1-BUTENE
	2561
	3
	3
	33

	1782
	TRICHLOROACETIC ACID SOLUTION
	2564
	8
	8
	80

	1783
	TRICHLOROACETIC ACID SOLUTION
	2564
	8
	8
	80

	1784
	DICYCLOHEXYLAMINE
	2565
	8
	8
	80

	1785
	SODIUM PENTACHLOROPHENATE
	2567
	6.1
	6.1
	60

	1786
	CADMIUM COMPOUND
	2570
	6.1
	6.1
	66

	1787
	CADMIUM COMPOUND
	2570
	6.1
	6.1
	60

	1788
	CADMIUM COMPOUND
	2570
	6.1
	6.1
	60

	1789
	ALKYLSULPHURIC ACIDS
	2571
	8
	8
	80

	1790
	PHENYLHYDRAZINE
	2572
	6.1
	6.1
	60

	1791
	THALLIUM CHLORATE
	2573
	5.1
	5.1

+6.1
	56

	1792
	TRICRESYL PHOSPHATE with more than 3% ortho isomer
	2574
	6.1
	6.1
	60

	1793
	PHOSPHORUS OXYBROMIDE, MOLTEN
	2576
	8
	8
	80

	1794
	PHENYLACETYL CHLORIDE
	2577
	8
	8
	80

	1795
	PHOSPHORUS TRIOXIDE
	2578
	8
	8
	80

	1796
	PIPERAZINE
	2579
	8
	8
	80

	1797
	ALUMINIUM BROMIDE SOLUTION
	2580
	8
	8
	80

	1798
	ALUMINIUM CHLORIDE SOLUTION
	2581
	8
	8
	80

	1799
	FERRIC CHLORIDE SOLUTION
	2582
	8
	8
	80

	1800
	ALKYLSULPHONIC ACIDS, SOLID or ARYLSULPHONIC ACIDS, SOLID with more than 5% free sulphuric acid
	2583
	8
	8
	80

	1801
	ALKYLSULPHONIC ACIDS, LIQUID or ARYLSULPHONIC ACIDS, LIQUID with more than 5% free sulphuric acid
	2584
	8
	8
	80

	1802
	ALKYLSULPHONIC ACIDS, SOLID or ARYLSULPHONIC ACIDS, SOLID with not more than 5% free sulphuric acid
	2585
	8
	8
	80

	1803
	ALKYLSULPHONIC ACIDS, LIQUID or ARYLSULPHONIC ACIDS, LIQUID with not more than 5% free sulphuric acid
	2586
	8
	8
	80

	1804
	BENZOQUINONE
	2587
	6.1
	6.1
	60

	1805
	PESTICIDE, SOLID, TOXIC, N.O.S
	2588
	6.1
	6.1
	66

	1806
	PESTICIDE, SOLID, TOXIC, N.O.S.
	2588
	6.1
	6.1
	60

	1807
	PESTICIDE, SOLID, TOXIC, N.O.S
	2588
	6.1
	6.1
	60

	1808
	VINYL CHLOROACETATE
	2589
	6.1
	6.1

+3
	63

	1809
	ASBESTOS, CHRYSOTILE
	2590
	9
	9
	90

	1810
	XENON, REFRIGERATED LIQUID
	2591
	2
	2.2
	22

	1811
	CHLOROTRIFLUORO-METHANE AND TRIFLUOROMETHANE AZEOTROPIC MIXTURE with approximately 60% chlorotrifluoromethane (REFRIGERANT GAS R 503)
	2599
	2
	2.2
	20

	1812
	CYCLOBUTANE
	2601
	2
	2.1
	23

	1813
	DICHLORODIFLUORO-​METHANE AND 1,1- DIFLUOROETHANE AZEOTROPIC MIXTURE with approximately 74% dichlorodifluoromethane (REFRIGERANT GAS R 500)
	2602
	2
	2.2
	20

	1814
	CYCLOHEPTATRIENE
	2603
	3
	3

+6.1
	336

	1815
	BORON TRIFLUORIDE DIETHYL ETHERATE
	2604
	8
	8

+3
	883

	1816
	METHOXYMETHYL ISOCYANATE
	2605
	6.1
	6.1

+3
	663

	1817
	METHYL ORTHOSILICATE
	2606
	6.1
	6.1

+3
	663

	1818
	ACROLEIN DIMER, STABILIZED
	2607
	3
	3
	39

	1819
	NITROPROPANES
	2608
	3
	3
	30

	1820
	TRIALLYL BORATE
	2609
	6.1
	6.1
	60

	1821
	TRIALLYLAMINE
	2610
	3
	3+8
	38

	1822
	PROPYLENE CHLOROHYDRIN
	2611
	6.1
	6.1

+3
	63

	1823
	METHYL PROPYL ETHER
	2612
	3
	3
	33

	1824
	METHALLYL ALCOHOL
	2614
	3
	3
	30

	1825
	ETHYL PROPYL ETHER
	2615
	3
	3
	33

	1826
	TRIISOPROPYL BORATE
	2616
	3
	3
	33

	1827
	TRIISOPROPYL BORATE
	2616
	3
	3
	30

	1828
	METHYLCYCLO-HEXANOLS, flammable
	2617
	3
	3
	30

	1829
	VINYLTOLUENES, STABILIZED
	2618
	3
	3
	39

	1830
	BENZYLDIMETHYLAMINE
	2619
	8
	8

+3
	83

	1831
	AMYL BUTYRATES
	2620
	3
	3
	30

	1832
	ACETYL METHYL CARBINOL
	2621
	3
	3
	30

	1833
	GLYCIDALDEHYDE
	2622
	3
	3

+6.1
	336

	1834
	FIRELIGHTERS, SOLID with flammable liquid
	2623
	4.1
	4.1
	

	1835
	MAGNESIUM SILICIDE
	2624
	4.3
	4.3
	423

	1836
	CHLORIC ACID, AQUEOUS SOLUTION with not more than 10% chloric acid
	2626
	5.1
	5.1
	50

	1837
	NITRITES, INORGANIC, NO.S.
	2627
	5.1
	5.1
	50

	1838
	POTASSIUM FLUOROACETATE
	2628
	6.1
	6.1
	66

	1839
	SODIUM FLUOROACETATE
	2629
	6.1
	6.1
	66

	1840
	SELENATES or SELENITES
	2630
	6.1
	6.1
	66

	1841
	FLUOROACETIC ACID
	2642
	6.1
	6.1
	66

	1842
	METHYL BROMOACETATE
	2643
	6.1
	6.1
	60

	1843
	METHYL IODIDE
	2644
	6.1
	6.1
	66

	1844
	PHENACYL BROMIDE
	2645
	6.1
	6.1
	60

	1845
	HEXACHLOROCYCLO-PENTADIENE
	2646
	6.1
	6.1
	66

	1846
	MALONONITRILE
	2647
	6.1
	6.1
	60

	1847
	1,2-DIBROMOBUTAN-3-ONE
	2648
	6.1
	6.1
	60

	1848
	1,3-DICHLOROACETONE
	2649
	6.1
	6.1
	60

	1849
	1,1 -DICH LORO-1 -NITROETHANE
	2650
	6.1
	6.1
	60

	1850
	4,4'-DIAMINODIPHENYL- METHANE
	2651
	6.1
	6.1
	60

	1851
	BENZYL IODIDE
	2653
	6.1
	6.1
	60

	1852
	POTASSIUM FLUOROSILICATE
	2655
	6.1
	6.1
	60

	1853
	QUINOLINE
	2656
	6.1
	6.1
	60

	1854
	SELENIUM DISULPHIDE
	2657
	6.1
	6.1
	60

	1855
	SODIUM CHLOROACETATE
	2659
	6.1
	6.1
	60

	1856
	NITROTOLUIDINES (MONO)
	2660
	6.1
	6.1
	60

	1857
	HEXACHLOROACETONE
	2661
	6.1
	6.1
	60

	1858
	DIBROMOMETHANE
	2664
	6.1
	6.1
	60

	1859
	BUTYLTOLUENES
	2667
	6.1
	6.1
	60

	1860
	CHLOROACETONITRILE
	2668
	6.1
	6.1

+3
	663

	1861
	CHLOROCRESOLS SOLUTION
	2669
	6.1
	6.1
	60

	1862
	CHLOROCRESOLS SOLUTION
	2669
	6.1
	6.1
	60

	1863
	CYANURIC CHLORIDE
	2670
	8
	8
	80

	1864
	AMINOPYRIDINES (o-, m-, p-)
	2671
	6.1
	6.1
	60

	1865
	AMMONIA SOLUTION, relative density between 0.880 and 0.957 at 15 °C in water, with more than 10% but not more than 35% ammonia
	2672
	8
	8
	80

	1866
	2-AMINO-4-CHLOROPHENOL
	2673
	6.1
	6.1
	60

	1867
	SODIUM FLUOROSILICATE
	2674
	6.1
	6.1
	60

	1868
	STIBINE
	2676
	2
	2.3

+2.1
	

	1869
	RUBIDIUM HYDROXIDE SOLUTION
	2677
	8
	8
	80

	1870
	RUBIDIUM HYDROXIDE SOLUTION
	2677
	8
	8
	80

	1871
	RUBIDIUM HYDROXIDE
	2678
	8
	8
	80

	1872
	LITHIUM HYDROXIDE SOLUTION
	2679
	8
	8
	80

	1873
	LITHIUM HYDROXIDE SOLUTION
	2679
	8
	8
	80

	1874
	LITHIUM HYDROXIDE
	2680
	8
	8
	80

	1875
	CAESIUM HYDROXIDE SOLUTION
	2681
	8
	8
	80

	1876
	CAESIUM HYDROXIDE SOLUTION
	2681
	8
	8
	80

	1877
	CAESIUM HYDROXIDE
	2682
	8
	8
	80

	1878
	AMMONIUM SULPHIDE SOLUTION
	2683
	8
	8

+3

+6.1
	86

	1879
	3-DIETHYLAMI NO PROPYL- AMINE
	2684
	3
	3

+8
	38

	1880
	N,N-DIETHYLETHYLENE- DIAMINE
	2685
	8
	8 +3
	83

	1881
	2-DIETHYLAMINO-ETHANOL
	2686
	8
	8 +3
	83

	1882
	DICYCLOHEXYL-AMMONIUM NITRITE
	2687
	4.1
	4.1
	40

	1883
	1-BROMO-3-CHLOROPROPANE
	2688
	6.1
	6.1
	60

	1884
	GLYCEROL alpha- MONOCHLOROHYDRIN
	2689
	6.1
	6.1
	60

	1885
	N,n-BUTYLIMIDAZOLE
	2690
	6.1
	6.1
	60

	1886
	PHOSPHORUS PENTABROMIDE
	2691
	8
	8
	80

	1887
	BORON TRIBROMIDE
	2692
	8
	8
	X88

	1888
	BISULPHITES, AQUEOUS SOLUTION, N.O.S.
	2693
	8
	8
	80

	1889
	TETRAHYDROPHTHALIC ANHYDRIDES with more than 0.05% of maleic anhydride
	2698
	8
	8
	80

	1890
	TRIFLUOROACETIC ACID
	2699
	8
	8
	88

	1891
	1-PENTOL
	2705
	8
	8
	80

	1892
	DIMETHYLDIOXANES
	2707
	3
	3
	33

	1893
	DIMETHYLDIOXANES
	2707
	3
	3
	30

	1894
	BUTYLBENZENES
	2709
	3
	3
	30

	1895
	DIPROPYL KETONE
	2710
	3
	3
	30

	1896
	ACRIDINE
	2713
	6.1
	6.1
	60

	1897
	ZINC RESINATE
	2714
	4.1
	4.1
	40

	1898
	ALUMINIUM RESINATE
	2715
	4.1
	4.1
	40

	1899
	1,4-BUTYNEDIOL
	2716
	6.1
	6.1
	60

	1900
	CAMPHOR, synthetic
	2717
	4.1
	4.1
	40

	1901
	BARIUM BROMATE
	2719
	5.1
	5.1+6.1
	56

	1902
	CHROMIUM NITRATE
	2720
	5.1
	5.1
	50

	1903
	COPPER CHLORATE
	2721
	5.1
	5.1
	50

	1904
	LITHIUM NITRATE
	2722
	5.1
	5.1
	50

	1905
	MAGNESIUM CHLORATE
	2723
	5.1
	5.1
	50

	1906
	MANGANESE NITRATE
	2724
	5.1
	5.1
	50

	1907
	NICKEL NITRATE
	2725
	5.1
	5.1
	50

	1908
	NICKEL NITRITE
	2726
	5.1
	5.1
	50

	1909
	THALLIUM NITRATE
	2727
	6.1
	6.1

+5.1
	65

	1910
	ZIRCONIUM NITRATE
	2728
	5.1
	5.1
	50

	1911
	HEXACHLOROBENZENE
	2729
	6.1
	6.1
	60

	1912
	NITROANISOLES, LIQUID
	2730
	6.1
	6.1
	60

	1913
	NITROBROMOBENZENES, LIQUID
	2732
	6.1
	6.1
	60

	1914
	AMINES, FLAMMABLE, CORROSIVE, N.O.S. or POLYAMINES, FLAMMABLE, CORROSIVE, N.O.S
	2733
	3
	3

+8
	338

	1915
	AMINES, FLAMMABLE, CORROSIVE, N.O.S. or POLYAMINES, FLAMMABLE, CORROSIVE, N.O.S.
	2733
	3
	3

+8
	338

	1916
	AMINES, FLAMMABLE, CORROSIVE, N.O.S. or POLYAMINES, FLAMMABLE, CORROSIVE, N.O.S.
	2733
	3
	3

+8
	38

	1917
	AMINES, LIQUID, CORROSIVE, FLAMMABLE, N.O.S. or POLYAMINES, LIQUID, CORROSIVE, FLAMMABLE, N.O.S.
	2734
	8
	8

+3
	883

	1918
	AMINES, LIQUID, CORROSIVE, FLAMMABLE, N.O.S. or POLYAMINES, LIQUID, CORROSIVE, FLAMMABLE, N.O.S.
	2734
	8
	8

+3
	83

	1919
	AMINES, LIQUID, CORROSIVE, N.O.S. or POLYAMINES, LIQUID, CORROSIVE, N.O.S.
	2735
	8
	8
	88

	1920
	AMINES, LIQUID. CORROSIVE, N.O.S. or POLYAMINES, LIQUID. CORROSIVE, N.O.S.
	2735
	8
	8
	80

	1921
	AMINES, LIQUID, CORROSIVE, N.O.S. or POLYAMINES, LIQUID, CORROSIVE, N.O.S.
	2735
	8
	8
	80

	1922
	N-BUTYLANILINE
	2738
	6.1
	6.1
	60

	1923
	BUTYRIC ANHYDRIDE
	2739
	8
	8
	80

	1924
	n-PROPYL CHLOROFORMATE
	2740
	6.1
	6.1

+3

+8
	668

	1925
	BARIUM HYPOCHLORITE with more than 22% available chlorine
	2741
	5.1
	5.1

+6.1
	56

	1926
	CHLOROFORMATES, TOXIC, CORROSIVE, FLAMMABLE, N.O.S.
	2742
	6.1
	6.1

+3

+8
	638

	1927
	n-BUTYL CHLOROFORMATE
	2743
	6.1
	6.1+3+8
	638

	1928
	CYCLOBUTYL CHLOROFORMATE
	2744
	6.1
	6.1

+3

+8
	638

	1929
	CHLOROMETHYL CHLOROFORMATE
	2745
	6.1
	6.1

+8
	68

	1930
	PHENYL CHLOROFORMATE
	2746
	6.1
	6.1

+8
	68

	1931
	tert-BUTYLCYCLOHEXYL CHLOROFORMATE
	2747
	6.1
	6.1
	60

	1932
	2-ETHYLHEXYL CHLOROFORMATE
	2748
	6.1
	6.1

+8
	68

	1933
	TETRAMETHYLSILANE
	2749
	3
	3
	33

	1934
	1,3-DICHLOROPROPANOL-2
	2750
	6.1
	6.1
	60

	1935
	DIETHYLTHIO-PHOSPHORYL CHLORIDE
	2751
	8
	8
	80

	1936
	1,2-EPOXY-3-ETHOXYPROPANE
	2752
	3
	3
	30

	1937
	N-ETHYLBENZYL-TOLUIDINES, LIQUID
	2753
	6.1
	6.1
	60

	1938
	N-ETHYLTOLUIDINES
	2754
	6.1
	6.1
	60

	1939
	CARBAMATE PESTICIDE, SOLID, TOXIC
	2757
	6.1
	6.1
	66

	1940
	CARBAMATE PESTICIDE, SOLID, TOXIC
	2757
	6.1
	6.1
	60

	1941
	CARBAMATE PESTICIDE, SOLID, TOXIC
	2757
	6.1
	6.1
	60

	1942
	CARBAMATE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2758
	3
	3

+6.1
	336

	1943
	CARBAMATE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2758
	3
	3

+6.1
	336

	1944
	ARSENICAL PESTICIDE, SOLID. TOXIC
	2759
	6.1
	6.1
	66

	1945
	ARSENICAL PESTICIDE, SOLID. TOXIC
	2759
	6.1
	6.1
	60

	1946
	ARSENICAL PESTICIDE, SOLID. TOXIC
	2759
	6.1
	6.1
	60

	1947
	ARSENICAL PESTICIDE. LIQUID, FLAMMABLE TOXIC, flash-point less than 23 °C
	2760
	3
	3

+6.1
	336

	1948
	ARSENICAL PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2760
	3
	3

+6.1
	336

	1949
	ORGANOCHLORINE PESTICIDE, SOLID, TOXIC
	2761
	6.1
	6.1
	66

	1950
	ORGANOCHLORINE PESTICIDE, SOLID, TOXIC
	2761
	6.1
	6.1
	60

	1951
	ORGANOCHLORINE PESTICIDE, SOLID, TOXIC
	2761
	6.1
	6.1
	60

	1952
	ORGANOCHLORINE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2762
	3
	3

+6.1
	336

	1953
	ORGANOCHLORINE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2762
	3
	3

+6.1
	336

	1954
	TRIAZINE PESTICIDE, SOLID, TOXIC
	2763
	6.1
	6.1
	66

	1955
	TRIAZINE PESTICIDE, SOLID, TOXIC
	2763
	6.1
	6.1
	60

	1956
	TRIAZINE PESTICIDE, SOLID, TOXIC
	2763
	6.1
	6.1
	60

	1957
	TRIAZINE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2764
	3
	3

+6.1
	336

	1958
	TRIAZINE PESTICIDE, LIQUID, FLAMMABLE TOXIC, flash-point less than 23 °C
	2764
	3
	3

+6.1
	336

	1959
	THIOCARBAMATE PESTICIDE, SOLID, TOXIC
	2771
	6.1
	6.1
	66

	1960
	THIOCARBAMATE PESTICIDE, SOLID, TOXIC
	2771
	6.1
	6.1
	60

	1961
	THIOCARBAMATE PESTICIDE, SOLID, TOXIC
	2771
	6.1
	6.1
	60

	1962
	THIOCARBAMATE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2772
	3
	3

+6.1
	336

	1963
	THIOCARBAMATE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2772
	3
	3

+6.1
	336

	1964
	COPPER BASED PESTICIDE, SOLID, TOXIC
	2775
	6.1
	6.1
	66

	1965
	COPPER BASED PESTICIDE, SOLID, TOXIC
	2775
	6.1
	6.1
	60

	1966
	COPPER BASED PESTICIDE, SOLID, TOXIC
	2775
	6.1
	6.1
	60

	1967
	COPPER BASED PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2776
	3
	3

+6.1
	336

	1968
	COPPER BASED PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2776
	3
	3+6.1
	336

	1969
	MERCURY BASED PESTICIDE, SOLID, TOXIC
	2777
	6.1
	6.1
	66

	1970
	MERCURY BASED PESTICIDE, SOLID, TOXIC
	2777
	6.1
	6.1
	60

	1971
	MERCURY BASED PESTICIDE, SOLID, TOXIC
	2777
	6.1
	6.1
	60

	1972
	MERCURY BASED PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2778
	3
	3

+6.1
	336

	1973
	MERCURY BASED PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2778
	3
	3

+6.1
	336

	1974
	SUBSTITUTED NITROPHENOL PESTICIDE, SOLID, TOXIC
	2779
	6.1
	6.1
	66

	1975
	SUBSTITUTED NITROPHENOL PESTICIDE, SOLID, TOXIC
	2779
	6.1
	6.1
	60

	1976
	SUBSTITUTED NITROPHENOL PESTICIDE, SOLID, TOXIC
	2779
	6.1
	6.1
	60

	1977
	SUBSTITUTED NITROPHENOL PESTICIDE, LIQUID, FLAMMABLE TOXIC, flash-point less than 23 °C
	2780
	3
	3

+6.1
	336

	1978
	SUBSTITUTED NITROPHENOL PESTICIDE, LIQUID, FLAMMABLE TOXIC, flash-point less than 23 °C
	2780
	3
	3

+6.1
	336

	1979
	BIPYRIDILIUM PESTICIDE, SOLID, TOXIC
	2781
	6.1
	6.1
	66

	1980
	BIPYRIDILIUM PESTICIDE, SOLID, TOXIC
	2781
	6.1
	6.1
	60

	1981
	BIPYRIDILIUM PESTICIDE, SOLID, TOXIC
	2781
	6.1
	6.1
	60

	1982
	BIPYRIDILIUM PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2782
	3
	3

+6.1
	336

	1983
	BIPYRIDILIUM PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2782
	3
	3

+6.1
	336

	1984
	ORGANOPHOSPHORUS PESTICIDE, SOLID, TOXIC
	2783
	6.1
	6.1
	66

	1985
	ORGANOPHOSPHORUS PESTICIDE, SOLID, TOXIC
	2783
	6.1
	6.1
	60

	1986
	ORGANOPHOSPHORUS PESTICIDE, SOLID, TOXIC
	2783
	6.1
	6.1
	60

	1987
	ORGANOPHOSPHORUS PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2784
	3
	3

+6.1
	336

	1988
	ORGANOPHOSPHORUS PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2784
	3
	3

+6.1
	336

	1989
	4-THIAPENTANAL
	2785
	6.1
	6.1
	60

	1990
	ORGANOTIN PESTICIDE, SOLID, TOXIC
	2786
	6.1
	6.1
	66

	1991
	ORGANOTIN PESTICIDE, SOLID, TOXIC
	2786
	6.1
	6.1
	60

	1992
	ORGANOTIN PESTICIDE, SOLID, TOXIC
	2786
	6.1
	6.1
	60

	1993
	ORGANOTIN PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	2787
	3
	3

+6.1
	336

	1994
	ORGANOTIN PESTICIDE, LIQUID, FLAMMABLE. TOXIC, flash-point less than 23 °C
	2787
	3
	3

+6.1
	336

	1995
	ORGANOTIN COMPOUND, LIQUID, N.O.S.
	2788
	6.1
	6.1
	66

	1996
	ORGANOTIN COMPOUND, LIQUID, N.O.S.
	2788
	6.1
	6.1
	60

	1997
	ORGANOTIN COMPOUND, LIQUID, N.O.S.
	2788
	6.1
	6.1
	60

	1998
	ACETIC ACID, GLACIAL or ACETIC ACID SOLUTION, more than 80% acid, by mass
	2789
	8
	8

+3
	83

	1999
	ACETIC ACID SOLUTION, not less than 50% but not more than 80% acid, by mass
	2790
	8
	8
	80

	2000
	ACETIC ACID SOLUTION, more than 10% and less than 50% acid, by mass
	2790
	8
	8
	80

	2001
	FERROUS METAL BORINGS, SHAVINGS, TURNINGS or CUTTINGS in a form liable to self​heating
	2793
	4.2
	4.2
	40

	2002
	BATTERIES, WET, FILLED WITH ACID, electric storage
	2794
	8
	8
	80

	2003
	BATTERIES, WET, FILLED WITH ALKALI, electric storage
	2795
	8
	8
	80

	2004
	SULPHURIC ACID with not more than 51% acid or BATTERY FLUID, ACID
	2796
	8
	8
	80

	2005
	BATTERY FLUID, ALKALI
	2797
	8
	8
	80

	2006
	PHENYLPHOSPHORUS DICHLORIDE
	2798
	8
	8
	80

	2007
	PHENYLPHOSPHORUS THIODICHLORIDE
	2799
	8
	8
	80

	2008
	BATTERIES, WET, NON-SPILLABLE, electric storage
	2800
	8
	8
	80

	2009
	DYE, LIQUID, CORROSIVE, N.O.S. or DYE INTERMEDIATE, LIQUID, CORROSIVE, N.O.S.
	2801
	8
	8
	88

	2010
	DYE, LIQUID, CORROSIVE, N.O.S. or DYE INTERMEDIATE, LIQUID, CORROSIVE, N.O.S.
	2801
	8
	8
	80

	2011
	DYE, LIQUID. CORROSIVE, N.O.S. or DYE INTERMEDIATE. LIQUID. CORROSIVE, N.O.S.
	2801
	8
	8
	80

	2012
	COPPER CHLORIDE
	2802
	8
	8
	80

	2013
	GALLIUM
	2803
	8
	8
	80

	2014
	LITHIUM HYDRIDE, FUSED SOLID
	2805
	4.3
	4.3
	423

	2015
	LITHIUM NITRIDE
	2806
	4.3
	4.3
	

	2016
	Magnetized material
	2807
	9
	
	

	2017
	MERCURY
	2809
	8
	8

+6.1
	86

	2018
	TOXIC LIQUID, ORGANIC, N.O.S.
	2810
	6.1
	6.1
	66

	2019
	TOXIC LIQUID, ORGANIC, N.O.S.
	2810
	6.1
	6.1
	60

	2020
	TOXIC LIQUID, ORGANIC, N.O.S.
	2810
	6.1
	6.1
	60

	2021
	TOXIC SOLID, ORGANIC, N.O.S.
	2811
	6.1
	6.1
	66

	2022
	TOXIC SOLID, ORGANIC, N.O.S.
	2811
	6.1
	6.1
	60

	2023
	TOXIC SOLID, ORGANIC, N.O.S.
	2811
	6.1
	6.1
	60

	2024
	Sodium aluminate, solid
	2812
	8
	
	

	2025
	WATER-REACTIVE SOLID, N.O.S
	2813
	4.3
	4.3
	X423

	2026
	WATER-REACTIVE SOLID, N.O.S
	2813
	4.3
	4.3
	423

	2027
	WATER-REACTIVE SOLID, N.O.S
	2813
	4.3
	4.3
	423

	2028
	INFECTIOUS SUBSTANCE, AFFECTING HUMANS
	2814
	6.2
	6.2
	

	2029
	INFECTIOUS SUBSTANCE, AFFECTING HUMANS, in refrigerated liquid nitrogen
	2814
	6.2
	6.2

+2.2
	

	2030
	INFECTIOUS SUBSTANCE, AFFECTING HUMANS (animal material only)
	2814
	6.2
	6.2
	606

	2031
	N-AMINOETHYLPIPERAZINE
	2815
	8
	8

+6.1
	86

	2032
	AMMONIUM HYDROGENDIFLUORIDE SOLUTION
	2817
	8
	8

+6.1
	86

	2033
	AMMONIUM HYDROGENDIFLUORIDE SOLUTION
	2817
	8
	8

+6.1
	86

	2034
	AMMONIUM POLYSULPHIDE SOLUTION
	2818
	8
	8

+6.1
	86

	2035
	AMMONIUM POLYSULPHIDE SOLUTION
	2818
	8
	8

+6.1
	86

	2036
	AMYL ACID PHOSPHATE
	2819
	8
	8
	80

	2037
	BUTYRIC ACID
	2820
	8
	8
	80

	2038
	PHENOL SOLUTION
	2821
	6.1
	6.1
	60

	2039
	PHENOL SOLUTION
	2821
	6.1
	6.1
	60

	2040
	2-CHLOROPYRIDINE
	2822
	6.1
	6.1
	60

	2041
	CROTONIC ACID, SOLID
	2823
	8
	8
	80

	2042
	ETHYL CHLOROTHIOFORMATE
	2826
	8
	8

+3
	83

	2043
	CAPROIC ACID
	2829
	8
	8
	80

	2044
	LITHIUM FERROSILICON
	2830
	4.3
	4.3
	423

	2045
	1,1,1-TRICHLOROETHANE
	2831
	6.1
	6.1
	60

	2046
	PHOSPHOROUS ACID
	2834
	8
	8
	80

	2047
	SODIUM ALUMINIUM HYDRIDE
	2835
	4.3
	4.3
	423

	2048
	BISULPHATES, AQUEOUS SOLUTION
	2837
	8
	8
	80

	2049
	BISULPHATES, AQUEOUS SOLUTION
	2837
	8
	8
	80

	2050
	VINYL BUTYRATE, STABILIZED
	2838
	3
	3
	339

	2051
	ALDOL
	2839
	6.1
	6.1
	60

	2052
	BUTYRALDOXIME
	2840
	3
	3
	30

	2053
	DI-n-AMYLAMINE
	2841
	3
	3

+6.1
	36

	2054
	NITROETHANE
	2842
	3
	3
	30

	2055
	CALCIUM MANGANESE SILICON
	2844
	4.3
	4.3
	423

	2056
	PYROPHORIC LIQUID, ORGANIC, N.O.S
	2845
	4.2
	4.2
	333

	2057
	PYROPHORIC SOLID, ORGANIC, NOS.
	2846
	4.2
	4.2
	

	2058
	3-CHLOROPROPANOL-1
	2849
	6.1
	6.1
	60

	2059
	PROPYLENE TETRAMER
	2850
	3
	3
	30

	2060
	BORON TRIFLUORIDE DIHYDRATE
	2851
	8
	8
	80

	2061
	DIPICRYL SULPHIDE, WETTED with not less than 10% water, by mass
	2852
	4.1
	4.1
	

	2062
	MAGNESIUM FLUOROSILICATE
	2853
	6.1
	6.1
	60

	2063
	AMMONIUM FLUOROSILICATE
	2854
	6.1
	6.1
	60

	2064
	ZINC FLUOROSILICATE
	2855
	6.1
	6.1
	60

	2065
	FLUOROSILICATES, N.O.S.
	2856
	6.1
	6.1
	60

	2066
	REFRIGERATING MACHINES containing non-flammable, non​toxic gases or ammonia solutions (UN 2672)
	2857
	2
	2.2
	

	2067
	ZIRCONIUM, DRY, coiled wire, finished metal sheets, strip (thinner than 254 microns but not thinner than 18 microns)
	2858
	4.1
	4.1
	40

	2068
	AMMONIUM METAVANADATE
	2859
	6.1
	6.1
	60

	2069
	AMMONIUM POLYVANADATE
	2861
	6.1
	6.1
	60

	2070
	VANADIUM PENTOXIDE, non​fused form
	2862
	6.1
	6.1
	60

	2071
	SODIUM AMMONIUM VANADATE
	2863
	6.1
	6.1
	60

	2072
	POTASSIUM METAVANADATE
	2864
	6.1
	6.1
	60

	2073
	HYDROXYLAMINE SULPHATE
	2865
	8
	8
	80

	2074
	TITANIUM TRICHLORIDE MIXTURE
	2869
	8
	8
	80

	2075
	TITANIUM TRICHLORIDE MIXTURE
	2869
	8
	8
	80

	2076
	ALUMINIUM BOROHYDRIDE
	2870
	4.2
	4.2

+4.3
	X333

	2077
	ALUMINIUM BOROHYDRIDE IN DEVICES
	2870
	4.2
	4.2

+4.3
	

	2078
	ANTIMONY POWDER
	2871
	6.1
	6.1
	60

	2079
	DIBROMOCHLORO-PROPANES
	2872
	6.1
	6.1
	60

	2080
	DIBROMOCHLORO-PROPANES
	2872
	6.1
	6.1
	60

	2081
	DIBUTYLAMINOETHANOL
	2873
	6.1
	6.1
	60

	2082
	FURFURYL ALCOHOL
	2874
	6.1
	6.1
	60

	2083
	HEXACHLOROPHENE
	2875
	6.1
	6.1
	60

	2084
	RESORCINOL
	2876
	6.1
	6.1
	60

	2085
	TITANIUM SPONGE GRANULES or TITANIUM SPONGE POWDERS
	2878
	4.1
	4.1
	40

	2086
	SELENIUM OXYCHLORIDE
	2879
	8
	8

+6.1
	X886

	2087
	CALCIUM HYPOCHLORITE. HYDRATED, or CALCIUM HYPOCHLORITE, HYDRATED MIXTURE, with not less than 5.5% but not more than 16% water
	2880
	5.1
	5.1
	50

	2088
	CALCIUM HYPOCHLORITE, HYDRATED, or CALCIUM HYPOCHLORITE, HYDRATED MIXTURE, with not less than 5.5% but not more than 16% water
	2880
	5.1
	5.1
	50

	2089
	METAL CATALYST, DRY
	2881
	4.2
	4.2
	43

	2090
	METAL CATALYST, DRY
	2881
	4.2
	4.2
	40

	2091
	METAL CATALYST, DRY
	2881
	4.2
	4.2
	40

	2092
	INFECTIOUS SUBSTANCE, AFFECTING ANIMALS only
	2900
	6.2
	6.2
	

	2093
	INFECTIOUS SUBSTANCE, AFFECTING ANIMALS only, in refrigerated liquid nitrogen
	2900
	6.2
	6.2+2.2
	

	2094
	INFECTIOUS SUBSTANCE, AFFECTING ANIMALS only (animal material only)
	2900
	6.2
	6.2
	606

	2095
	BROMINE CHLORIDE
	2901
	2
	2.3

+5.1

+8
	265

	2096
	PESTICIDE. LIQUID, TOXIC, N.O.S.
	2902
	6.1
	6.1
	66

	2097
	PESTICIDE, LIQUID. TOXIC, N.O.S.
	2902
	6.1
	6.1
	60

	2098
	PESTICIDE, LIQUID, TOXIC, N.O.S
	2902
	6.1
	6.1
	60

	2099
	PESTICIDE, LIQUID, TOXIC, FLAMMABLE, N.O.S., flash-point not less than 23 °C
	2903
	6.1
	6.1

+3
	663

	2100
	PESTICIDE, LIQUID, TOXIC, FLAMMABLE, N.O.S., flash-point not less than 23 °C
	2903
	6.1
	6.1 

+3
	63

	2101
	PESTICIDE, LIQUID, TOXIC, FLAMMABLE, N.O.S., flash-point not less than 23 °C
	2903
	6.1
	6.1

+3
	63

	2102
	CHLOROPHENOLATES, LIQUID or PHENOLATES, LIQUID
	2904
	8
	8
	80

	2103
	CHLOROPHENOLATES, SOLID or PHENOLATES, SOLID
	2905
	8
	8
	80

	2104
	ISOSORBIDE DINITRATE MIXTURE with not less than 60% lactose, mannose, starch or calcium hydrogen phosphate
	2907
	4.1
	4.1
	

	2105
	RADIOACTIVE MATERIAL, EXCEPTED PACKAGE - EMPTY PACKAGING
	2908
	7
	
	

	2106
	RADIOACTIVE MATERIAL. EXCEPTED PACKAGE - ARTICLES MANUFACTURED FROM NATURAL URANIUM or DEPLETED URANIUM or NATURAL THORIUM
	2909
	7
	
	

	2107
	RADIOACTIVE MATERIAL, EXCEPTED PACKAGE - LIMITED QUANTITY OF MATERIAL
	2910
	7
	
	

	2108
	RADIOACTIVE MATERIAL, EXCEPTED PACKAGE INSTRUMENTS or ARTICLES
	2911
	7
	
	

	2109
	RADIOACTIVE MATERIAL. LOW SPECIFIC ACTIVITY (LSA-I), non fissile or fissile-excepted
	2912
	7
	7X
	70

	2110
	RADIOACTIVE MATERIAL, SURFACE CONTAMINATED OBJECTS (SCO-I or SCO-II), non fissile or fissile-excepted
	2913
	7
	7X
	70

	2111
	RADIOACTIVE MATERIAL, TYPE A PACKAGE, non-special form, non fissile or fissile-excepted
	2915
	7
	7X
	70

	2112
	RADIOACTIVE MATERIAL, TYPE B(U) PACKAGE, non fissile or fissile-excepted
	2916
	7
	7X
	70

	2113
	RADIOACTIVE MATERIAL, TYPE B(M) PACKAGE, non fissile or fissile-excepted
	2917
	7
	7X
	70

	2114
	RADIOACTIVE MATERIAL, TRANSPORTED UNDER SPECIAL ARRANGEMENT, non fissile or fissile-excepted
	2919
	7
	7X
	70

	2115
	CORROSIVE LIQUID, FLAMMABLE, N.O.S.
	2920
	8
	8

+3
	883

	2116
	CORROSIVE LIQUID, FLAMMABLE, N.O.S.
	2920
	8
	8

+3
	83

	2117
	CORROSIVE SOLID, FLAMMABLE, N.O.S.
	2921
	8
	8

+4.1
	884

	2118
	CORROSIVE SOLID, FLAMMABLE, N.O.S.
	2921
	8
	8

+4.1
	84

	2119
	CORROSIVE LIQUID, TOXIC, N.O.S.
	2922
	8
	8

+6.1
	886

	2120
	CORROSIVE LIQUID, TOXIC, N.O.S.
	2922
	8
	8

+6.1
	86

	2121
	CORROSIVE LIQUID, TOXIC, N.O.S.
	2922
	8
	8

+6.1
	86

	2122
	CORROSIVE SOLID, TOXIC, N.O.S.
	2923
	8
	8

+6.1
	886

	2123
	CORROSIVE SOLID, TOXIC, N.O.S.
	2923
	8
	8

+6.1
	86

	2124
	CORROSIVE SOLID, TOXIC, N.O.S.
	2923
	8
	8

+6.1
	86

	2125
	FLAMMABLE LIQUID, CORROSIVE, N.O.S.
	2924
	3
	3

+8
	338

	2126
	FLAMMABLE LIQUID, CORROSIVE, N.O.S.
	2924
	3
	3

+8
	338

	2127
	FLAMMABLE LIQUID, CORROSIVE, N.O.S.
	2924
	3
	3

+8
	38

	2128
	FLAMMABLE SOLID, CORROSIVE, ORGANIC, N.O.S.
	2925
	4.1
	4.1

+8
	48

	2129
	FLAMMABLE SOLID, CORROSIVE, ORGANIC, N.O.S.
	2925
	4.1
	4.1

+8
	48

	2130
	FLAMMABLE SOLID, TOXIC, ORGANIC, N.O.S.
	2926
	4.1
	4.1

+6.1
	46

	2131
	FLAMMABLE SOLID, TOXIC, ORGANIC, N.O.S.
	2926
	4.1
	4.1

+6.1
	46

	2132
	TOXIC LIQUID, CORROSIVE, ORGANIC, N.O.S.
	2927
	6.1
	6.1

+8
	668

	2133
	TOXIC LIQUID, CORROSIVE, ORGANIC, N.O.S.
	2927
	6.1
	6.1

+8
	68

	2134
	TOXIC SOLID, CORROSIVE, ORGANIC, N.O.S.
	2928
	6.1
	6.1

+8
	668

	2135
	TOXIC SOLID, CORROSIVE, ORGANIC, N.O.S.
	2928
	6.1
	6.1

+8
	68

	2136
	TOXIC LIQUID, FLAMMABLE, ORGANIC, N.O.S.
	2929
	6.1
	6.1+3
	663

	2137
	TOXIC LIQUID. FLAMMABLE, ORGANIC, N.O.S.
	2929
	6.1
	6.1

+3
	63

	2138
	TOXIC SOLID, FLAMMABLE, ORGANIC, NOS.
	2930
	6.1
	6.1

+4.1
	664

	2139
	TOXIC SOLID. FLAMMABLE, ORGANIC, N.O.S.
	2930
	6.1
	6.1

+4.1
	64

	2140
	VANADYL SULPHATE
	2931
	6.1
	6.1
	60

	2141
	METHYL 2- CHLOROPROPIONATE
	2933
	3
	3
	30

	2142
	ISOPROPYL 2-CHLOROPROPIONATE
	2934
	3
	3
	30

	2143
	ETHYL 2-CHLOROPROPIONATE
	2935
	3
	3
	30

	2144
	THIOLACTIC ACID
	2936
	6.1
	6.1
	60

	2145
	alpha-METHYLBENZYL ALCOHOL, LIQUID
	2937
	6.1
	6.1
	60

	2146
	9-PHOSPHABICYCLO-NONANES (CYCLOOCTADIENE PHOSPHINES)
	2940
	4.2
	4.2
	40

	2147
	FLUOROANILINES
	2941
	6.1
	6.1
	60

	2148
	2-TRIFLUOROMETHYL-ANILINE
	2942
	6.1
	6.1
	60

	2149
	TETRAHYDROFURFURYL​AMINE
	2943
	3
	3
	30

	2150
	N-METHYLBUTYLAMINE
	2945
	3
	3

+8
	338

	2151
	2-AMINO-5-DIETHYLAMINOPENTANE
	2946
	6.1
	6.1
	60

	2152
	ISOPROPYL CHLOROACETATE
	2947
	3
	3
	30

	2153
	3-TRIFLUOROMETHYL-ANILINE
	2948
	6.1
	6.1
	60

	2154
	SODIUM HYDROSULPHIDE, HYDRATED with not less than 25% water of crystallization
	2949
	8
	8
	80

	2155
	MAGNESIUM GRANULES, COATED, particle size not less than 149 microns
	2950
	4.3
	4.3
	423

	2156
	5-tert-BUTYL-2,4,6-TRINITRO-m- XYLENE (MUSK XYLENE)
	2956
	4.1
	4.1
	

	2157
	BORON TRIFLUORIDE DIMETHYL ETHERATE
	2965
	4.3
	4.3

+3

+8
	382

	2158
	THIOGLYCOL
	2966
	6.1
	6.1
	60

	2159
	SULPHAMIC ACID
	2967
	8
	8
	80

	2160
	MANEB, STABILIZED or MANEB PREPARATION, STABILIZED against self-heating
	2968
	4.3
	4.3
	423

	2161
	CASTOR BEANS or CASTOR MEAL or CASTOR POMACE or CASTOR FLAKE
	2969
	9
	9
	90

	2162
	RADIOACTIVE MATERIAL, URANIUM HEXAFLUORIDE, FISSILE
	2977
	7
	7X 

+7E +6.1

+8
	768

	2163
	RADIOACTIVE MATERIAL, URANIUM HEXAFLUORIDE, non fissile or fissile-excepted
	2978
	7
	7X +6.1 +8
	768

	2164
	ETHYLENE OXIDE AND PROPYLENE OXIDE MIXTURE, not more than 30% ethylene oxide
	2983
	3
	3+6.1
	336

	2165
	HYDROGEN PEROXIDE, AQUEOUS SOLUTION with not less than 8% but less than 20% hydrogen peroxide (stabilized as necessary)
	2984
	5.1
	5.1
	50

	2166
	CHLOROSILANES, FLAMMABLE, CORROSIVE, N.O.S.
	2985
	3
	3

+8
	X338

	2167
	CHLOROSILANES, CORROSIVE, FLAMMABLE, N.O.S.
	2986
	8
	8

+3
	X83

	2168
	CHLOROSILANES, CORROSIVE, N.O.S.
	2987
	8
	8
	X80

	2169
	CHLOROSILANES, WATER- REACTIVE, FLAMMABLE, CORROSIVE, N.O.S.
	2988
	4.3
	4.3

+3

+8
	X338

	2170
	LEAD PHOSPHITE. DIBASIC
	2989
	4.1
	4.1
	40

	2171
	LEAD PHOSPHITE, DIBASIC
	2989
	4.1
	4.1
	40

	2172
	LIFE-SAVING APPLIANCES, SELF-INFLATING
	2990
	9
	9
	

	2173
	CARBAMATE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2991
	6.1
	6.1

+3
	663

	2174
	CARBAMATE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2991
	6.1
	6.1

+3
	63

	2175
	CARBAMATE PESTICIDE, LIQUID. TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2991
	6.1
	6.1

+3
	63

	2176
	CARBAMATE PESTICIDE, LIQUID, TOXIC
	2992
	6.1
	6.1
	66

	2177
	CARBAMATE PESTICIDE, LIQUID, TOXIC
	2992
	6.1
	6.1
	60

	2178
	CARBAMATE PESTICIDE, LIQUID, TOXIC
	2992
	6.1
	6.1
	60

	2179
	ARSENICAL PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2993
	6.1
	6.1

+3
	663

	2180
	ARSENICAL PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2993
	6.1
	6.1

+3
	63

	2181
	ARSENICAL PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2993
	6.1
	6.1

+3
	63

	2182
	ARSENICAL PESTICIDE, LIQUID, TOXIC
	2994
	6.1
	6.1
	66

	2183
	ARSENICAL PESTICIDE, LIQUID, TOXIC
	2994
	6.1
	6.1
	60

	2184
	ARSENICAL PESTICIDE, LIQUID, TOXIC
	2994
	6.1
	6.1
	60

	2185
	ORGANOCHLORINE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2995
	6.1
	6.1

+3
	663

	2186
	ORGANOCHLORINE PESTICIDE, LIQUID. TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2995
	6.1
	6.1

+3
	63

	2187
	ORGANOCHLORINE PESTICIDE, LIQUID. TOXIC. FLAMMABLE, flash-point not less than 23 °C
	2995
	6.1
	6.1

+3
	63

	2188
	ORGANOCHLORINE PESTICIDE, LIQUID, TOXIC
	2996
	6.1
	6.1
	66

	2189
	ORGANOCHLORINE PESTICIDE, LIQUID, TOXIC
	2996
	6.1
	6.1
	60

	2190
	ORGANOCHLORINE PESTICIDE, LIQUID. TOXIC
	2996
	6.1
	6.1
	60

	2191
	TRIAZINE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2997
	6.1
	6.1

+3
	663

	2192
	TRIAZINE PESTICIDE. LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2997
	6.1
	6.1

+3
	63

	2193
	TRIAZINE PESTICIDE, LIQUID​TOXIC, FLAMMABLE, flash-point not less than 23 °C
	2997
	6.1
	6.1

+3
	63

	2194
	TRIAZINE PESTICIDE, LIQUID, TOXIC
	2998
	6.1
	6.1
	66

	2195
	TRIAZINE PESTICIDE, LIQUID, TOXIC
	2998
	6.1
	6.1
	60

	2196
	TRIAZINE PESTICIDE, LIQUID, TOXIC
	2998
	6.1
	6.1
	60

	2197
	THIOCARBAMATE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3005
	6.1
	6.1

+3
	663

	2198
	THIOCARBAMATE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3005
	6.1
	6.1

+3
	63

	2199
	THIOCARBAMATE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3005
	6.1
	6.1

+3
	63

	2200
	THIOCARBAMATE PESTICIDE, LIQUID, TOXIC
	3006
	6.1
	6.1
	66

	2201
	THIOCARBAMATE PESTICIDE, LIQUID, TOXIC
	3006
	6.1
	6.1
	60

	2202
	THIOCARBAMATE PESTICIDE, LIQUID, TOXIC
	3006
	6.1
	6.1
	60

	2203
	COPPER BASED PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3009
	6.1
	6.1

+3
	663

	2204
	COPPER BASED PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3009
	6.1
	6.1

+3
	63

	2205
	COPPER BASED PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3009
	6.1
	6.1

+3
	63

	2206
	COPPER BASED PESTICIDE, LIQUID, TOXIC
	3010
	6.1
	6.1
	66

	2207
	COPPER BASED PESTICIDE, LIQUID, TOXIC
	3010
	6.1
	6.1
	60

	2208
	COPPER BASED PESTICIDE, LIQUID, TOXIC
	3010
	6.1
	6.1
	60

	2209
	MERCURY BASED PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3011
	6.1
	6.1

+3
	663

	2210
	MERCURY BASED PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3011
	6.1
	6.1

+3
	63

	2211
	MERCURY BASED PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3011
	6.1
	6.1

+3
	63

	2212
	MERCURY BASED PESTICIDE, LIQUID, TOXIC
	3012
	6.1
	6.1
	66

	2213
	MERCURY BASED PESTICIDE, LIQUID, TOXIC
	3012
	6.1
	6.1
	60

	2214
	MERCURY BASED PESTICIDE, LIQUID, TOXIC
	3012
	6.1
	6.1
	60

	2215
	SUBSTITUTED NITROPHENOL PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3013
	6.1
	6.1

+3
	663

	2216
	SUBSTITUTED NITROPHENOL PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3013
	6.1
	6.1

+3
	63

	2217
	SUBSTITUTED NITROPHENOL PESTICIDE LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3013
	6.1
	6.1

+3
	63

	2218
	SUBSTITUTED NITROPHENOL PESTICIDE, LIQUID, TOXIC
	3014
	6.1
	6.1
	66

	2219
	SUBSTITUTED NITROPHENOL PESTICIDE, LIQUID, TOXIC
	3014
	6.1
	6.1
	60

	2220
	SUBSTITUTED NITROPHENOL PESTICIDE, LIQUID, TOXIC
	3014
	6.1
	6.1
	60

	2221
	BIPYRIDILIUM PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3015
	6.1
	6.1

+3
	663

	2222
	BIPYRIDILIUM PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3015
	6.1
	6.1

+3
	63

	2223
	BIPYRIDILIUM PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3015
	6.1
	6.1

+3
	63

	2224
	BIPYRIDILIUM PESTICIDE, LIQUID, TOXIC
	3016
	6.1
	6.1
	66

	2225
	BIPYRIDILIUM PESTICIDE, LIQUID, TOXIC
	3016
	6.1
	6.1
	60

	2226
	BIPYRIDILIUM PESTICIDE, LIQUID, TOXIC
	3016
	6.1
	6.1
	60

	2227
	ORGANOPHOSPHORUS PESTICIDE LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3017
	6.1
	6.1

+3
	663

	2228
	ORGANOPHOSPHORUS PESTICIDE LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3017
	6.1
	6.1

+3
	63

	2229
	ORGANOPHOSPHORUS PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3017
	6.1
	6.1

+3
	63

	2230
	ORGANOPHOSPHORUS PESTICIDE, LIQUID, TOXIC
	3018
	6.1
	6.1
	66

	2231
	ORGANOPHOSPHORUS PESTICIDE, LIQUID, TOXIC
	3018
	6.1
	6.1
	60

	2232
	ORGANOPHOSPHORUS

PESTICIDE, LIQUID, TOXIC
	3018
	6.1
	6.1
	60

	2233
	ORGANOTIN PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3019
	6.1
	6.1

+3
	663

	2234
	ORGANOTIN PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3019
	6.1
	6.1

+3
	63

	2235
	ORGANOTIN PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3019
	6.1
	6.1

+3
	63

	2236
	ORGANOTIN PESTICIDE, LIQUID, TOXIC
	3020
	6.1
	6.1
	66

	2237
	ORGANOTIN PESTICIDE, LIQUID, TOXIC
	3020
	6.1
	6.1
	60

	2238
	ORGANOTIN PESTICIDE, LIQUID, TOXIC
	3020
	6.1
	6.1
	60

	2239
	PESTICIDE, LIQUID, FLAMMABLE, TOXIC, N.O.S., flash-point less than 23 °C
	3021
	3
	3

+6.1
	336

	2240
	PESTICIDE, LIQUID, FLAMMABLE, TOXIC, N.O.S., flash-point less than 23 °C
	3021
	3
	3

+6.1
	336

	2241
	1,2-BUTYLENE OXIDE, STABILIZED
	3022
	3
	3
	339

	2242
	2-METHYL-2-HEPTANETHIOL
	3023
	6.1
	6.1

+3
	663

	2243
	COUMARIN DERIVATIVE PESTICIDE, LIQUID, FLAMMABLE TOXIC, flash-point less than 23 °C
	3024
	3
	3

+6.1
	336

	2244
	COUMARIN DERIVATIVE PESTICIDE, LIQUID, FLAMMABLE TOXIC, flash-point less than 23 °C
	3024
	3
	3

+6.1
	336

	2245
	COUMARIN DERIVATIVE PESTICIDE LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3025
	6.1
	6.1

+3
	663

	2246
	COUMARIN DERIVATIVE PESTICIDE LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3025
	6.1
	6.1

+3
	63

	2247
	COUMARIN DERIVATIVE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3025
	6.1
	6.1

+3
	63

	2248
	COUMARIN DERIVATIVE PESTICIDE, LIQUID, TOXIC
	3026
	6.1
	6.1
	66

	2249
	COUMARIN DERIVATIVE PESTICIDE, LIQUID, TOXIC
	3026
	6.1
	6.1
	60

	2250
	COUMARIN DERIVATIVE PESTICIDE, LIQUID, TOXIC
	3026
	6.1
	6.1
	60

	2251
	COUMARIN DERIVATIVE PESTICIDE, SOLID, TOXIC
	3027
	6.1
	6.1
	66

	2252
	COUMARIN DERIVATIVE PESTICIDE, SOLID, TOXIC
	3027
	6.1
	6.1
	60

	2253
	COUMARIN DERIVATIVE

PESTICIDE, SOLID, TOXIC
	3027
	6.1
	6.1
	60

	2254
	BATTERIES, DRY, CONTAINING POTASSIUM HYDROXIDE SOLID, electric storage
	3028
	8
	8
	80

	2255
	ALUMINIUM PHOSPHIDE PESTICIDE
	3048
	6.1
	6.1
	642

	2256
	CYCLOHEXYL MERCAPTAN
	3054
	3
	3
	30

	2257
	2-(2-AMINOETHOXY) ETHANOL
	3055
	8
	8
	80

	2258
	n-HEPTALDEHYDE
	3056
	3
	3
	30

	2259
	TRIFLUOROACETYL CHLORIDE
	3057
	2
	2.3

+8
	268

	2260
	NITROGLYCERIN, SOLUTION IN ALCOHOL with more than 1% but not more than 5% nitroglycerin
	3064
	3
	3
	

	2261
	ALCOHOLIC BEVERAGES, with more than 70% alcohol by volume
	3065
	3
	3
	33

	2262
	ALCOHOLIC BEVERAGES, with more than 24% but not more than 70% alcohol by volume
	3065
	3
	3
	30

	2263
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound)
	3066
	8
	8
	80

	2264
	PAINT (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL (including paint thinning and reducing compound)
	3066
	8
	8
	80

	2265
	ETHYLENE OXIDE AND DICHLORODIFLUORO​METHANE MIXTURE with not more than 12.5% ethylene oxide
	3070
	2
	2.2
	20

	2266
	MERCAPTANS, LIQUID, TOXIC, FLAMMABLE, N.O.S. or MERCAPTAN MIXTURE. LIQUID, TOXIC, FLAMMABLE, N.O.S.
	3071
	6.1
	6.1

+3
	63

	2267
	LIFE-SAVING APPLIANCES NOT SELF-INFLATING containing dangerous goods as equipment
	3072
	9
	9
	

	2268
	VINYLPYRIDINES, STABILIZED
	3073
	6.1
	6.1

+3

+8
	638

	2269
	ENVIRONMENTALLY HAZARDOUS SUBSTANCE, SOLID, N.O.S.
	3077
	9
	9
	90

	2270
	CERIUM, turnings or gritty powder
	3078
	4.3
	4.3
	423

	2271
	METHACRYLONITRILE, STABILIZED
	3079
	6.1
	6.1

+3
	663

	2272
	ISOCYANATES, TOXIC, FLAMMABLE, N.O.S. or ISOCYANATE SOLUTION, TOXIC, FLAMMABLE, N.O.S.
	3080
	6.1
	6.1 

+3
	63

	2273
	ENVIRONMENTALLY HAZARDOUS SUBSTANCE, LIQUID, N.O.S.
	3082
	9
	9
	90

	2274
	PERCHLORYL FLUORIDE
	3083
	2
	2.3+5.1
	265

	2275
	CORROSIVE SOLID, OXIDIZING, N.O.S.
	3084
	8
	8

+5.1
	885

	2276
	CORROSIVE SOLID, OXIDIZING, N.O.S.
	3084
	8
	8

+5.1
	85

	2277
	OXIDIZING SOLID, CORROSIVE, N.O.S.
	3085
	5.1
	5.1

+8
	

	2278
	OXIDIZING SOLID, CORROSIVE, N.O.S.
	3085
	5.1
	5.1

+8
	58

	2279
	OXIDIZING SOLID, CORROSIVE, N.O.S.
	3085
	5.1
	5.1

+8
	58

	2280
	TOXIC SOLID, OXIDIZING, N.O.S.
	3086
	6.1
	6.1

+5.1
	665

	2281
	TOXIC SOLID, OXIDIZING, N.O.S.
	3086
	6.1
	6.1

+5.1
	65

	2282
	OXIDIZING SOLID, TOXIC, N.O.S.
	3087
	5.1
	5.1

+6.1
	

	2283
	OXIDIZING SOLID, TOXIC, N.O.S.
	3087
	5.1
	5.1

+6.1
	56

	2284
	OXIDIZING SOLID, TOXIC, N.O.S.
	3087
	5.1
	5.1

+6.1
	56

	2285
	SELF-HEATING SOLID, ORGANIC, N.O.S.
	3088
	4.2
	4.2
	40

	2286
	SELF-HEATING SOLID, ORGANIC, N.O.S.
	3088
	4.2
	4.2
	40

	2287
	METAL POWDER, FLAMMABLE, N.O.S.
	3089
	4.1
	4.1
	40

	2288
	METAL POWDER. FLAMMABLE, N.O.S.
	3089
	4.1
	4.1
	40

	2289
	LITHIUM METAL BATTERIES (including lithium alloy batteries)
	3090
	9
	9A
	

	2290
	LITHIUM METAL BATTERIES CONTAINED IN EQUIPMENT or LITHIUM METAL BATTERIES PACKED WITH EQUIPMENT (including lithium alloy batteries)
	3091
	9
	9A
	

	2291
	1-METHOXY-2-PROPANOL
	3092
	3
	3
	30

	2292
	CORROSIVE LIQUID. OXIDIZING, N.O.S.
	3093
	8
	8

+5.1
	885

	2293
	CORROSIVE LIQUID, OXIDIZING, N.O.S.
	3093
	8
	8

+5.1
	85

	2294
	CORROSIVE LIQUID, WATER- REACTIVE, N.O.S.
	3094
	8
	8

+4.3
	823

	2295
	CORROSIVE LIQUID, WATER- REACTIVE, N.O.S.
	3094
	8
	8

+4.3
	823

	2296
	CORROSIVE SOLID, SELF​HEATING, N.O.S.
	3095
	8
	8

+4.2
	884

	2297
	CORROSIVE SOLID, SELF​HEATING, N.O.S.
	3095
	8
	8

+4.2
	84

	2298
	CORROSIVE SOLID, WATER- REACTIVE, N.O.S.
	3096
	8
	8

+4.3
	842

	2299
	CORROSIVE SOLID, WATER- REACTIVE, N.O.S.
	3096
	8
	8

+4.3
	842

	2300
	FLAMMABLE SOLID, OXIDIZING, N.O.S.
	3097
	4.1
	
	

	2301
	OXIDIZING LIQUID, CORROSIVE, N.O.S.
	3098
	5.1
	5.1

+8
	

	2302
	OXIDIZING LIQUID, CORROSIVE, N.O.S.
	3098
	5.1
	5.1

+8
	

	2303
	OXIDIZING LIQUID, CORROSIVE, N.O.S.
	3098
	5.1
	5.1

+8
	

	2304
	OXIDIZING LIQUID, TOXIC, N.O.S.
	3099
	5.1
	5.1

+6.1
	

	2305
	OXIDIZING LIQUID, TOXIC, N.O.S.
	3099
	5.1
	5.1

+6.1
	

	2306
	OXIDIZING LIQUID, TOXIC, N.O.S.
	3099
	5.1
	5.1

+6.1
	

	2307
	OXIDIZING SOLID, SELF​HEATING, N.O.S.
	3100
	5.1
	
	

	2308
	ORGANIC PEROXIDE TYPE B, LIQUID
	3101
	5.2
	5.2 

+1
	

	2309
	ORGANIC PEROXIDE TYPE B, SOLID
	3102
	5.2
	5.2 

+1
	

	2310
	ORGANIC PEROXIDE TYPE C, LIQUID
	3103
	5.2
	5.2
	

	2311
	ORGANIC PEROXIDE TYPE C, SOLID
	3104
	5.2
	5.2
	

	2312
	ORGANIC PEROXIDE TYPE D, LIQUID
	3105
	5.2
	5.2
	

	2313
	ORGANIC PEROXIDE TYPE D, SOLID
	3106
	5.2
	5.2
	

	2314
	ORGANIC PEROXIDE TYPE E, LIQUID
	3107
	5.2
	5.2
	

	2315
	ORGANIC PEROXIDE TYPE E, SOLID
	3108
	5.2
	5.2
	

	2316
	ORGANIC PEROXIDE TYPE F, LIQUID
	3109
	5.2
	5.2
	539

	2317
	ORGANIC PEROXIDE TYPE F, SOLID
	3110
	5.2
	5.2
	539

	2318
	ORGANIC PEROXIDE TYPE B, LIQUID, TEMPERATURE CONTROLLED
	3111
	5.2
	5.2

+1
	

	2319
	ORGANIC PEROXIDE TYPE B, SOLID, TEMPERATURE CONTROLLED
	3112
	5.2
	5.2

+1
	

	2320
	ORGANIC PEROXIDE TYPE C, LIQUID, TEMPERATURE CONTROLLED
	3113
	5.2
	5.2
	

	2321
	ORGANIC PEROXIDE TYPE C, SOLID, TEMPERATURE CONTROLLED
	3114
	5.2
	5.2
	

	2322
	ORGANIC PEROXIDE TYPE D, LIQUID, TEMPERATURE CONTROLLED
	3115
	5.2
	5.2
	

	2323
	ORGANIC PEROXIDE TYPE D, SOLID, TEMPERATURE CONTROLLED
	3116
	5.2
	5.2
	

	2324
	ORGANIC PEROXIDE TYPE E, LIQUID, TEMPERATURE CONTROLLED
	3117
	5.2
	5.2
	

	2325
	ORGANIC PEROXIDE TYPE E, SOLID, TEMPERATURE CONTROLLED
	3118
	5.2
	5.2
	

	2326
	ORGANIC PEROXIDE TYPE F, LIQUID, TEMPERATURE CONTROLLED
	3119
	5.2
	5.2
	539

	2327
	ORGANIC PEROXIDE TYPE F, SOLID, TEMPERATURE CONTROLLED
	3120
	5.2
	5.2
	539

	2328
	OXIDIZING SOLID, WATER- REACTIVE, N.O.S.
	3121
	5.1
	
	

	2329
	TOXIC LIQUID, OXIDIZING, N.O.S.
	3122
	6.1
	6.1

+5.1
	665

	2330
	TOXIC LIQUID, OXIDIZING, N.O.S.
	3122
	6.1
	6.1

+5.1
	65

	2331
	TOXIC LIQUID, WATER- REACTIVE, N.O.S.
	3123
	6.1
	6.1

+4.3
	623

	2332
	TOXIC LIQUID, WATER- REACTIVE, N.O.S.
	3123
	6.1
	6.1

+4.3
	623

	2333
	TOXIC SOLID, SELF-HEATING, N.O.S.
	3124
	6.1
	6.1

+4.2
	664

	2334
	TOXIC SOLID. SELF-HEATING, N.O.S.
	3124
	6.1
	6.1

+4.2
	64

	2335
	TOXIC SOLID, WATER- REACTIVE, N.O.S.
	3125
	6.1
	6.1

+4.3
	642

	2336
	TOXIC SOLID, WATER- REACTIVE, N.O.S.
	3125
	6.1
	6.1

+4.3
	642

	2337
	SELF-HEATING SOLID, CORROSIVE, ORGANIC, N.O.S.
	3126
	4.2
	4.2

+8
	48

	2338
	SELF-HEATING SOLID, CORROSIVE, ORGANIC, N.O.S.
	3126
	4.2
	4.2

+8
	48

	2339
	SELF-HEATING SOLID, OXIDIZING, N.O.S
	3127
	4.2
	
	

	2340
	SELF-HEATING SOLID, TOXIC, ORGANIC, N.O.S.
	3128
	4.2
	4.2

+6.1
	46

	2341
	SELF-HEATING SOLID. TOXIC, ORGANIC, N.O.S.
	3128
	4.2
	4.2

+6.1
	46

	2342
	WATER-REACTIVE LIQUID, CORROSIVE, N.O.S
	3129
	4.3
	4.3

+8
	X382

	2343
	WATER-REACTIVE LIQUID,

CORROSIVE, N.O.S.
	3129
	4.3
	4.3

+8
	382

	2344
	WATER-REACTIVE LIQUID, CORROSIVE, N.O.S.
	3129
	4.3
	4.3

+8
	382

	2345
	WATER-REACTIVE LIQUID, TOXIC, N.O.S.
	3130
	4.3
	4.3

+6.1
	X362

	2346
	WATER-REACTIVE LIQUID, TOXIC, N.O.S.
	3130
	4.3
	4.3

+6.1
	362

	2347
	WATER-REACTIVE LIQUID, TOXIC, N.O.S.
	3130
	4.3
	4.3+6.1
	362

	2348
	WATER-REACTIVE SOLID, CORROSIVE, N.O.S.
	3131
	4.3
	4.3

+8
	X482

	2349
	WATER-REACTIVE SOLID, CORROSIVE, N.O.S.
	3131
	4.3
	4.3

+8
	482

	2350
	WATER-REACTIVE SOLID, CORROSIVE, N.O.S.
	3131
	4.3
	4.3

+8
	482

	2351
	WATER-REACTIVE SOLID, FLAMMABLE, N.O.S.
	3132
	4.3
	4.3

+4.1
	

	2352
	WATER-REACTIVE SOLID, FLAMMABLE, N.O.S.
	3132
	4.3
	4.3

+4.1
	423

	2353
	WATER-REACTIVE SOLID, FLAMMABLE, N.O.S.
	3132
	4.3
	4.3

+4.1
	423

	2354
	WATER-REACTIVE SOLID, OXIDIZING, N.O.S
	3133
	4.3
	
	

	2355
	WATER-REACTIVE SOLID, TOXIC, N.O.S.
	3134
	4.3
	4.3

+6.1
	

	2356
	WATER-REACTIVE SOLID, TOXIC, N.O.S.
	3134
	4.3
	4.3

+6.1
	462

	2357
	WATER-REACTIVE SOLID, TOXIC, N.O.S.
	3134
	4.3
	4.3

+6.1
	462

	2358
	WATER-REACTIVE SOLID, SELF​-HEATING, N.O.S.
	3135
	4.3
	4.3

+4.2
	

	2359
	WATER-REACTIVE SOLID, SELF-​HEATING, N.O.S.
	3135
	4.3
	4.3

+4.2
	423

	2360
	WATER-REACTIVE SOLID. SELF​-HEATING, N.O.S.
	3135
	4.3
	4.3

+4.2
	423

	2361
	TRIFLUOROMETHANE, REFRIGERATED LIQUID
	3136
	2
	2.2
	22

	2362
	OXIDIZING SOLID, FLAMMABLE, N.O.S.
	3137
	5.1
	
	

	2363
	ETHYLENE. ACETYLENE AND PROPYLENE MIXTURE, REFRIGERATED LIQUID containing at least 71.5% ethylene with not more than 22.5% acetylene and not more than 6% propylene
	3138
	2
	2.1
	223

	2364
	OXIDIZING LIQUID, N.O.S.
	3139
	5.1
	5.1
	

	2365
	OXIDIZING LIQUID, N.O.S.
	3139
	5.1
	5.1
	

	2366
	OXIDIZING LIQUID, N.O.S.
	3139
	5.1
	5.1
	

	2367
	ALKALOIDS, LIQUID, N.O.S. or ALKALOID SALTS, LIQUID, N.O.S.
	3140
	6.1
	6.1
	66

	2368
	ALKALOIDS, LIQUID, N.O.S. or ALKALOID SALTS. LIQUID, N.O.S.
	3140
	6.1
	6.1
	60

	2369
	ALKALOIDS, LIQUID, N.O.S. or ALKALOID SALTS. LIQUID, N.O.S.
	3140
	6.1
	6.1
	60

	2370
	ANTIMONY COMPOUND, INORGANIC. LIQUID, N.O.S.
	3141
	6.1
	6.1
	60

	2371
	DISINFECTANT, LIQUID, TOXIC, N.O.S.
	3142
	6.1
	6.1
	66

	2372
	DISINFECTANT, LIQUID, TOXIC, N.O.S.
	3142
	6.1
	6.1
	60

	2373
	DISINFECTANT, LIQUID, TOXIC, NOS.
	3142
	6.1
	6.1
	60

	2374
	DYE. SOLID. TOXIC, N.O.S. or DYE INTERMEDIATE. SOLID, TOXIC, N.O.S.
	3143
	6.1
	6.1
	66

	2375
	DYE, SOLID, TOXIC, N.O.S. or DYE INTERMEDIATE, SOLID, TOXIC, N.O.S.
	3143
	6.1
	6.1
	60

	2376
	DYE, SOLID. TOXIC, N.O.S. or DYE INTERMEDIATE, SOLID, TOXIC, N.O.S.
	3143
	6.1
	6.1
	60

	2377
	NICOTINE COMPOUND, LIQUID, N.O.S. or NICOTINE PREPARATION, LIQUID, N.O.S.
	3144
	6.1
	6.1
	66

	2378
	NICOTINE COMPOUND, LIQUID, N.O.S. or NICOTINE PREPARATION, LIQUID, N.O.S.
	3144
	6.1
	6.1
	60

	2379
	NICOTINE COMPOUND, LIQUID, N.O.S. or NICOTINE PREPARATION, LIQUID, N.O.S.
	3144
	6.1
	6.1
	60

	2380
	ALKYLPHENOLS, LIQUID, N.O.S, (including C2-C12 homologues)
	3145
	8
	8
	88

	2381
	ALKYLPHENOLS, LIQUID, N.O.S. (including C2-C12 homologues)
	3145
	8
	8
	80

	2382
	ALKYLPHENOLS, LIQUID, N.O.S. (including C2-C12 homologues)
	3145
	8
	8
	80

	2383
	ORGANOTIN COMPOUND, SOLID, N.O.S.
	3146
	6.1
	6.1
	66

	2384
	ORGANOTIN COMPOUND, SOLID, N.O.S.
	3146
	6.1
	6.1
	60

	2385
	ORGANOTIN COMPOUND, SOLID, N.O.S.
	3146
	6.1
	6.1
	60

	2386
	DYE, SOLID, CORROSIVE, N.O.S, or DYE INTERMEDIATE, SOLID, CORROSIVE, N.O.S.
	3147
	8
	8
	88

	2387
	DYE, SOLID. CORROSIVE, N.O.S. or DYE INTERMEDIATE, SOLID, CORROSIVE, N.O.S.
	3147
	8
	8
	80

	2388
	DYE. SOLID. CORROSIVE, N.O.S. or DYE INTERMEDIATE, SOLID, CORROSIVE, N.O.S.
	3147
	8
	8
	80

	2389
	WATER-REACTIVE LIQUID, N.O.S.
	3148
	4.3
	4.3
	X323

	2390
	WATER-REACTIVE LIQUID, N.O.S.
	3148
	4.3
	4.3
	323

	2391
	WATER-REACTIVE LIQUID, N.O.S.
	3148
	4.3
	4.3
	323

	2392
	HYDROGEN PEROXIDE AND PEROXYACETIC ACID MIXTURE with acid(s), water and not more than 5% peroxyacetic acid, STABILIZED
	3149
	5.1
	5.1

+8
	58

	2393
	DEVICES, SMALL, HYDROCARBON GAS POWERED or HYDROCARBON GAS REFILLS FOR SMALL DEVICES with release device
	3150
	2
	2.1
	

	2394
	POLYHALOGENATED BIPHENYLS, LIQUID or HALOGENATED MONOMETHYLDIPHENYLMETH ANES, LIQUID or POLYHALOGENATED TERPHENYLS, LIQUID
	3151
	9
	9
	90

	2395
	POLYHALOGENATED BIPHENYLS, SOLID or HALOGENATED MONOMETHYLDIPHENYLMETH ANES, SOLID or POLYHALOGENATED TERPHENYLS, SOLID
	3152
	9
	9
	90

	2396
	PERFLUORO(METHYL VINYL ETHER)
	3153
	2
	2.1
	23

	2397
	PERFLUORO(ETHYL VINYL ETHER)
	3154
	2
	2.1
	23

	2398
	PENTACHLOROPHENOL
	3155
	6.1
	6.1
	60

	2399
	COMPRESSED GAS. OXIDIZING, NOS.
	3156
	2
	2.2

+5.1
	25

	2400
	LIQUEFIED GAS, OXIDIZING, N.O.S.
	3157
	2
	2.2

+5.1
	25

	2401
	GAS, REFRIGERATED LIQUID, N.O.S.
	3158
	2
	2.2
	22

	2402
	1,1,1,2-TETRAFLUOROETHANE (REFRIGERANT GAS R 134a)
	3159
	2
	2.2
	20

	2403
	LIQUEFIED GAS, TOXIC, FLAMMABLE, N.O.S.
	3160
	2
	2.3

+2.1
	263

	2404
	LIQUEFIED GAS, FLAMMABLE, N.O.S.
	3161
	2
	2.1
	23

	2405
	LIQUEFIED GAS, TOXIC, N.O.S.
	3162
	2
	2.3
	26

	2406
	LIQUEFIED GAS, N.O.S.
	3163
	2
	2.2
	20

	2407
	ARTICLES. PRESSURIZED, PNEUMATIC or HYDRAULIC (containing non-flammable gas)
	3164
	2
	2.2
	

	2408
	AIRCRAFT HYDRAULIC POWER UNIT FUEL TANK (containing a mixture of anhydrous hydrazine and methylhydrazine) (M86 fuel)
	3165
	3
	3

+6.1

+8
	

	2409
	VEHICLE, FLAMMABLE GAS POWERED or VEHICLE, FLAMMABLE LIQUID POWERED or VEHICLE, FUEL CELL, FLAMMABLE GAS POWERED or VEHICLE, FUEL CELL, FLAMMABLE LIQUID POWERED
	3166
	9
	
	

	2410
	GAS SAMPLE, NON​PRESSURIZED, FLAMMABLE, N.O.S., not refrigerated liquid
	3167
	2
	2.1
	

	2411
	GAS SAMPLE, NON​PRESSURIZED, TOXIC, FLAMMABLE, N.O.S., not refrigerated liquid
	3168
	2
	2.3

+2.1
	

	2412
	GAS SAMPLE, NON- PRESSURIZED, TOXIC, N.O.S., not refrigerated liquid
	3169
	2
	2.3
	

	2413
	ALUMINIUM SMELTING BY​PRODUCTS or ALUMINIUM REMELTING BY-PRODUCTS
	3170
	4.3
	4.3
	423

	2414
	ALUMINIUM SMELTING BY​PRODUCTS or ALUMINIUM REMELTING BY-PRODUCTS
	3170
	4.3
	4.3
	423

	2415
	BATTERY POWERED VEHICLE or BATTERY POWERED EQUIPMENT
	3171
	9
	
	

	2416
	TOXINS, EXTRACTED FROM LIVING SOURCES, LIQUID, N.O.S.
	3172
	6.1
	6.1
	66

	2417
	TOXINS, EXTRACTED FROM LIVING SOURCES, LIQUID, N.O.S.
	3172
	6.1
	6.1
	60

	2418
	TOXINS, EXTRACTED FROM LIVING SOURCES, LIQUID, N.O.S.
	3172
	6.1
	6.1
	60

	2419
	TITANIUM DISULPHIDE
	3174
	4.2
	4.2
	40

	2420
	SOLIDS or mixtures of solids (such as preparations and wastes) CONTAINING FLAMMABLE LIQUID, N.O.S. having a flash​point up to 60 °C
	3175
	4.1
	4.1
	40

	2421
	FLAMMABLE SOLID, ORGANIC, MOLTEN, N.O.S.
	3176
	4.1
	4.1
	44

	2422
	FLAMMABLE SOLID, ORGANIC, MOLTEN, N.O.S.
	3176
	4.1
	4.1
	44

	2423
	FLAMMABLE SOLID.

INORGANIC, N.O.S.
	3178
	4.1
	4.1
	40

	2424
	FLAMMABLE SOLID, INORGANIC, N.O.S.
	3178
	4.1
	4.1
	40

	2425
	FLAMMABLE SOLID, TOXIC, INORGANIC, N.O.S.
	3179
	4.1
	4.1+6.1
	46

	2426
	FLAMMABLE SOLID, TOXIC, INORGANIC, N.O.S.
	3179
	4.1
	4.1

+6.1
	46

	2427
	FLAMMABLE SOLID, CORROSIVE, INORGANIC, N.O.S.
	3180
	4.1
	4.1

+8
	48

	2428
	FLAMMABLE SOLID, CORROSIVE, INORGANIC, N.O.S.
	3180
	4.1
	4.1

+8
	48

	2429
	METAL SALTS OF ORGANIC COMPOUNDS, FLAMMABLE, N.O.S.
	3181
	4.1
	4.1
	40

	2430
	METAL SALTS OF ORGANIC COMPOUNDS, FLAMMABLE, N.O.S.
	3181
	4.1
	4.1
	40

	2431
	METAL HYDRIDES, FLAMMABLE, N.O.S.
	3182
	4.1
	4.1
	40

	2432
	METAL HYDRIDES, FLAMMABLE, N.O.S.
	3182
	4.1
	4.1
	40

	2433
	SELF-HEATING LIQUID, ORGANIC, N.O.S.
	3183
	4.2
	4.2
	30

	2434
	SELF-HEATING LIQUID, ORGANIC, N.O.S.
	3183
	4.2
	4.2
	30

	2435
	SELF-HEATING LIQUID, TOXIC, ORGANIC, N.O.S.
	3184
	4.2
	4.2

+6.1
	36

	2436
	SELF-HEATING LIQUID, TOXIC, ORGANIC, N.O.S.
	3184
	4.2
	4.2

+6.1
	36

	2437
	SELF-HEATING LIQUID, CORROSIVE, ORGANIC, N.O.S.
	3185
	4.2
	4.2

+8
	38

	2438
	SELF-HEATING LIQUID, CORROSIVE, ORGANIC, N.O.S.
	3185
	4.2
	4.2

+8
	38

	2439
	SELF-HEATING LIQUID, INORGANIC, N.O.S.
	3186
	4.2
	4.2
	30

	2440
	SELF-HEATING LIQUID, INORGANIC, N.O.S.
	3186
	4.2
	4.2
	30

	2441
	SELF-HEATING LIQUID, TOXIC. INORGANIC, N.O.S.
	3187
	4.2
	4.2

+6.1
	36

	2442
	SELF-HEATING LIQUID, TOXIC, INORGANIC, N.O.S.
	3187
	4.2
	4.2

+6.1
	36

	2443
	SELF-HEATING LIQUID, CORROSIVE, INORGANIC, N.O.S.
	3188
	4.2
	4.2

+8
	38

	2444
	SELF-HEATING LIQUID, CORROSIVE, INORGANIC, N.O.S.
	3188
	4.2
	4.2

+8
	38

	2445
	METAL POWDER, SELF​HEATING, N.O.S.
	3189
	4.2
	4.2
	40

	2446
	METAL POWDER, SELF​HEATING, N.O.S.
	3189
	4.2
	4.2
	40

	2447
	SELF-HEATING SOLID. INORGANIC, N.O.S.
	3190
	4.2
	4.2
	40

	2448
	SELF-HEATING SOLID, INORGANIC, N.O.S.
	3190
	4.2
	4.2
	40

	2449
	SELF-HEATING SOLID, TOXIC, INORGANIC, N.O.S.
	3191
	4.2
	4.2

+6.1
	46

	2450
	SELF-HEATING SOLID, TOXIC, INORGANIC, N.O.S
	3191
	4.2
	4.2

+6.1
	46

	2451
	SELF-HEATING SOLID, CORROSIVE, INORGANIC, N.O.S.
	3192
	4.2
	4.2

+8
	48

	2452
	SELF-HEATING SOLID, CORROSIVE, INORGANIC, N.O.S.
	3192
	4.2
	4.2+8
	48

	2453
	PYROPHORIC LIQUID, INORGANIC, N.O.S.
	3194
	4.2
	4.2
	333

	2454
	PYROPHORIC SOLID, INORGANIC, N.O.S.
	3200
	4.2
	4.2
	43

	2455
	ALKALINE EARTH METAL ALCOHOLATES, N.O.S.
	3205
	4.2
	4.2
	40

	2456
	ALKALINE EARTH METAL ALCOHOLATES, N.O.S.
	3205
	4.2
	4.2
	40

	2457
	ALKALI METAL ALCOHOLATES, SELF-HEATING, CORROSIVE, N.O.S.
	3206
	4.2
	4.2

+8
	48

	2458
	ALKALI METAL ALCOHOLATES, SELF-HEATING, CORROSIVE, N.O.S.
	3206
	4.2
	4.2

+8
	48

	2459
	METALLIC SUBSTANCE, WATER-REACTIVE, N.O.S.
	3208
	4.3
	4.3
	

	2460
	METALLIC SUBSTANCE, WATER-REACTIVE, N.O.S.
	3208
	4.3
	4.3
	423

	2461
	METALLIC SUBSTANCE, WATER-REACTIVE, N.O.S.
	3208
	4.3
	4.3
	423

	2462
	METALLIC SUBSTANCE, WATER-REACTIVE, SELF​HEATING, N.O.S.
	3209
	4.3
	4.3

+4.2
	

	2463
	METALLIC SUBSTANCE, WATER-REACTIVE, SELF​HEATING, N.O.S.
	3209
	4.3
	4.3

+4.2
	423

	2464
	METALLIC SUBSTANCE, WATER-REACTIVE, SELF​HEATING, N.O.S.
	3209
	4.3
	4.3

+4.2
	423

	2465
	CHLORATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3210
	5.1
	5.1
	50

	2466
	CHLORATES. INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3210
	5.1
	5.1
	50

	2467
	PERCHLORATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3211
	5.1
	5.1
	50

	2468
	PERCHLORATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3211
	5.1
	5.1
	50

	2469
	HYPOCHLORITES, INORGANIC, N.O.S.
	3212
	5.1
	5.1
	50

	2470
	BROMATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3213
	5.1
	5.1
	50

	2471
	BROMATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3213
	5.1
	5.1
	50

	2472
	PERMANGANATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3214
	5.1
	5.1
	50

	2473
	PERSULPHATES, INORGANIC, N.O.S.
	3215
	5.1
	5.1
	50

	2474
	PERSULPHATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3216
	5.1
	5.1
	50

	2475
	NITRATES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3218
	5.1
	5.1
	50

	2476
	NITRATES. INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3218
	5.1
	5.1
	50

	2477
	NITRITES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3219
	5.1
	5.1
	50

	2478
	NITRITES, INORGANIC, AQUEOUS SOLUTION, N.O.S.
	3219
	5.1
	5.1
	50

	2479
	PENTAFLUOROETHANE (REFRIGERANT GAS R 125)
	3220
	2
	2.2
	20

	2480
	SELF-REACTIVE LIQUID TYPE B
	3221
	4.1
	4.1

+1
	

	2481
	SELF-REACTIVE SOLID TYPE B
	3222
	4.1
	4.1

+1
	

	2482
	SELF-REACTIVE LIQUID TYPE C
	3223
	4.1
	4.1
	

	2483
	SELF-REACTIVE SOLID TYPE C
	3224
	4.1
	4.1
	

	2484
	SELF-REACTIVE LIQUID TYPE D
	3225
	4.1
	4.1
	

	2485
	SELF-REACTIVE SOLID TYPE D
	3226
	4.1
	4.1
	

	2486
	SELF-REACTIVE LIQUID TYPE E
	3227
	4.1
	4.1
	

	2487
	SELF-REACTIVE SOLID TYPE E
	3228
	4.1
	4.1
	

	2488
	SELF-REACTIVE LIQUID TYPE F
	3229
	4.1
	4.1
	40

	2489
	SELF-REACTIVE SOLID TYPE F
	3230
	4.1
	4.1
	40

	2490
	SELF-REACTIVE LIQUID TYPE B, TEMPERATURE CONTROLLED
	3231
	4.1
	4.1

+1
	

	2491
	SELF-REACTIVE SOLID TYPE B, TEMPERATURE CONTROLLED
	3232
	4.1
	4.1

+1
	

	2492
	SELF-REACTIVE LIQUID TYPE C, TEMPERATURE CONTROLLED
	3233
	4.1
	4.1
	

	2493
	SELF-REACTIVE SOLID TYPE C, TEMPERATURE CONTROLLED
	3234
	4.1
	4.1
	

	2494
	SELF-REACTIVE LIQUID TYPE D, TEMPERATURE CONTROLLED
	3235
	4.1
	4.1
	

	2495
	SELF-REACTIVE SOLID TYPE D, TEMPERATURE CONTROLLED
	3236
	4.1
	4.1
	

	2496
	SELF-REACTIVE LIQUID TYPE E, TEMPERATURE CONTROLLED
	3237
	4.1
	4.1
	

	2497
	SELF-REACTIVE SOLID TYPE E, TEMPERATURE CONTROLLED
	3238
	4.1
	4.1
	

	2498
	SELF-REACTIVE LIQUID TYPE F, TEMPERATURE CONTROLLED
	3239
	4.1
	4.1
	40

	2499
	SELF-REACTIVE SOLID TYPE F, TEMPERATURE CONTROLLED
	3240
	4.1
	4.1
	40

	2500
	2-BROMO-2-NITROPROPANE-1,3- DIOL
	3241
	4.1
	4.1
	

	2501
	AZODICARBONAMIDE
	3242
	4.1
	4.1
	40

	2502
	SOLIDS CONTAINING TOXIC LIQUID, N.O.S.
	3243
	6.1
	6.1
	60

	2503
	SOLIDS CONTAINING CORROSIVE LIQUID, N.O.S.
	3244
	8
	8
	80

	2504
	GENETICALLY MODIFIED MICROORGANISMS or GENETICALLY MODIFIED ORGANISMS
	3245
	9
	9
	

	2505
	GENETICALLY MODIFIED MICROORGANISMS or GENETICALLY MODIFIED ORGANISMS, in refrigerated liquid nitrogen
	3245
	9
	9

+2.2
	

	2506
	METHANESULPHONYL CHLORIDE
	3246
	6.1
	6.1

+8
	668

	2507
	SODIUM PEROXOBORATE, ANHYDROUS
	3247
	5.1
	5.1
	50

	2508
	MEDICINE, LIQUID, FLAMMABLE, TOXIC, N.O.S.
	3248
	3
	3

+6.1
	336

	2509
	MEDICINE, LIQUID, FLAMMABLE, TOXIC, N.O.S.
	3248
	3
	3

+6.1
	36

	2510
	MEDICINE, SOLID, TOXIC, N.O.S.
	3249
	6.1
	6.1
	60

	2511
	MEDICINE, SOLID, TOXIC, N.O.S.
	3249
	6.1
	6.1
	60

	2512
	CHLOROACETIC ACID, MOLTEN
	3250
	6.1
	6.1

+8
	68

	2513
	ISOSORBIDE-5-MONONITRATE
	3251
	4.1
	4.1
	

	2514
	DIFLUOROMETHANE (REFRIGERANT GAS R 32)
	3252
	2
	2.1
	23

	2515
	DISODIUM TRIOXOSILICATE
	3253
	8
	8
	80

	2516
	TRIBUTYLPHOSPHANE
	3254
	4.2
	4.2
	333

	2517
	tert-BUTYL HYPOCHLORITE
	3255
	4.2
	
	

	2518
	ELEVATED TEMPERATURE LIQUID, FLAMMABLE, N.O.S. with flashpoint above 60° C, at or above its flashpoint and below 100° C
	3256
	3
	3
	30

	2519
	ELEVATED TEMPERATURE LIQUID, FLAMMABLE, N.O.S. with flashpoint above 60° C, at or above its flashpoint and at or above 100° C
	3256
	3
	3
	30

	2520
	ELEVATED TEMPERATURE LIQUID, N.O.S., at or above 100 °C and below its flash-point (including molten metals, molten salts, etc.), filled at a temperature higher than 190 °C
	3257
	9
	9
	99

	2521
	ELEVATED TEMPERATURE LIQUID, N.O.S., at or above 100 °C and below its flash-point (including molten metals, molten salts, etc.), filled at or below 190 °C
	3257
	9
	9
	99

	2522
	ELEVATED TEMPERATURE SOLID, N.O.S., at or above 240 °C
	3258
	9
	9
	99

	2523
	AMINES, SOLID, CORROSIVE, N.O.S. or POLYAMINES, SOLID, CORROSIVE, N.O.S.
	3259
	8
	8
	88

	2524
	AMINES, SOLID, CORROSIVE, N.O.S. or POLYAMINES, SOLID, CORROSIVE, N.O.S.
	3259
	8
	8
	80

	2525
	AMINES, SOLID, CORROSIVE, N.O.S. or POLYAMINES, SOLID, CORROSIVE, N.O.S.
	3259
	8
	8
	80

	2526
	CORROSIVE SOLID, ACIDIC, INORGANIC, N.O.S.
	3260
	8
	8
	88

	2527
	CORROSIVE SOLID, ACIDIC, INORGANIC, N.O.S.
	3260
	8
	8
	80

	2528
	CORROSIVE SOLID, ACIDIC, INORGANIC, N.O.S.
	3260
	8
	8
	80

	2529
	CORROSIVE SOLID, ACIDIC, ORGANIC, N.O.S.
	3261
	8
	8
	88

	2530
	CORROSIVE SOLID, ACIDIC, ORGANIC, N.O.S.
	3261
	8
	8
	80

	2531
	CORROSIVE SOLID, ACIDIC, ORGANIC, N.O.S.
	3261
	8
	8
	80

	2532
	CORROSIVE SOLID, BASIC, INORGANIC, N.O.S.
	3262
	8
	8
	88

	2533
	CORROSIVE SOLID, BASIC, INORGANIC, N.O.S.
	3262
	8
	8
	80

	2534
	CORROSIVE SOLID, BASIC, INORGANIC, N.O.S.
	3262
	8
	8
	80

	2535
	CORROSIVE SOLID, BASIC, ORGANIC, N.O.S.
	3263
	8
	8
	88

	2536
	CORROSIVE SOLID, BASIC, ORGANIC, N.O.S.
	3263
	8
	8
	80

	2537
	CORROSIVE SOLID, BASIC, ORGANIC, N.O.S.
	3263
	8
	8
	80

	2538
	CORROSIVE LIQUID, ACIDIC, INORGANIC, N.O.S.
	3264
	8
	8
	88

	2539
	CORROSIVE LIQUID, ACIDIC, INORGANIC, N.O.S.
	3264
	8
	8
	80

	2540
	CORROSIVE LIQUID, ACIDIC, INORGANIC, N.O.S.
	3264
	8
	8
	80

	2541
	CORROSIVE LIQUID, ACIDIC, ORGANIC, N.O.S.
	3265
	8
	8
	88

	2542
	CORROSIVE LIQUID, ACIDIC, ORGANIC, N.O.S.
	3265
	8
	8
	80

	2543
	CORROSIVE LIQUID, ACIDIC, ORGANIC, N.O.S.
	3265
	8
	8
	80

	2544
	CORROSIVE LIQUID, BASIC, INORGANIC, N.O.S.
	3266
	8
	8
	88

	2545
	CORROSIVE LIQUID, BASIC, INORGANIC, N.O.S.
	3266
	8
	8
	80

	2546
	CORROSIVE LIQUID, BASIC, INORGANIC, N.O.S.
	3266
	8
	8
	80

	2547
	CORROSIVE LIQUID, BASIC, ORGANIC, N.O.S.
	3267
	8
	8
	88

	2548
	CORROSIVE LIQUID, BASIC, ORGANIC, N.O.S.
	3267
	8
	8
	80

	2549
	CORROSIVE LIQUID, BASIC, ORGANIC, N.O.S.
	3267
	8
	8
	80

	2550
	SAFETY DEVICES, electrically initiated
	3268
	9
	9
	

	2551
	POLYESTER RESIN KIT, liquid base material
	3269
	3
	3
	

	2552
	POLYESTER RESIN KIT, liquid base material
	3269
	3
	3
	

	2553
	NITROCELLULOSE MEMBRANE FILTERS, with not more than 12.6% nitrogen, by dry mass
	3270
	4.1
	4.1
	

	2554
	ETHERS, N.O.S.
	3271
	3
	3
	33

	2555
	ETHERS, N.O.S.
	3271
	3
	3
	30

	2556
	ESTERS, N.O.S.
	3272
	3
	3
	33

	2557
	ESTERS, N.O.S.
	3272
	3
	3
	30

	2558
	NITRILES, FLAMMABLE, TOXIC, N.O.S.
	3273
	3
	3

+6.1
	336

	2559
	NITRILES, FLAMMABLE, TOXIC, N.O.S.
	3273
	3
	3

6.1
	336

	2560
	ALCOHOLATES SOLUTION, N.O.S., in alcohol
	3274
	3
	3

+8
	338

	2561
	NITRILES, TOXIC, FLAMMABLE, N.O.S.
	3275
	6.1
	6.1

+3
	663

	2562
	NITRILES, TOXIC, FLAMMABLE, N.O.S.
	3275
	6.1
	6.1

+3
	63

	2563
	NITRILES, LIQUID, TOXIC, N.O.S.
	3276
	6.1
	6.1
	66

	2564
	NITRILES, LIQUID, TOXIC, N.O.S.
	3276
	6.1
	6.1
	60

	2565
	NITRILES, LIQUID, TOXIC, N.O.S.
	3276
	6.1
	6.1
	60

	2566
	CHLOROFORMATES, TOXIC, CORROSIVE, N.O.S.
	3277
	6.1
	6.1

+8
	68

	2567
	ORGANOPHOSPHORUS COMPOUND, LIQUID, TOXIC, N.O.S.
	3278
	6.1
	6.1
	66

	2568
	ORGANOPHOSPHORUS COMPOUND, LIQUID, TOXIC, N.O.S.
	3278
	6.1
	6.1
	60

	2569
	ORGANOPHOSPHORUS COMPOUND, LIQUID, TOXIC, N.O.S.
	3278
	6.1
	6.1
	60

	2570
	ORGANOPHOSPHORUS COMPOUND, TOXIC, FLAMMABLE, N.O.S.
	3279
	6.1
	6.1

+3
	663

	2571
	ORGANOPHOSPHORUS COMPOUND, TOXIC, FLAMMABLE, N.O.S.
	3279
	6.1
	6.1

+3
	63

	2572
	ORGANOARSENIC COMPOUND, LIQUID, N.O.S.
	3280
	6.1
	6.1
	66

	2573
	ORGANOARSENIC COMPOUND, LIQUID, N.O.S.
	3280
	6.1
	6.1
	60

	2574
	ORGANOARSENIC COMPOUND, LIQUID, N.O.S.
	3280
	6.1
	6.1
	60

	2575
	METAL CARBONYLS, LIQUID, N.O.S.
	3281
	6.1
	6.1
	66

	2576
	METAL CARBONYLS, LIQUID, N.O.S.
	3281
	6.1
	6.1
	60

	2577
	METAL CARBONYLS, LIQUID, N.O.S.
	3281
	6.1
	6.1
	60

	2578
	ORGANOMETALLIC COMPOUND, LIQUID, TOXIC, N.O.S.
	3282
	6.1
	6.1
	66

	2579
	ORGANOMETALLIC COMPOUND, LIQUID, TOXIC, N.O.S.
	3282
	6.1
	6.1
	60

	2580
	ORGANOMETALLIC COMPOUND, LIQUID, TOXIC, N.O.S.
	3282
	6.1
	6.1
	60

	2581
	SELENIUM COMPOUND, SOLID, N.O.S.
	3283
	6.1
	6.1
	66

	2582
	SELENIUM COMPOUND, SOLID, N.O.S.
	3283
	6.1
	6.1
	60

	2583
	SELENIUM COMPOUND, SOLID, N.O.S.
	3283
	6.1
	6.1
	60

	2584
	TELLURIUM COMPOUND, N.O.S.
	3284
	6.1
	6.1
	66

	2585
	TELLURIUM COMPOUND, N.O.S.
	3284
	6.1
	6.1
	60

	2586
	TELLURIUM COMPOUND, N.O.S.
	3284
	6.1
	6.1
	60

	2587
	VANADIUM COMPOUND, N.O.S.
	3285
	6.1
	6.1
	66

	2588
	VANADIUM COMPOUND, N.O.S.
	3285
	6.1
	6.1
	60

	2589
	VANADIUM COMPOUND, N.O.S.
	3285
	6.1
	6.1
	60

	2590
	FLAMMABLE LIQUID, TOXIC, CORROSIVE, N.O.S.
	3286
	3
	3

+6.1

+8
	368

	2591
	FLAMMABLE LIQUID, TOXIC, CORROSIVE, N.O.S.
	3286
	3
	3

+6.1

+8
	368

	2592
	TOXIC LIQUID, INORGANIC, N.O.S.
	3287
	6.1
	6.1
	66

	2593
	TOXIC LIQUID, INORGANIC, N.O.S.
	3287
	6.1
	6.1
	60

	2594
	TOXIC LIQUID, INORGANIC, N.O.S.
	3287
	6.1
	6.1
	60

	2595
	TOXIC SOLID, INORGANIC, N.O.S.
	3288
	6.1
	6.1
	66

	2596
	TOXIC SOLID, INORGANIC, N.O.S.
	3288
	6.1
	6.1
	60

	2597
	TOXIC SOLID, INORGANIC, N.O.S.
	3288
	6.1
	6.1
	60

	2598
	TOXIC LIQUID, CORROSIVE, INORGANIC, N.O.S.
	3289
	6.1
	6.1

+8
	668

	2599
	TOXIC LIQUID, CORROSIVE, INORGANIC, N.O.S.
	3289
	6.1
	6.1

+8
	68

	2600
	TOXIC SOLID, CORROSIVE, INORGANIC, N.O.S.
	3290
	6.1
	6.1

+8
	668

	2601
	TOXIC SOLID, CORROSIVE, INORGANIC, N.O.S.
	3290
	6.1
	6.1

+8
	68

	2602
	CLINICAL WASTE, UNSPECIFIED, N.O.S. or (BIO) MEDICAL WASTE, N.O.S. or REGULATED MEDICAL WASTE, N.O.S.
	3291
	6.2
	6.2
	606

	2603
	CLINICAL WASTE, UNSPECIFIED, N.O.S. or (BIO) MEDICAL WASTE, N.O.S. or REGULATED MEDICAL WASTE, N.O.S., in refrigerated liquid nitrogen
	3291
	6.2
	6.2

+2.2
	

	2604
	BATTERIES, CONTAINING SODIUM, or CELLS, CONTAINING SODIUM
	3292
	4.3
	4.3
	

	2605
	HYDRAZINE, AQUEOUS SOLUTION with not more than 37% hydrazine, by mass
	3293
	6.1
	6.1
	60

	2606
	HYDROGEN CYANIDE, SOLUTION IN ALCOHOL with not more than 45% hydrogen cyanide
	3294
	6.1
	6.1

+3
	663

	2607
	HYDROCARBONS, LIQUID, N.O.S.
	3295
	3
	3
	33

	2608
	HYDROCARBONS, LIQUID, N.O.S. (vapour pressure at 50 °C more than 110 kPa)
	3295
	3
	3
	33

	2609
	HYDROCARBONS, LIQUID, N.O.S. (vapour pressure at 50 °C not more than 110 kPa)
	3295
	3
	3
	33

	2610
	HYDROCARBONS, LIQUID, N.O.S.
	3295
	3
	3
	30

	2611
	HEPTAFLUOROPROPANE (REFRIGERANT GAS R 227)
	3296
	2
	2.2
	20

	2612
	ETHYLENE OXIDE AND CHLOROTETRAFLUORO- ETHANE MIXTURE with not more than 8.8% ethylene oxide
	3297
	2
	2.2
	20

	2613
	ETHYLENE OXIDE AND PENTAFLUOROETHANE MIXTURE with not more than 7.9% ethylene oxide
	3298
	2
	2.2
	20

	2614
	ETHYLENE OXIDE AND TETRAFLUOROETHANE MIXTURE with not more than 5.6% ethylene oxide
	3299
	2
	2.2
	20

	2615
	ETHYLENE OXIDE AND CARBON DIOXIDE MIXTURE with more than 87% ethylene oxide
	3300
	2
	2.3

+2.1
	263

	2616
	CORROSIVE LIQUID, SELF- HEATING, N.O.S.
	3301
	8
	8

+4.2
	884

	2617
	CORROSIVE LIQUID, SELF- HEATING, N.O.S.
	3301
	8
	8

+4.2
	84

	2618
	2-DIMETHYLAMINOETHYL ACRYLATE
	3302
	6.1
	6.1
	60

	2619
	COMPRESSED GAS, TOXIC, OXIDIZING, N.O.S.
	3303
	2
	2.3

+5.1
	265

	2620
	COMPRESSED GAS, TOXIC, CORROSIVE, N.O.S
	3304
	2
	2.3

+8
	268

	2621
	COMPRESSED GAS, TOXIC, FLAMMABLE, CORROSIVE, N.O.S.
	3305
	2
	2.3

+2.1

+8
	263

	2622
	COMPRESSED GAS, TOXIC, OXIDIZING, CORROSIVE, N.O.S.
	3306
	2
	2.3

+5.1

+8
	265

	2623
	LIQUEFIED GAS, TOXIC, OXIDIZING, N.O.S.
	3307
	2
	2.3

+5.1
	265

	2624
	LIQUEFIED GAS, TOXIC, CORROSIVE, N.O.S.
	3308
	2
	2.3

+8
	268

	2625
	LIQUEFIED GAS, TOXIC, FLAMMABLE, CORROSIVE, N.O.S.
	3309
	2
	2.3

+2.1

+8
	263

	2626
	LIQUEFIED GAS, TOXIC, OXIDIZING, CORROSIVE, N.O.S.
	3310
	2
	2.3

+5.1

+8
	265

	2627
	GAS, REFRIGERATED LIQUID, OXIDIZING, N.O.S.
	3311
	2
	2.2

+5.1
	225

	2628
	GAS, REFRIGERATED LIQUID, FLAMMABLE, N.O.S.
	3312
	2
	2.1
	223

	2629
	ORGANIC PIGMENTS, SELF- HEATING
	3313
	4.2
	4.2
	40

	2630
	ORGANIC PIGMENTS, SELF- HEATING
	3313
	4.2
	4.2
	40

	2631
	PLASTICS MOULDING COMPOUND in dough, sheet or extruded rope form evolving flammable vapour
	3314
	9
	None
	90

	2632
	CHEMICAL SAMPLE, TOXIC
	3315
	6.1
	6.1
	

	2633
	CHEMICAL KIT or FIRST AID KIT
	3316
	9
	9
	

	2634
	CHEMICAL KIT or FIRST AID KIT
	3316
	9
	9
	

	2635
	2-AMINO-4,6-DINITROPHENOL, WETTED with not less than 20% water, by mass
	3317
	4.1
	4.1
	

	2636
	AMMONIA SOLUTION, relative density less than 0.880 at 15 °C in water, with more than 50% ammonia
	3318
	2
	2.3

+8
	268

	2637
	NITROGLYCERIN MIXTURE, DESENSITIZED, SOLID, N.O.S. with more than 2% but not more than 10% nitroglycerin, by mass
	3319
	4.1
	4.1
	

	2638
	SODIUM BOROHYDRIDE AND SODIUM HYDROXIDE SOLUTION, with not more than 12% sodium borohydride and not more than 40% sodium hydroxide by mass
	3320
	8
	8
	80

	2639
	SODIUM BOROHYDRIDE AND SODIUM HYDROXIDE SOLUTION, with not more than 12% sodium borohydride and not more than 40% sodium hydroxide by mass
	3320
	8
	8
	80

	2640
	RADIOACTIVE MATERIAL, LOW SPECIFIC ACTIVITY (LSA-II), non fissile or fissile-excepted
	3321
	7
	7X
	70

	2641
	RADIOACTIVE MATERIAL, LOW SPECIFIC ACTIVITY (LSA-III), non fissile or fissile-excepted
	3322
	7
	7X
	70

	2642
	RADIOACTIVE MATERIAL, TYPE C PACKAGE, non fissile or fissile-excepted
	3323
	7
	7X
	70

	2643
	RADIOACTIVE MATERIAL, LOW SPECIFIC ACTIVITY (LSA-II), FISSILE
	3324
	7
	7X

+7E
	70

	2644
	RADIOACTIVE MATERIAL, LOW SPECIFIC ACTIVITY, (LSA-III), FISSILE
	3325
	7
	7X

+7E
	70

	2645
	RADIOACTIVE MATERIAL, SURFACE CONTAMINATED OBJECTS (SCO-I or SCO-II), FISSILE
	3326
	7
	7X

+7E
	70

	2646
	RADIOACTIVE MATERIAL, TYPE A PACKAGE, FISSILE, non- special form
	3327
	7
	7X

+7E
	70

	2647
	RADIOACTIVE MATERIAL, TYPE B(U) PACKAGE, FISSILE
	3328
	7
	7X

+7E
	70

	2648
	RADIOACTIVE MATERIAL, TYPE B(M) PACKAGE, FISSILE
	3329
	7
	7X+7E
	70

	2649
	RADIOACTIVE MATERIAL, TYPE C PACKAGE, FISSILE
	3330
	7
	7X

+7E
	70

	2650
	RADIOACTIVE MATERIAL, TRANSPORTED UNDER SPECIAL ARRANGEMENT, FISSILE
	3331
	7
	7X

+7E
	70

	2651
	RADIOACTIVE MATERIAL, TYPE A PACKAGE, SPECIAL FORM, non fissile or fissile-excepted
	3332
	7
	7X
	70

	2652
	RADIOACTIVE MATERIAL, TYPE A PACKAGE, SPECIAL FORM, FISSILE
	3333
	7
	7X

+7E
	70

	2653
	Aviation regulated liquid, n.o.s.
	3334
	9
	
	

	2654
	Aviation regulated solid, n.o.s.
	3335
	9
	
	

	2655
	MERCAPTANS, LIQUID, FLAMMABLE, N.O.S. or MERCAPTAN MIXTURE, LIQUID, FLAMMABLE, N.O.S.
	3336
	3
	3
	33

	2656
	MERCAPTANS, LIQUID, FLAMMABLE, N.O.S. or MERCAPTAN MIXTURE, LIQUID, FLAMMABLE, N.O.S. (vapour pressure at 50 °C more than 110 kPa)
	3336
	3
	3
	33

	2657
	MERCAPTANS, LIQUID, FLAMMABLE, N.O.S. or MERCAPTAN MIXTURE, LIQUID, FLAMMABLE, N.O.S. (vapour pressure at 50 °C not more than 110 kPa)
	3336
	3
	3
	33

	2658
	MERCAPTANS, LIQUID, FLAMMABLE, N.O.S. or MERCAPTAN MIXTURE, LIQUID, FLAMMABLE, N.O.S.
	3336
	3
	3
	30

	2659
	REFRIGERANT GAS R 404A (Pentafluoroethane, 1,1,1- trifluoroethane, and 1,1,1,2- tetrafluoroethane zeotropic mixture with approximately 44% pentafluoroethane and 52% 1,1,1- trifluoroethane)
	3337
	2
	2.2
	20

	2660
	REFRIGERANT GAS R 407A (Difluoromethane, pentafluoroethane, and 1,1,1,2-tetrafluoroethane zeotropic mixture with approximately 20% difluoromethane and 40% pentafluoroethane)
	3338
	2
	2.2
	20

	2661
	REFRIGERANT GAS R 407B (Difluoromethane, pentafluoroethane, and 1,1,1,2-tetrafluoroethane zeotropic mixture with approximately 10% difluoromethane and 70% pentafluoroethane)
	3339
	2
	2.2
	20

	2662
	REFRIGERANT GAS R 407C (Difluoromethane, pentafluoroethane, and 1,1,1,2-tetrafluoroethane zeotropic mixture with approximately 23%difluoromethane and 25% pentafluoroethane)
	3340
	2
	2.2
	20

	2663
	THIOUREA DIOXIDE
	3341
	4.2
	4.2
	40

	2664
	THIOUREA DIOXIDE
	3341
	4.2
	4.2
	40

	2665
	XANTHATES
	3342
	4.2
	4.2
	40

	2666
	XANTHATES
	3342
	4.2
	4.2
	40

	2667
	NITROGLYCERIN MIXTURE, DESENSITIZED, LIQUID, FLAMMABLE, N.O.S. with not more than 30% nitroglycerin, by mass
	3343
	3
	3
	

	2668
	PENTAERYTHRITE TETRANITRATE (PENTAERYTHRITOL TETRANITRATE; PETN) MIXTURE, DESENSITIZED, SOLID, N.O.S. with more than 10% but not more than 20% PETN, by mass
	3344
	4.1
	4.1
	

	2669
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, SOLID, TOXIC
	3345
	6.1
	6.1
	66

	2670
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, SOLID, TOXIC
	3345
	6.1
	6.1
	60

	2671
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, SOLID, TOXIC
	3345
	6.1
	6.1
	60

	2672
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	3346
	3
	3

+6.1
	336

	2673
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	3346
	3
	3

+6.1
	336

	2674
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3347
	6.1
	6.1

+3
	663

	2675
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3347
	6.1
	6.1

+3
	63

	2676
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3347
	6.1
	6.1+3
	63

	2677
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, TOXIC
	3348
	6.1
	6.1
	66

	2678
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, TOXIC
	3348
	6.1
	6.1
	60

	2679
	PHENOXYACETIC ACID DERIVATIVE PESTICIDE, LIQUID, TOXIC
	3348
	6.1
	6.1
	60

	2680
	PYRETHROID PESTICIDE, SOLID, TOXIC
	3349
	6.1
	6.1
	66

	2681
	PYRETHROID PESTICIDE, SOLID, TOXIC
	3349
	6.1
	6.1
	60

	2682
	PYRETHROID PESTICIDE, SOLID, TOXIC
	3349
	6.1
	6.1
	60

	2683
	PYRETHROID PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	3350
	3
	3

+6.1
	336

	2684
	PYRETHROID PESTICIDE, LIQUID, FLAMMABLE, TOXIC, flash-point less than 23 °C
	3350
	3
	3

+6.1
	336

	2685
	PYRETHROID PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3351
	6.1
	6.1

+3
	663

	2686
	PYRETHROID PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3351
	6.1
	6.1

+3
	63

	2687
	PYRETHROID PESTICIDE, LIQUID, TOXIC, FLAMMABLE, flash-point not less than 23 °C
	3351
	6.1
	6.1

+3
	63

	2688
	PYRETHROID PESTICIDE, LIQUID, TOXIC
	3352
	6.1
	6.1
	66

	2689
	PYRETHROID PESTICIDE, LIQUID, TOXIC
	3352
	6.1
	6.1
	60

	2690
	PYRETHROID PESTICIDE, LIQUID, TOXIC
	3352
	6.1
	6.1
	60

	2691
	INSECTICIDE GAS, FLAMMABLE, N.O.S.
	3354
	2
	2.1
	23

	2692
	INSECTICIDE GAS, TOXIC, FLAMMABLE, N.O.S.
	3355
	2
	2.3

+2.1
	263

	2693
	OXYGEN GENERATOR, CHEMICAL
	3356
	5.1
	5.1
	

	2694
	NITROGLYCERIN MIXTURE, DESENSITIZED, LIQUID, N.O.S. with not more than 30% nitroglycerin, by mass
	3357
	3
	3
	

	2695
	REFRIGERATING MACHINES containing flammable, non-toxic, liquefied gas
	3358
	2
	2.1
	

	2696
	FUMIGATED CARGO TRANSPORT UNIT
	3359
	9
	
	

	2697
	Fibres, vegetable, dry
	3360
	4.1
	
	

	2698
	CHLOROSILANES, TOXIC, CORROSIVE, N.O.S.
	3361
	6.1
	6.1

+8
	68

	2699
	CHLOROSILANES, TOXIC, CORROSIVE, FLAMMABLE, N.O.S.
	3362
	6.1
	6.1

+3

+8
	638

	2700
	Dangerous goods in machinery or dangerous goods in apparatus
	3363
	9
	
	

	2701
	TRINITROPHENOL (PICRIC ACID), WETTED with not less than 10% water, by mass
	3364
	4.1
	4.1
	

	2702
	TRINITROCHLOROBENZENE (PICRYL CHLORIDE), WETTED with not less than 10% water, by mass
	3365
	4.1
	4.1
	

	2703
	TRINITROTOLUENE (TNT), WETTED with not less than 10% water, by mass
	3366
	4.1
	4.1
	

	2704
	TRINITROBENZENE, WETTED with not less than 10% water, by mass
	3367
	4.1
	4.1
	

	2705
	TRINITROBENZOIC ACID, WETTED with not less than 10% water, by mass
	3368
	4.1
	4.1
	

	2706
	SODIUM DINITRO-o- CRESOLATE, WETTED with not less than 10% water, by mass
	3369
	4.1
	4.1

+6.1
	

	2707
	UREA NITRATE, WETTED with not less than 10% water, by mass
	3370
	4.1
	4.1
	

	2708
	2 –METHYLBUTANAL
	3371
	3
	3
	33

	2709
	BIOLOGICAL SUBSTANCE, CATEGORY B
	3373
	6.2
	6.2
	606

	2710
	BIOLOGICAL SUBSTANCE, CATEGORY B (animal material only)
	3373
	6.2
	6.2
	606

	2711
	ACETYLENE, SOLVENT FREE
	3374
	2
	2.1
	

	2712
	AMMONIUM NITRATE EMULSION or SUSPENSION or GEL, intermediate for blasting explosives, liquid
	3375
	5.1
	5.1
	50

	2713
	AMMONIUM NITRATE EMULSION or SUSPENSION or GEL, intermediate for blasting explosives, solid
	3375
	5.1
	5.1
	50

	2714
	4-NITROPHENYL-HYDRAZINE, with not less than 30% water, by mass
	3376
	4.1
	4.1
	

	2715
	SODIUM PERBORATE MONOHYDRATE
	3377
	5.1
	5.1
	50

	2716
	SODIUM CARBONATE PEROXYHYDRATE
	3378
	5.1
	5.1
	50

	2717
	SODIUM CARBONATE PEROXYHYDRATE
	3378
	5.1
	5.1
	50

	2718
	DESENSITIZED EXPLOSIVE, LIQUID, N.O.S.
	3379
	3
	3
	

	2719
	DESENSITIZED EXPLOSIVE, SOLID, N.O.S.
	3380
	4.1
	4.1
	

	2720
	TOXIC BY INHALATION LIQUID, N.O.S. with an LC50 lower than or equal to 200 ml/m³ and saturated vapour concentration greater than or equal to 500 LC50
	3381
	6.1
	6.1
	66

	2721
	TOXIC BY INHALATION LIQUID, N.O.S. with an LC50 lower than or equal to 1000 ml/m³ and saturated vapour concentration greater than or equal to 10 LC50
	3382
	6.1
	6.1
	66

	2722
	TOXIC BY INHALATION LIQUID, FLAMMABLE, N.O.S. with an LC50 lower than or equal to 200 ml/m³ and saturated vapour concentration greater than or equal to 500 LC50
	3383
	6.1
	6.1

+3
	663

	2723
	TOXIC BY INHALATION LIQUID, FLAMMABLE, N.O.S. with with an LC50 lower than or equal to 1000 ml/m³ and saturated vapour concentration greater than or equal to 10 LC50
	3384
	6.1
	6.1

+3
	663

	2724
	TOXIC BY INHALATION LIQUID, WATER-REACTIVE, N.O.S. with an LC50 lower than or equal to 200 ml/m³ and saturated vapour concentration greater than or equal to 500 LC50
	3385
	6.1
	6.1

+4.3
	623

	2725
	TOXIC BY INHALATION LIQUID, WATER-REACTIVE, N.O.S. with an LC50 lower than or equal to 1000 ml/m³ and saturated vapour concentration greater than or equal to 10 LC50
	3386
	6.1
	6.1

+4.3
	623

	2726
	TOXIC BY INHALATION LIQUID, OXIDIZING, N.O.S.with an LC50 lower than or equal to 200 ml/m³ and saturated vapour concentration greater than or equal to 500 LC50
	3387
	6.1
	6.1

+5.1
	665

	2727
	TOXIC BY INHALATION LIQUID, OXIDIZING, N.O.S. with an LC50 lower than or equal to 1000 ml/m³ and saturated vapour concentration greater than or equal to 10 LC50
	3388
	6.1
	6.1

+5.1
	665

	2728
	TOXIC BY INHALATION LIQUID, CORROSIVE, N.O.S. with an LC50 lower than or equal to 200 ml/m³ and saturated vapour concentration greater than or equal to 500 LC50
	3389
	6.1
	6.1

+8
	668

	2729
	TOXIC BY INHALATION LIQUID, CORROSIVE, N.O.S. with an LC50 lower than or equal to 1000 ml/m³ and saturated vapour concentration greater than or equal to 10 LC50
	3390
	6.1
	6.1

+8
	668

	2730
	ORGANOMETALLIC SUBSTANCE, SOLID, PYROPHORIC
	3391
	4.2
	4.2
	43

	2731
	ORGANOMETALLIC SUBSTANCE, LIQUID, PYROPHORIC
	3392
	4.2
	4.2
	333

	2732
	ORGANOMETALLIC SUBSTANCE, SOLID, PYROPHORIC, WATER- REACTIVE
	3393
	4.2
	4.2

+4.3
	X432

	2733
	ORGANOMETALLIC SUBSTANCE, LIQUID, PYROPHORIC, WATER- REACTIVE
	3394
	4.2
	4.2

+4.3
	X333

	2734
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE
	3395
	4.3
	4.3
	X423

	2735
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE
	3395
	4.3
	4.3
	423

	2736
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE
	3395
	4.3
	4.3
	423

	2737
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE, FLAMMABLE
	3396
	4.3
	4.3

+4.1
	X423

	2738
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE, FLAMMABLE
	3396
	4.3
	4.3

+4.1
	423

	2739
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE, FLAMMABLE
	3396
	4.3
	4.3

+4.1
	423

	2740
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE, SELF-HEATING
	3397
	4.3
	4.3

+4.2
	X423

	2741
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE, SELF-HEATING
	3397
	4.3
	4.3+4.2
	423

	2742
	ORGANOMETALLIC SUBSTANCE, SOLID, WATER- REACTIVE, SELF-HEATING
	3397
	4.3
	4.3

+4.2
	423

	2743
	ORGANOMETALLIC SUBSTANCE, LIQUID, WATER- REACTIVE
	3398
	4.3
	4.3
	X323

	2744
	ORGANOMETALLIC SUBSTANCE, LIQUID, WATER- REACTIVE
	3398
	4.3
	4.3
	323

	2745
	ORGANOMETALLIC SUBSTANCE, LIQUID, WATER- REACTIVE
	3398
	4.3
	4.3
	323

	2746
	ORGANOMETALLIC SUBSTANCE, LIQUID, WATER- REACTIVE, FLAMMABLE
	3399
	4.3
	4.3

+3
	X323

	2747
	ORGANOMETALLIC SUBSTANCE, LIQUID, WATER- REACTIVE, FLAMMABLE
	3399
	4.3
	4.3

+3
	323

	2748
	ORGANOMETALLIC SUBSTANCE, LIQUID, WATER- REACTIVE, FLAMMABLE
	3399
	4.3
	4.3

+3
	323

	2749
	ORGANOMETALLIC SUBSTANCE, SOLID, SELF- HEATING
	3400
	4.2
	4.2
	40

	2750
	ORGANOMETALLIC SUBSTANCE, SOLID, SELF- HEATING
	3400
	4.2
	4.2
	40

	2751
	ALKALI METAL AMALGAM, SOLID
	3401
	4.3
	4.3
	X423

	2752
	ALKALINE EARTH METAL AMALGAM, SOLID
	3402
	4.3
	4.3
	X423

	2753
	POTASSIUM METAL ALLOYS, SOLID
	3403
	4.3
	4.3
	X423

	2754
	POTASSIUM SODIUM ALLOYS, SOLID
	3404
	4.3
	4.3
	X423

	2755
	BARIUM CHLORATE SOLUTION
	3405
	5.1
	5.1

+6.1
	56

	2756
	BARIUM CHLORATE SOLUTION
	3405
	5.1
	5.1

+6.1
	56

	2757
	BARIUM PERCHLORATE SOLUTION
	3406
	5.1
	5.1

+6.1
	56

	2758
	BARIUM PERCHLORATE SOLUTION
	3406
	5.1
	5.1

+6.1
	56

	2759
	CHLORATE AND MAGNESIUM CHLORIDE MIXTURE SOLUTION
	3407
	5.1
	5.1
	50

	2760
	CHLORATE AND MAGNESIUM CHLORIDE MIXTURE SOLUTION
	3407
	5.1
	5.1
	50

	2761
	LEAD PERCHLORATE SOLUTION
	3408
	5.1
	5.1+6.1
	56

	2762
	LEAD PERCHLORATE SOLUTION
	3408
	5.1
	5.1

+6.1
	56

	2763
	CHLORONITROBENZENES, LIQUID
	3409
	6.1
	6.1
	60

	2764
	4-CHLORO-o-TOLUIDINE HYDROCHLORIDE SOLUTION
	3410
	6.1
	6.1
	60

	2765
	beta-NAPHTHYLAMINE SOLUTION
	3411
	6.1
	6.1
	60

	2766
	beta-NAPHTHYLAMINE SOLUTION
	3411
	6.1
	6.1
	60

	2767
	FORMIC ACID with not less than 10% but not more than 85% acid by mass
	3412
	8
	8
	80

	2768
	FORMIC ACID with not less than 5% but less than 10% acid by mass
	3412
	8
	8
	80

	2769
	POTASSIUM CYANIDE SOLUTION
	3413
	6.1
	6.1
	66

	2770
	POTASSIUM CYANIDE SOLUTION
	3413
	6.1
	6.1
	60

	2771
	POTASSIUM CYANIDE SOLUTION
	3413
	6.1
	6.1
	60

	2772
	SODIUM CYANIDE SOLUTION
	3414
	6.1
	6.1
	66

	2773
	SODIUM CYANIDE SOLUTION
	3414
	6.1
	6.1
	60

	2774
	SODIUM CYANIDE SOLUTION
	3414
	6.1
	6.1
	60

	2775
	SODIUM FLUORIDE SOLUTION
	3415
	6.1
	6.1
	60

	2776
	CHLOROACETO-PHENONE, LIQUID
	3416
	6.1
	6.1
	60

	2777
	XYLYL BROMIDE, SOLID
	3417
	6.1
	6.1
	60

	2778
	2,4-TOLUYLENEDIAMINE SOLUTION
	3418
	6.1
	6.1
	60

	2779
	BORON TRIFLUORIDE ACETIC ACID COMPLEX, SOLID
	3419
	8
	8
	80

	2780
	BORON TRIFLUORIDE PROPIONIC ACID COMPLEX, SOLID
	3420
	8
	8
	80

	2781
	POTASSIUM HYDROGENDIFLUORIDE SOLUTION
	3421
	8
	8

+6.1
	86

	2782
	POTASSIUM HYDROGENDIFLUORIDE SOLUTION
	3421
	8
	8

+6.1
	86

	2783
	POTASSIUM FLUORIDE SOLUTION
	3422
	6.1
	6.1
	60

	2784
	TETRAMETHYL-AMMONIUM HYDROXIDE, SOLID
	3423
	8
	8
	80

	2785
	AMMONIUM DINITRO-o-CRESOLATE SOLUTION
	3424
	6.1
	6.1
	60

	2786
	AMMONIUM DINITRO-o-CRESOLATE SOLUTION
	3424
	6.1
	6.1
	60

	2787
	BROMOACETIC ACID, SOLID
	3425
	8
	8
	80

	2788
	ACRYLAMIDE SOLUTION
	3426
	6.1
	6.1
	60

	2789
	CHLOROBENZYL CHLORIDES, SOLID
	3427
	6.1
	6.1
	60

	2790
	3-CHLORO-4-METHYLPHENYL ISOCYANATE, SOLID
	3428
	6.1
	6.1
	60

	2791
	CHLOROTOLUIDINES, LIQUID
	3429
	6.1
	6.1
	60

	2792
	XYLENOLS, LIQUID
	3430
	6.1
	6.1
	60

	2793
	NITROBENZO-TRIFLUORIDES, SOLID
	3431
	6.1
	6.1
	60

	2794
	POLYCHLORINATED BIPHENYLS, SOLID
	3432
	9
	9
	90

	2795
	NITROCRESOLS, LIQUID
	3434
	6.1
	6.1
	60

	2796
	HEXAFLUOROACETONE HYDRATE, SOLID
	3436
	6.1
	6.1
	60

	2797
	CHLOROCRESOLS, SOLID
	3437
	6.1
	6.1
	60

	2798
	alpha-METHYLBENZYL ALCOHOL, SOLID
	3438
	6.1
	6.1
	60

	2799
	NITRILES. SOLID, TOXIC, N.O.S.
	3439
	6.1
	6.1
	66

	2800
	NITRILES, SOLID, TOXIC, N.O.S.
	3439
	6.1
	6.1
	60

	2801
	NITRILES, SOLID, TOXIC, N.O.S.
	3439
	6.1
	6.1
	60

	2802
	SELENIUM COMPOUND. LIQUID, N.O.S.
	3440
	6.1
	6.1
	66

	2803
	SELENIUM COMPOUND, LIQUID, N.O.S.
	3440
	6.1
	6.1
	60

	2804
	SELENIUM COMPOUND. LIQUID, N.O.S.
	3440
	6.1
	6.1
	60

	2805
	CHLORODINITROBENZENES, SOLID
	3441
	6.1
	6.1
	60

	2806
	DICHLOROANILINES, SOLID
	3442
	6.1
	6.1
	60

	2807
	DINITROBENZENES, SOLID
	3443
	6.1
	6.1
	60

	2808
	NICOTINE HYDROCHLORIDE, SOLID
	3444
	6.1
	6.1
	60

	2809
	NICOTINE SULPHATE, SOLID
	3445
	6.1
	6.1
	60

	2810
	NITROTOLUENES, SOLID
	3446
	6.1
	6.1
	60

	2811
	NITROXYLENES. SOLID
	3447
	6.1
	6.1
	60

	2812
	TEAR GAS SUBSTANCE, SOLID, N.O.S.
	3448
	6.1
	6.1
	66

	2813
	TEAR GAS SUBSTANCE, SOLID, N.O.S.
	3448
	6.1
	6.1
	60

	2814
	BROMOBENZYL CYANIDES, SOLID
	3449
	6.1
	6.1
	66

	2815
	DIPHENYLCHLORO-ARSINE, SOLID
	3450
	6.1
	6.1
	66

	2816
	TOLUIDINES, SOLID
	3451
	6.1
	6.1
	60

	2817
	XYLIDINES, SOLID
	3452
	6.1
	6.1
	60

	2818
	PHOSPHORIC ACID, SOLID
	3453
	8
	8
	80

	2819
	DINITROTOLUENES, SOLID
	3454
	6.1
	6.1
	60

	2820
	CRESOLS, SOLID
	3455
	6.1
	6.1

+8
	68

	2821
	NITROSYLSULPHURIC ACID, SOLID
	3456
	8
	8
	X80

	2822
	CHLORONITROTOLUENES. SOLID
	3457
	6.1
	6.1
	60

	2823
	NITROANISOLES, SOLID
	3458
	6.1
	6.1
	60

	2824
	NITROBROMOBENZENES, SOLID
	3459
	6.1
	6.1
	60

	2825
	N-ETHYLBENZYL-TOLUIDINES, SOLID
	3460
	6.1
	6.1
	60

	2826
	TOXINS, EXTRACTED FROM LIVING SOURCES. SOLID, N.O.S.
	3462
	6.1
	6.1
	66

	2827
	TOXINS. EXTRACTED FROM LIVING SOURCES, SOLID, N.O.S.
	3462
	6.1
	6.1
	60

	2828
	TOXINS, EXTRACTED FROM LIVING SOURCES, SOLID, N.O.S
	3462
	6.1
	6.1
	60

	2829
	PROPIONIC ACID with not less than 90% acid by mass
	3463
	8
	8 

+3
	83

	2830
	ORGANOPHOSPHORUS COMPOUND, SOLID, TOXIC, N.O.S.
	3464
	6.1
	6.1
	66

	2831
	ORGANOPHOSPHORUS COMPOUND, SOLID. TOXIC, N.O.S.
	3464
	6.1
	6.1
	60

	2832
	ORGANOPHOSPHORUS COMPOUND, SOLID, TOXIC, N.O.S.
	3464
	6.1
	6.1
	60

	2833
	ORGANOARSENIC COMPOUND, SOLID, N.O.S.
	3465
	6.1
	6.1
	66

	2834
	ORGANOARSENIC COMPOUND, SOLID, N.O.S.
	3465
	6.1
	6.1
	60

	2835
	ORGANOARSENIC COMPOUND, SOLID, N.O.S.
	3465
	6.1
	6.1
	60

	2836
	METAL CARBONYLS, SOLID, N.O.S.
	3466
	6.1
	6.1
	66

	2837
	METAL CARBONYLS, SOLID, N.O.S.
	3466
	6.1
	6.1
	60

	2838
	METAL CARBONYLS, SOLID, N.O.S.
	3466
	6.1
	6.1
	60

	2839
	ORGANOMETALLIC COMPOUND, SOLID, TOXIC, NOS.
	3467
	6.1
	6.1
	66

	2840
	ORGANOMETALLIC COMPOUND, SOLID, TOXIC, NOS.
	3467
	6.1
	6.1
	60

	2841
	ORGANOMETALLIC

COMPOUND, SOLID, TOXIC, N.O.S.
	3467
	6.1
	6.1
	60

	2842
	HYDROGEN IN A METAL HYDRIDE STORAGE SYSTEM or HYDROGEN IN A METAL HYDRIDE STORAGE SYSTEM CONTAINED IN EQUIPMENT or HYDROGEN IN A METAL HYDRIDE STORAGE SYSTEM PACKED WITH EQUIPMENT
	3468
	2
	2.1
	

	2843
	PAINT FLAMMABLE, CORROSIVE (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL, FLAMMABLE, CORROSIVE (including paint thinning and reducing compound)
	3469
	3
	3+8
	338

	2844
	PAINT, FLAMMABLE, CORROSIVE (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL, FLAMMABLE, CORROSIVE (including paint thinning and reducing compound)
	3469
	3
	3

+8
	338

	2845
	PAINT, FLAMMABLE. CORROSIVE (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL, FLAMMABLE, CORROSIVE (including paint thinning and reducing compound)
	3469
	3
	3 

+8
	38

	2846
	PAINT, CORROSIVE, FLAMMABLE (including paint, lacquer, enamel, stain, shellac, varnish, polish, liquid filler and liquid lacquer base) or PAINT RELATED MATERIAL, CORROSIVE, FLAMMABLE (including paint thinning and reducing compound)
	3470
	8
	8 

+3
	83

	2847
	HYDROGENDIFLUORIDES SOLUTION, N.O.S.
	3471
	8
	8

+6.1
	86

	2848
	HYDROGENDIFLUORIDES SOLUTION, N.O.S.
	3471
	8
	8

+6.1
	86

	2849
	CROTONIC ACID, LIQUID
	3472
	8
	8
	80

	2850
	FUEL CELL CARTRIDGES or FUEL CELL CARTRIDGES CONTAINED IN EQUIPMENT or FUEL CELL CARTRIDGES PACKED WITH EQUIPMENT containing flammable liquids
	3473
	3
	3
	

	2851
	1-HYDROXYBENZOTRIAZOLE MONOHYDRATE
	3474
	4.1
	4.1
	

	2852
	ETHANOL AND GASOLINE MIXTURE or ETHANOL AND MOTOR SPIRIT MIXTURE or ETHANOL AND PETROL MIXTURE, with more than 10% ethanol
	3475
	3
	3
	33

	2853
	FUEL CELL CARTRIDGES or FUEL CELL CARTRIDGES CONTAINED IN EQUIPMENT or FUEL CELL CARTRIDGES PACKED WITH EQUIPMENT, containing water-reactive substances
	3476
	4.3
	4.3
	

	2854
	FUEL CELL CARTRIDGES or FUEL CELL CARTRIDGES CONTAINED IN EQUIPMENT or FUEL CELL CARTRIDGES PACKED WITH EQUIPMENT, containing corrosive substances
	3477
	8
	8
	

	2855
	FUEL CELL CARTRIDGES or FUEL CELL CARTRIDGES CONTAINED IN EQUIPMENT or FUEL CELL CARTRIDGES PACKED WITH EQUIPMENT, containing liquefied flammable gas
	3478
	2
	2.1
	

	2856
	FUEL CELL CARTRIDGES or FUEL CELL CARTRIDGES CONTAINED IN EQUIPMENT or FUEL CELL CARTRIDGES PACKED WITH EQUIPMENT, containing hydrogen in metal hydride
	3479
	2
	2.1
	

	2857
	LITHIUM ION BATTERIES (including lithium ion polymer batteries)
	3480
	9
	9A
	

	2858
	LITHIUM ION BATTERIES CONTAINED IN EQUIPMENT or LITHIUM ION BATTERIES PACKED WITH EQUIPMENT (including lithium ion polymer batteries)
	3481
	9
	9A
	

	2859
	ALKALI METAL DISPERSION. FLAMMABLE or ALKALINE EARTH METAL DISPERSION, FLAMMABLE
	3482
	4.3
	4.3

+3
	X323

	2860
	MOTOR FUEL ANTI-KNOCK MIXTURE, FLAMMABLE
	3483
	6.1
	6.1

+3
	663

	2861
	HYDRAZINE AQUEOUS SOLUTION, FLAMMABLE with more than 37% hydrazine, by mass
	3484
	8
	8

+3

+6.1
	886

	2862
	CALCIUM HYPOCHLORITE, DRY. CORROSIVE or CALCIUM HYPOCHLORITE MIXTURE, DRY, CORROSIVE with more than 39% available chlorine (8.8% available oxygen)
	3485
	5.1
	5.1

+8
	58

	2863
	CALCIUM HYPOCHLORITE MIXTURE. DRY, CORROSIVE with more than 10% but not more than 39% available chlorine
	3486
	5.1
	5.1

+8
	58

	2864
	CALCIUM HYPOCHLORITE, HYDRATED. CORROSIVE or CALCIUM HYPOCHLORITE, HYDRATED MIXTURE, CORROSIVE with not less than 5.5% but not more than 16% water
	3487
	5.1
	5.1+8
	58

	2865
	CALCIUM HYPOCHLORITE, HYDRATED, CORROSIVE or CALCIUM HYPOCHLORITE, HYDRATED MIXTURE, CORROSIVE with not less than 5,5% but not more than 16% water
	3487
	5.1
	5.1

+8
	58

	2866
	TOXIC BY INHALATION LIQUID, FLAMMABLE, CORROSIVE, N.O.S. with an LC50 lower than or equal to 200 ml/m3 and saturated vapour concentration greater than or equal to 500 LC50
	3488
	6.1
	6.1

+3

+8
	663

	2867
	TOXIC BY INHALATION LIQUID, FLAMMABLE, CORROSIVE, N.O.S. with an LC50 lower than or equal to 1000 ml/m3 and saturated vapour concentration greater than or equal to 10 LC50
	3489
	6.1
	6.1

+3

+8
	663

	2868
	TOXIC BY INHALATION LIQUID, WATER-REACTIVE, FLAMMABLE, N.O.S. with an LC50 lower than or equal to 200 ml/m3 and saturated vapour concentration greater than or equal to 500 LC50
	3490
	6.1
	6.1

+3

+4.3
	623

	2869
	TOXIC BY INHALATION LIQUID, WATER-REACTIVE, FLAMMABLE, N.O.S. with an LC50 lower than or equal to 1000 ml/m3 and saturated vapour concentration greater than or equal to 10 LC50
	3491
	6.1
	6.1

+3

+4.3
	623

	2870
	PETROLEUM SOUR CRUDE OIL, FLAMMABLE, TOXIC
	3494
	3
	3

+6.1
	336

	2871
	PETROLEUM SOUR CRUDE OIL, FLAMMABLE, TOXIC
	3494
	3
	3

+6.1
	336

	2872
	PETROLEUM SOUR CRUDE OIL, FLAMMABLE, TOXIC
	3494
	3
	3

+6.1
	36

	2873
	IODINE
	3495
	8
	8

+6.1
	86

	2874
	Batteries, nickel-metal hydride
	3496
	9
	
	

	2875
	KRILL MEAL
	3497
	4.2
	4.2
	40

	2876
	KRILL MEAL
	3497
	4.2
	4.2
	40

	2877
	IODINE MONOCHLORIDE, LIQUID
	3498
	8
	8
	80

	2878
	CAPACITOR, ELECTRIC DOUBLE LAYER (with an energy storage capacity greater than 0.3Wh)
	3499
	9
	9
	

	2879
	CHEMICAL UNDER PRESSURE, N.O.S.
	3500
	2
	2.2
	20

	2880
	CHEMICAL UNDER PRESSURE, FLAMMABLE, N.O.S.
	3501
	2
	2.1
	23

	2881
	CHEMICAL UNDER PRESSURE, TOXIC, N.O.S.
	3502
	2
	2.2

+6.1
	26

	2882
	CHEMICAL UNDER PRESSURE, CORROSIVE, N.O.S.
	3503
	2
	2.2

+8
	28

	2883
	CHEMICAL UNDER PRESSURE, FLAMMABLE, TOXIC, N.O.S.
	3504
	2
	2.1

+6.1
	263

	2884
	CHEMICAL UNDER PRESSURE, FLAMMABLE, CORROSIVE, N.O.S.
	3505
	2
	2.1

+8
	238

	2885
	MERCURY CONTAINED IN MANUFACTURED ARTICLES
	3506
	8
	8

+6.1
	

	2886
	URANIUM HEXAFLUORIDE, RADIOACTIVE MATERIAL. EXCEPTED PACKAGE, less than 0.1 kg per package, non-fissile or fissile-excepted
	3507
	6,1
	6.1

+8
	

	2887
	CAPACITOR, ASYMMETRIC (with an energy storage capacity greater than 0.3Wh)
	3508
	9
	9
	

	2888
	PACKAGINGS, DISCARDED, EMPTY, UNCLEANED
	3509
	9
	9
	90

	2889
	ADSORBED GAS. FLAMMABLE, N.O.S.
	3510
	2
	2.1
	

	2890
	ADSORBED GAS, N.O.S.
	3511
	2
	2.2
	

	2891
	ADSORBED GAS, TOXIC, N.O.S.
	3512
	2
	2.3
	

	2892
	ADSORBED GAS, OXIDIZING, N.O.S.
	3513
	2
	2.2

+5.1
	

	2893
	ADSORBED GAS, TOXIC, FLAMMABLE, N.O.S.
	3514
	2
	2.3

+2.1
	

	2894
	ADSORBED GAS, TOXIC, OXIDIZING, N.O.S.
	3515
	2
	2.3

+5.1
	

	2895
	ADSORBED GAS, TOXIC, CORROSIVE, N.O.S.
	3516
	2
	2.3

+8
	

	2896
	ADSORBED GAS. TOXIC, FLAMMABLE, CORROSIVE, N.O.S.
	3517
	2
	2.3

+2.1

+8
	

	2897
	ADSORBED GAS. TOXIC, OXIDIZING, CORROSIVE, N.O.S.
	3518
	2
	2.3 

+5.1

+8
	

	2898
	BORON TRIFLUORIDE, ADSORBED
	3519
	2
	2.3

+8
	

	2899
	CHLORINE, ADSORBED
	3520
	2
	2.3

+5.1

+8
	

	2900
	SILICON TETRAFLUORIDE. ADSORBED
	3521
	2
	2.3

+8
	

	2901
	ARSINE, ADSORBED
	3522
	2
	2.3

+2.1
	

	2902
	GERMANE. ADSORBED
	3523
	2
	2.3

+2.1


	

	2903
	PHOSPHORUS PENTAFLUORIDE. ADSORBED
	3524
	2
	2.3+8
	

	2904
	PHOSPHINE, ADSORBED
	3525
	2
	2.3

+2.1
	

	2905
	HYDROGEN SELENIDE, ADSORBED
	3526
	2
	2.3

+2.1
	

	2906
	POLYESTER RESIN KIT, solid base material
	3527
	4.1
	4.1
	

	2907
	POLYESTER RESIN KIT, solid base material
	3527
	4.1
	4.1
	

	2908
	ENGINE, INTERNAL COMBUSTION, FLAMMABLE LIQUID POWERED or ENGINE, FUEL CELL, FLAMMABLE LIQUID POWERED or MACHINERY, INTERNAL COMBUSTION, FLAMMABLE LIQUID POWERED or MACHINERY, FUEL CELL, FLAMMABLE LIQUID POWERED
	3528
	3
	3
	

	2909
	ENGINE, INTERNAL COMBUSTION, FLAMMABLE GAS POWERED or ENGINE, FUEL CELL, FLAMMABLE GAS POWERED or MACHINERY, INTERNAL COMBUSTION, FLAMMABLE GAS POWERED or MACHINERY, FUEL CELL, FLAMMABLE GAS POWERED
	3529
	2
	2.1
	

	2910
	ENGINE, INTERNAL COMBUSTION or MACHINERY, INTERNAL COMBUSTION
	3530
	9
	9
	

	2911
	POLYMERIZING SUBSTANCE, SOLID, STABILIZED, N.O.S.
	3531
	4.1
	4.1
	40

	2912
	POLYMERIZING SUBSTANCE, LIQUID, STABILIZED, N.O.S.
	3532
	4.1
	4.1
	40

	2913
	POLYMERIZING SUBSTANCE, SOLID, TEMPERATURE CONTROLLED, N.O.S.
	3533
	4.1
	4.1
	40

	2914
	POLYMERIZING SUBSTANCE, LIQUID. TEMPERATURE CONTROLLED, N.O.S.
	3534
	4.1
	4.1
	40

	2915
	AMMONIA, DEEPLY REFRIGERATED
	9000
	2
	2.3+8
	

	2916
	SUBSTANCES WITH A FLASH​POINT ABOVE 60°C which are carried heated within a limiting range of 15K below their flash​point
	9001
	3
	none
	

	2917
	SUBSTANCES WITH A SELF​IGNITION TEMPRATURE OF 200°C AND BELOW, N.O.S.
	9002
	3
	none
	

	2918
	SUBSTANCES WITH A FLASH​POINT ABOVE 60°C AND NOT MORE THAN 100°C, which do not be longing another Class
	9003
	9
	none
	

	2919
	DIPHENYMETHANE-4, 4’ DIISOCYANATE
	9004
	9
	none
	

	2920
	ENVIROMETALLY HAZARDOUS SUBSTANCE SOLID, N.O.S.
	9005
	9
	none
	

	2921
	ENVIROMETALLY HAZARDOUS SUBSTANCE LIQUID, N.O.S.
	9006
	9
	none
	


APPENDIX II
hazard identification number
(Enclosed with Decree No. 34/2024/ND-CP dated March 31, 2024 of the Government of Vietnam)
Section 1. Each hazard identification number consists of 2 or 3 figures. Such figures indicate the following hazards:
2. Emission of gases due to pressures or chemical reactions
3. Flammability of liquids (vapours) and gases or self-heating liquids
4. Flammability of solids or self-heating solids
5. Oxidizing (fire-intensifying) effect
6. Toxicity
7. Radioactivity
8. Corrosivity
9. Risk of spontaneous violent reactions
Notes: The risk of spontaneous violet reaction within the meaning of figure 9 include the possibility following from the nature of a substance of a risk of explosion, disintegration and polymerization reaction following the release of considerable heat or flammable and/or toxic gases.
Doubling of a figure indicates an intensification of that particular hazard.
Where the hazard associated with a toxic substance can be adequately indicated by a single figure, this is followed by a zero.
Such figure combinations have special meanings - see Section 2:
If a hazard identification number is prefixed by letter 'X', this indicates that the substance will react violently with water. For such substances, water may only be used by approval of experts.
Section 2. The hazard identification numbers listed in Column 3 of Appendix I have the following meanings:
	20
	asphyxiant gas or gas with no subsidiary risk

	22
	refrigerated liquefied gas, asphyxiant

	223
	refrigerated liquefied gas, flammable

	225
	refrigerated liquefied gas, oxidizing (fire-intensifying)

	23
	flammable gas

	238
	gas, flammable corrosive

	239
	flammable gas, which can spontaneously lead to violent reaction

	25
	oxidizing (fire-intensifying) gas

	26
	 toxic gas

	263
	toxic gas, flammable

	265
	toxic gas, oxidizing (fire-intensifying)

	268
	toxic gas, corrosive 

	28
	gas, corrosive 

	
	

	30
	flammable liquid (flash-point between 23 °C and 60 °C, inclusive) or
flammable liquid or solid in the molten state with a flash-point above 60 °C, heated to a temperature equal to or above its flash-point, or self-heating liquid

	323
	flammable liquid which reacts with water, emitting flammable gases

	X323
	flammable liquid which reacts dangerously with water, emitting flammable gases1

	33
	highly flammable liquid (flash-point below 23 °C)

	333
	pyrophoric liquid

	X333
	pyrophoric liquid which reacts dangerously with water1

	336
	highly flammable liquid, toxic

	338
	highly flammable liquid, corrosive

	X338
	highly flammable liquid, corrosive, which reacts dangerously with water1

	339
	highly flammable liquid which can spontaneously lead to violent reaction

	36
	flammable liquid (flash-point between 23 °C and 60 °C, inclusive), slightly toxic, or self-heating liquid, toxic

	362
	flammable liquid, toxic, which reacts with water, emitting flammable gases

	X362
	flammable liquid, toxic, which reacts dangerously with water, emitting flammable gases1

	368
	flammable liquid, toxic, corrosive

	38
	flammable liquid (flash-point between 23 °C and 60 °C, inclusive), slightly corrosive, or self-heating liquid, corrosive

	382
	flammable liquid, corrosive, which reacts with water, emitting flammable gases

	X382
	flammable liquid, corrosive, which reacts dangerously with water, emitting flammable gases1

	39
	flammable liquid, which can spontaneously lead to violent reaction

	
	

	40
	flammable solid, or self-reactive substance, or self-heating substance, or polymerizing substance

	423
	solid which reacts with water, emitting flammable gases, or flammable solid which reacts with water, emitting flammable gases or self-heating solid which reacts with water, emitting flammable gases

	X423
	solid which reacts dangerously with water, emitting flammable gases, or flammable solid which reacts dangerously with water, emitting flammable gases or self-heating solid which reacts dangerously with water, emitting flammable gases1

	43
	spontaneously flammable (pyrophoric) solid

	X432
	spontaneously flammable (pyrophoric) solid which reacts dangerously with water, emitting flammable gases1

	44
	flammable solid, in the molten state at an elevated temperature

	446
	flammable solid, toxic, in the molten state at an elevated temperature

	46
	flammable or self-heating solid, toxic

	462
	toxic solid which reacts with water, emitting flammable gases

	X462
	solid which reacts dangerously with water, emitting toxic gases1

	48
	flammable or self-heating solid, corrosive 

	482
	corrosive solid which reacts with water, emitting flammable gases

	X482
	solid which reacts dangerously with water, emitting corrosive gases1

	
	

	50
	oxidizing (fire-intensifying) substance

	539
	flammable organic peroxide

	55
	strongly oxidizing (fire-intensifying) substance

	556
	strongly oxidizing (fire-intensifying) substance, toxic

	558
	strongly oxidizing (fire-intensifying) substance, corrosive 

	559
	strongly oxidizing (fire-intensifying) substance, which can spontaneously lead to violet reaction

	56
	oxidizing substance (fire-intensifying), toxic

	568
	oxidizing substance (fire-intensifying), toxic, corrosive

	58
	oxidizing substance (fire-intensifying), corrosive

	59
	oxidizing (fire-intensifying) substance which can spontaneously lead to violent reaction

	
	

	60
	 toxic or slightly toxic substance

	606
	infectious substance

	623
	toxic liquid, which reacts with water, emitting flammable gases

	63
	 toxic substance, flammable (flash-point between 23 °C and 60 °C, inclusive)

	638
	toxic substance, flammable (flash-point between 23 °C and 60 °C, inclusive), corrosive

	639
	toxic substance, flammable (flash-point above 60 °C) which can spontaneously lead to violent reaction

	64
	toxic solid, flammable or self-heating

	642
	toxic solid, which reacts with water, emitting flammable gases

	65
	toxic substance, oxidizing (fire-intensifying)

	66
	highly toxic substance

	663
	highly toxic substance, flammable (flash-point above 60 °C)

	664
	highly toxic solid, flammable or self-heating

	665
	highly toxic substance, oxidizing (fire-intensifying)

	668
	highly toxic substance, corrosive

	X668
	highly toxic substance, corrosive, which reacts dangerously with water1

	669
	highly toxic substance which can spontaneously lead to violent reaction

	68
	 toxic substance, corrosive 

	69
	toxic or slightly toxic substance, which can spontaneously lead to violent reaction

	
	

	70
	radioactive material

	768
	radioactive material, toxic, corrosive

	78
	radioactive material, corrosive

	80
	corrosive or slightly corrosive substance

	X80
	corrosive or slightly corrosive substance, which reacts dangerously with water1

	823
	corrosive liquid which reacts with water, emitting flammable gases

	83
	corrosive or slightly corrosive substance, flammable (flash-point between 23 °C and 60 °C, inclusive)

	X83
	corrosive or slightly corrosive substance, flammable (flash-point between 23 °C and 60 °C, inclusive), which reacts dangerously with water1

	839
	corrosive or slightly corrosive substance, flammable (flash-point between 23 °C and 60 °C, inclusive) which can spontaneously lead to violent reaction

	X839
	corrosive or slightly corrosive substance, flammable (flash-point between 23 °C and 60 °C, inclusive), which can spontaneously lead to violent reaction and which reacts dangerously with water1

	84
	corrosive solid, flammable or self-heating

	842
	corrosive solid which reacts with water, emitting flammable gases

	85
	corrosive or slightly corrosive substance, oxidizing (fire-intensifying)

	856
	corrosive or slightly corrosive substance, oxidizing (fire-intensifying) and toxic

	86
	corrosive or slightly corrosive substance, toxic

	88
	highly corrosive substance

	X88
	highly toxic substance, which reacts dangerously with water1

	883
	highly corrosive substance, flammable (flash-point between 23 °C and 60 °C, inclusive)

	884
	highly corrosive solid, flammable or self-heating

	885
	highly corrosive substance, oxidizing (fire-intensifying)

	886
	highly corrosive substance, toxic

	X886
	highly toxic substance, toxic, which reacts dangerously with water1

	89
	corrosive or slightly corrosive substance, which can spontaneously lead to violent reaction

	
	

	90
	environmentally hazardous substance; miscellaneous dangerous substances

	99
	miscellaneous dangerous substance carried at an elevated temperature.


APPENDIX III
SPECIMEN LABELS, PLACARDS OF DANGEROUS GOODS
(Enclosed with Decree No. 34/2024/ND-CP dated March 31, 2024 of the Government of Vietnam)
1. Specimen labels and placards of dangerous goods:
1.1. Class 1 hazard:
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1.2. Class 2 hazard:
[image: image2.png]b2 (sb22)
K a chiy Khi khlg chdy, khing e
Bida wgng (agon 6a): mho den hoje ting Bib ngng (chai chir Kh: mi den hofe ring.
Ném: b ;54 27 & g gy Nen: anh 1 chys s 2" & g dby





[image: image3.png](s623)
Bidu (dhu “;.ﬂ{-k'-ad‘ miu den
N ke kg 47" ity





1.3. Class 3 hazard:
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1.4. Class 4 hazard:
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1.5. Class 5 hazard:
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1.6. Class 6 hazard:
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1.7. Class 7 hazard:
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1.8. Class 8 hazard:
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1.9. Class 9 hazard:
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 2. Dimensions of labels and placards:
- For packages:  100 mm x 100 mm;
- For containers: 250 mm x 250 mm;
- For vehicles: 500 mm x 500 mm.
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3. Hazard signs
3.1. Dimensions
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3.2. Example of orange-coloured plate with hazard identification number and UN number
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Notes: For a vehicle with a permitted cargo volume of less than 5 tonnes: The vehicle owner may reduce the size of the plate according to the dimensions of the side of a truck, provided the plate is not smaller by more than 50% of the dimensions specified above.
APPENDIX IV
Dangerous goods vehicle/driver licence application form
(Enclosed with Decree No. 34/2024/ND-CP dated March 31, 2024 of the Government of Vietnam)
	Name of applicant:…………
No. ……/…..
---------
	SOCIALIST REPUBLIC OF VIETNAM
Independence - Freedom – Happiness
---------------

	
	…(location)…, date….month…year…..


Dangerous goods vehicle/driver licence application FORM
To: ……………………………………………………
1. Name of the applicant: ………………………………..
Address:………………………………………………
Phone number
 ……………………….. Fax:………………….. Email:………………..
2. Business registration certificate No.…………………… issued on………(date)…….. at ………(location)……….. or ID card No. or citizen identification card No./passport No.…………… issued on……(date)…… at ………(location)…… (applicable to individuals).
3. Licence for transport business by automobile No. …………. granted by……(name of licensing authority)……… (applicable to transport business units).
4. Information on the vehicle, including: registered number plate, validity of the certificate of roadworthiness, payload capacity (if the licence is granted to each separate trip).
5. Information about the driver/operator, including: full name, date of birth, class of driver’s licence (if the licence is granted to each separate trip); certificate of completion of dangerous goods training programme; ID card No. or citizen identification card No./passport No.……… issued on ……(date)……… at………(location)……
6. Information about the escort (if any), including:  full name, date of birth, ID card No. or citizen identification card No./passport No….
I am filling this application to kindly request your authority to consider issuing a licence to transport the following dangerous goods:
	No.
	Name and description
	UN number
	Class or division
	Hazard identification number
	Quantity of goods (estimated)

	1
	
	
	
	
	

	2
	
	
	
	
	

	...
	
	
	
	
	


The application consists of the following documents:
1.

2.

…………………….

…..(name of the applicant)…………. undertakes to ensure safety during transport and fully comply with laws on transport of dangerous goods.
	
	........, date….month…year…..
Applicant’s representative
(signature and seal)



Notes:
- The mode of transport (grant/modification of licence to transport by road/inland waterway) must be clearly specified.
- In case of online application, information shall be provided according to instructions available on the online public service system of the licensing authority.
APPENDIX IVA
Form of application for modification of DANGEROUS GOODS VEHICLE/DRIVER LICENCE
(Enclosed with Decree No. 34/2024/ND-CP dated March 31, 2024 of the Government of Vietnam)
	Name of applicant:…………
No. ……/…..
-------
	SOCIALIST REPUBLIC OF VIETNAM
Independence - Freedom – Happiness
---------------

	
	…(location)…, date….month…year…..


APPLICATION FOR MODIFICATION OF DANGEROUS GOODS VEHICLE/DRIVER LICENCE APPLICATION
To: ……………………………………………………
1. Name of the applicant: ………………………………..
Address:………………………………………………
Phone number
 ……………………….. Fax:………………….. Email:………………..
2. Business registration certificate No.…………………… issued on………(date)…….. at ………(location)……….. or ID card No. or citizen identification card No./passport No.…………… issued on……(date)…… at ………(location)…… (applicable to individuals).
3. Dangerous goods vehicle/driver licence No. ……… . Issue date:………(date)………….. . Expiry date:…………..
4. Modifications:
- Information on the granted licence: ……………….
- Modifications: ……………….
…..(name of the applicant)…………. undertakes to ensure safety during transport and fully comply with laws on transport of dangerous goods.
	
	........, date….month…year…..
Applicant’s representative
(signature and seal)



Notes: In case of online application, information shall be provided according to instructions available on the online public service system of the licensing authority.
APPENDIX V
dangerous goods transport plan template
(Enclosed with Decree No. 34/2024/ND-CP dated March 31, 2024 of the Government of Vietnam)
	Name of applicant:…………
No. ……/…..
-------
	SOCIALIST REPUBLIC OF VIETNAM
Independence - Freedom – Happiness
---------------

	
	…(location)…, date….month…year…..


DANGEROUS GOODS transport plan
To: ……………………………………………………
1. Name of the organization/individual transporting dangerous goods: ………………………………..
Address:………………………………………………
Tel:…………………….. Fax:………………….. Email:………………..
2. Information about the vehicle (or the attached list), including: registered number plate, validity of the certificate of roadworthiness, payload capacity ………………
3. Full name of the driver/operator (or the attached list):………………
4. Class of dangerous goods, quantity of goods (specifying each class, division of dangerous goods)……………..
5. Route of road/inland waterway transport: ………………….
6. Transport time: ……………………………………..
7. Information about the vehicle, including: registered number plate, validity of the certificate of roadworthiness, payload capacity ………………
8. Emergency response measures upon occurrence of a fire or explosion incident ………………….
We are looking forward to receiving your opinions.
	
	........, date….month…year…..
Organization/individual representative
(signature and seal)


